{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["General Information","Bridge Tool","Sheet3"],"not_rendered":{"charts":1,"images":12,"macros":1,"external_links":0,"defined_names":12,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"General Information","index":0,"n_rows":45,"n_cols":8,"rows_kept":45,"cut":false,"hidden":false,"merged":[[6,7,7,7],[3,1,7,2],[44,1,48,2],[9,6,10,7],[9,1,10,2]]}
[]
[null,"Bridge Prioritization Tool for Truck Platoons"]
[]
[null,"Description: \nThis program prioritizes TxDOT's bridges for different truck platoon configurations. The user selects the platoon parameters and the TxDOT district. The program provides a summary plot with the number of structures in each prioritization category. In addition, information on each bridges is provided, which includes estimated load ratings. Detailed background information on the analysis is provided in the project reports."]
[]
[]
[null,null,null,null,null,null,null,"TxDOT Project: 0-6984 (Task 4F)\nProject Title: Evaluate Potential Impacts, Benefits, Impediments, and Solutions of Automated Trucks and Truck Platooning on Texas Highway Infrastructure"]
[]
[]
[null,"Instructions - INPUT",null,null,null,null,"Instructions - OUTPUT"]
[]
[null,1,"ENABLE EXCEL MACROS to run the Bridge Tool worksheet.\nFor additional information please visit - https://support.office.com/en-us/article/enable-or-disable-macros-in-office-files-12b036fd-d140-4e74-b45e-16fed1a7e5c6#__toc311698309",null,null,null,1,"BRIDGE ID, HIGHWAY DISTRICT, LATITUDE, LONGITUDE: These results identify the bridge and its location. The values are taken from the national bridge inventory (NBI) database.  "]
[null,2,"NUMBER OF TRUCKS: The number of trucks available for selection is 2 or 3.  If 2 TRUCK option is selected then the platoon will have 2 trucks in the system. If 3 TRUCK option is selected, then the system will have 3 trucks in platoon",null,null,null,2,"YEAR BUILT/REBUILT: Refers to the design year of the bridge. If the structure has undergone a rehabilitation, then that year is reported. The values are taken from the NBI database. "]
[null,3,"TRUCK SPACING: The truck spacing options available are 30 FEET, 40 FEET and 50 FEET. This spacing is the axle-to-axle spacing between the rear axle of the leading truck and the front axle of the following truck.",null,null,null,3,"SPAN & BRIDGE CATEGORY: Refers to the maximm bridge span length and the type of bridge based. The information is taken from the NBI database."]
[null,4,"TRUCK TYPE: Three truck types are available for selection, which include the Florida C5, Alabama ALDOT Type 3S2_AL,  and AASHTO Type 3S2. The axle configurations for each truck are provide below. ",null,null,null,4,"*OPERATOR RATING: Refers to the estimated bridge operator rating according to its design (or rehabilitation) method. The results for bridges before 1975 are allowable stress ratings (ASR), between 1975 and 2004 are load factor ratings (LFR), and from 2005 to present are load and resistance factor ratings (LRFR). "]
[null,5,"TxDOT DISTRICT: Any of the 25 districts in Texas may be selected. The location of each district is provided on the map below.",null,null,null,5,"*PRIORITY RATING: Refers to the operator rating of the bridge converted to the LRFR method (for ASR and LFR results) and then adjusted for bridge condition using the inspection appraisal ratings. "]
[null,6,"OUTPUT TYPE: Two output options are available. The ALL BRIDGES option shows the data of all the bridges within the district. The HIGH PRIORITY option only shows the Level 5 bridges.",null,null,null,6,"*PRIORITY LEVEL: Refers to the relative categorization of the bridge based on its operator rating level. The results range from Level 1 (low) to Level 5 (high). "]
[null,null,null,null,null,null,null,"*The details of the analysis approach and assumptions are provided in the project report."]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"FOR MORE INFORMATION CONTACT:\nMatthew Yarnold, Assistant Research Engineer, TTI\nPhone: 979-862-5659\nEmail: myarnold@tamu.edu"]

{"sheet":"Bridge Tool","index":1,"n_rows":99,"n_cols":50,"rows_kept":99,"cut":false,"hidden":false,"merged":[[27,3,28,5],[12,3,14,5],[1,3,1,11],[0,3,0,11],[0,16,0,20],[2,3,4,5],[19,3,21,5],[8,3,9,5]]}
[null,null,null,"ANALYSIS INPUT ",null,null,null,null,null,null,null,null,null,null,null,null,"OUTPUT"]
["30 FEET",null,null,null,null,null,null,null,null,null,null,null,null,null,"BRIDGE ID","HIGHWAY DISTRICT","SPAN","YEAR BUILT/ REBUILT","LATITUDE","LONGITUDE","BRIDGE CATEGORY","OPERATOR RATING","PRIORITY RATING","PRIORITY INDEX"]
["40 FEET",null,null,"NUMBER OF TRUCKS",null,null,null,null,null,null,null,null,null,null,10600013603132,1,60,2016,33.301048520000002,-95.848313689999998,"prestress concrete girder",2.4,2.4,1]
["50 FEET",null,null,null,null,null,null,null,null,null,null,null,null,null,10810061002077,1,65,1963,33.161074759999998,-95.131828130000002,"prestress concrete girder",2.21,0.78,4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,10810061002192,1,70,2004,33.162128500000001,-95.234763200000003,"prestress concrete girder",2.23,0.94,2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,10920004701353,1,90,1991,33.809254449999997,-96.534633850000006,"prestress concrete girder",2.16,0.8,4]
["2 TRUCK",null,null,null,null,null,null,null,null,null,null,null,null,null,10920004703424,1,100,2005,33.553323499999998,-96.60645882,"prestress concrete girder",2.4300000000000002,2.0699999999999998,1,null,1,{"$f":"COUNTIF(X3:X765,1)","v":13}]
["3 TRUCK",null,null,null,null,null,null,null,null,null,null,null,null,null,10920004718235,1,115,1981,33.662234769999998,-96.611564990000005,"prestress concrete girder",1.93,0.82,3,null,2,{"$f":"COUNTIF(X3:X765,2)","v":10}]
[null,null,null,"TRUCK SPACING",null,null,null,null,null,null,null,null,null,null,10920004718250,1,100,1984,33.721130610000003,-96.585726170000001,"prestress concrete girder",2.0499999999999998,0.86,3,null,3,{"$f":"COUNTIF(X3:X765,3)","v":19}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,10920004718290,1,110,1991,33.789012100000001,-96.572018740000004,"prestress concrete girder",1.97,0.74,4,null,4,{"$f":"COUNTIF(X3:X765,4)","v":41}]
["1-C5",null,null,null,null,null,null,null,null,null,null,null,null,null,11130001002109,1,60,1962,33.147367930000001,-95.525239979999995,"prestress concrete girder",2.2000000000000002,0.77,4,null,5,{"$f":"COUNTIF(X3:X765,5)","v":12}]
["2- TYPE 3S2",null,null,null,null,null,null,null,null,null,null,null,null,null,11130001002113,1,70,1962,33.146665120000002,-95.494113920000004,"prestress concrete girder",2.23,0.63,5]
["3- ALDOT",null,null,"TRUCK TYPE",null,null,null,null,null,null,null,null,null,null,11130001002114,1,65,1987,33.137207930000002,-95.572434580000007,"prestress concrete girder",2.25,0.67,5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,11170000913284,1,85,1965,33.129451230000001,-95.991146650000005,"steel girder",1.38,0.64,5]
["1- ALL BRIDGES",null,null,null,null,null,null,null,null,null,null,null,null,null,11170000913327,1,80,1974,33.119496900000001,-96.096575470000005,"prestress concrete girder",2.19,0.92,2]
["2- HIGH PRIORITY",null,null,null,null,null,null,null,null,null,null,null,null,null,11170000913462,1,120,2011,33.088757289999997,-96.125096099999993,"prestress concrete girder",2.33,1.98,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,11170013602117,1,110,2002,33.273424919999997,-95.898135530000005,"prestress concrete girder",1.97,0.83,3]
["01",null,null,null,null,null,null,null,null,null,null,null,null,null,11170013602118,1,110,2002,33.273323089999998,-95.897783419999996,"prestress concrete girder",1.97,0.83,3]
["02",null,null,null,null,null,null,null,null,null,null,null,null,null,10920004702147,1,60,1962,33.640171180000003,-96.616076750000005,"steel girder",1.27,0.74,4]
["03",null,null,"TxDOT DISTRICT",null,null,null,null,null,null,null,null,null,null,10920004702216,1,60,1961,33.63417329,-96.616122649999994,"steel girder",1.27,0.74,4]
["04",null,null,null,null,null,null,null,null,null,null,null,null,null,10920004703133,1,90,1961,33.600926860000001,-96.607476800000001,"steel girder",1.43,0.83,3]
["05",null,null,null,null,null,null,null,null,null,null,null,null,null,10920004703157,1,50,1963,33.576071300000002,-96.602693220000006,"prestress concrete girder",2.2000000000000002,0.88,3]
["06",null,null,null,null,null,null,null,null,null,null,null,null,null,10920004713174,1,60,2003,33.506826570000001,-96.618246479999996,"steel girder",1.27,0.74,4]
["07",null,null,null,null,null,null,null,null,null,"\r\n2 TRUCK\r\n",null,null,null,10920004713187,1,75,1968,33.40018517,-96.580244699999994,"prestress concrete girder",2.2599999999999998,0.9,3]
["08",null,null,null,null,null,null,null,null,"\r\n","\r\n30 FEET\r\n",null,null,null,10920004718246,1,70,1987,33.717612670000001,-96.585483109999998,"prestress concrete girder",2.23,0.94,2]
["09",null,null,null,null,null,null,null,null,null,"\r\n1-C5\r\n",null,null,null,10920004718264,1,100,1987,33.74827011,-96.585284619999996,"prestress concrete girder",2.0499999999999998,0.86,3]
["10",null,null,null,null,null,null,null,null,null,"\r\n01\r\n",null,null,null,10920004718266,1,95,1987,33.762293790000001,-96.585301810000004,"prestress concrete girder",2.1,0.78,4]
["11",null,null,"OUTPUT TYPE",null,null,null,null,null,null,"\r\n1- ALL BRIDGES\r\n",null,null,null,10920004718291,1,100,1991,33.794305899999998,-96.5557613,"prestress concrete girder",2.0499999999999998,0.86,3]
["12",null,null,null,null,null,null,null,null,null,null,null,null,null,11130000909260,1,65,1962,33.116335190000001,-95.612607980000007,"prestress concrete girder",2.21,0.78,4]
["13",null,null,null,null,null,null,null,null,null,null,null,null,null,11130001002260,1,50,2013,33.146228299999997,-95.550793470000002,"prestress concrete special",2.41,2.41,0]
["14",null,null,null,null,null,null,null,null,null,null,null,null,null,11170000913297,1,65,1967,33.132031980000001,-95.947153180000001,"prestress concrete girder",2.21,0.62,5]
["15",null,null,null,null,null,null,null,null,null,null,null,null,null,11170000913316,1,90,1971,33.126411689999998,-96.083666989999998,"prestress concrete girder",2.35,0.83,3]
["16",null,null,null,null,null,null,null,null,null,null,null,null,null,11170000913317,1,85,1971,33.115929989999998,-96.099687590000002,"prestress concrete girder",2.3199999999999998,0.93,2]
["17",null,null,null,null,null,null,null,null,null,null,null,null,null,10600013604127,1,80,2008,33.393499669999997,-95.672560869999998,"prestress concrete girder",2.4500000000000002,2.08,1]
["18",null,null,null,null,null,null,null,null,null,null,null,null,null,10750020203045,1,90,2004,33.436959020000003,-96.337731820000002,"prestress concrete girder",2.16,0.91,2]
[19,null,null,null,null,null,null,null,null,null,null,null,null,null,10920004703128,1,60,1961,33.615401609999999,-96.60968312,"steel girder",1.27,0.74,4]
[20,null,null,null,null,null,null,null,null,null,null,null,null,null,10920004718230,1,60,1981,33.650151989999998,-96.611533780000002,"prestress concrete girder",2.2799999999999998,0.96,2]
[21,null,null,null,null,null,null,null,null,null,null,null,null,null,10920004718231,1,60,1981,33.650151989999998,-96.611749790000005,"prestress concrete girder",2.2799999999999998,0.96,2]
[22,null,null,null,null,null,null,null,null,null,null,null,null,null,10920004718247,1,70,1984,33.71758767,-96.585270100000002,"prestress concrete girder",2.23,0.94,2]
[23,null,null,null,null,null,null,null,null,null,null,null,null,null,11130000909290,1,65,1967,33.129566529999998,-95.8360895,"prestress concrete girder",2.21,0.78,4]
[24,null,null,null,null,null,null,null,null,null,null,null,null,null,11130001002126,1,60,1962,33.1469144,-95.457299649999996,"prestress concrete girder",2.2000000000000002,0.77,4]
[25,null,null,null,null,null,null,null,null,null,null,null,null,null,11130001002146,1,60,1994,33.116378279999999,-95.596448420000002,"prestress concrete girder",2.2799999999999998,0.96,2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,11170000913463,1,85,2012,33.096299999999999,-96.109766999999991,"prestress concrete girder",2.4700000000000002,2.4700000000000002,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,11170000913478,1,120,2011,33.088100169999997,-96.125762199999997,"prestress concrete girder",2.33,1.98,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,10920004701383,1,110,1991,33.802357600000001,-96.537395939999996,"prestress concrete girder",1.97,0.74,4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,10920004701398,1,130,1996,33.822104529999997,-96.533529799999997,"prestress concrete girder",1.76,0.74,4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,10920004702125,1,60,1961,33.628558380000001,-96.613522470000007,"steel girder",1.27,0.74,4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,10920004702126,1,60,1961,33.628512379999997,-96.61373347,"steel girder",1.27,0.74,4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,10920004703153,1,60,1963,33.529601149999998,-96.612047700000005,"prestress concrete girder",2.2000000000000002,0.77,4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,10920004718236,1,75,1981,33.670424619999999,-96.609986079999999,"prestress concrete girder",2.21,0.82,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"You selected\r\n3 TRUCK\r\n"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,10920004718322,1,150,1982,33.680820429999997,-96.607768190000002,"prestress concrete girder",1.63,0.69,5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,10920004718325,1,120,1982,33.708020859999998,-96.589542069999993,"prestress concrete girder",1.87,0.79,4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,11130000909181,1,65,1960,33.12122875,-95.671523989999997,"prestress concrete girder",2.21,0.78,4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,11170000913330,1,80,1974,33.133369000000002,-96.056180999999995,"prestress concrete girder",1.63,0.49,5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,11170000913465,1,85,2012,33.096299999999999,-96.109800000000007,"prestress concrete girder",2.4700000000000002,2.4700000000000002,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,10810061002004,1,65,1963,33.166111610000002,-95.307086679999998,"prestress concrete girder",2.21,0.88,3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,10920004702215,1,60,1961,33.634202289999998,-96.615905639999994,"steel girder",1.27,0.74,4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,10920004703426,1,90,2005,33.595377790000001,-96.605156489999999,"prestress concrete girder",2.4900000000000002,1.87,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,10920004713176,1,60,2003,33.465396579999997,-96.613032419999996,"steel girder",1.27,0.74,4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,10920004718262,1,120,1987,33.72927146,-96.585217290000003,"prestress concrete girder",1.87,0.79,4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,10920004718272,1,125,1988,33.778602409999998,-96.584131990000003,"prestress concrete girder",1.81,0.68,5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,10920004718326,1,120,1982,33.708031869999999,-96.589782080000006,"prestress concrete girder",1.87,0.79,4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,11130000909193,1,65,1960,33.123393370000002,-95.73395112,"prestress concrete girder",2.21,0.78,4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,11130000909497,1,65,1960,33.1195278,-95.634166699999994,"prestress concrete girder",2.21,0.62,5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,11170000913328,1,90,1974,33.135609449999997,-96.073120599999996,"prestress concrete girder",1.76,0.74,4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,11940004601024,1,120,2005,33.622189169999999,-95.052034999999989,"prestress concrete girder",2.33,1.75,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,10920004503248,1,80,2010,33.620019999999997,-96.698250000000002,"prestress concrete girder",2.4500000000000002,2.08,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,10920004702141,1,75,1985,33.646898049999997,-96.612731760000003,"steel girder",1.29,0.74,4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,10920004702148,1,60,1962,33.640152180000001,-96.615860740000002,"steel girder",1.27,0.74,4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,10920004702217,1,60,1961,33.635137270000001,-96.616397669999998,"steel girder",1.27,0.74,4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,10920004702218,1,60,1961,33.635175269999998,-96.616180659999998,"steel girder",1.27,0.74,4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,10920004703127,1,60,1961,33.61544361,-96.609467109999997,"steel girder",1.27,0.74,4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,11130000909195,1,65,1960,33.120716559999998,-95.708676269999998,"prestress concrete girder",2.21,0.78,4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,11130000909291,1,65,1967,33.131433360000003,-95.806835520000007,"prestress concrete girder",2.21,0.78,4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,10920004701052,1,110,1991,33.801341479999998,-96.538090629999999,"prestress concrete girder",1.97,0.83,3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,10920004703158,1,50,1963,33.576079300000004,-96.602481220000001,"prestress concrete girder",2.2000000000000002,0.88,3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,10920004718249,1,100,1987,33.720991609999999,-96.58549816,"prestress concrete girder",2.0499999999999998,0.86,3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,10920004718263,1,120,1987,33.729140459999996,-96.585420299999996,"prestress concrete girder",1.87,0.79,4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,10920004718265,1,100,1987,33.748277109999997,-96.585501629999996,"prestress concrete girder",2.0499999999999998,0.76,4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,10920004718274,1,130,1988,33.771733570000002,-96.58473592,"prestress concrete girder",1.76,0.65,5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,10920004718324,1,110,1982,33.693009179999997,-96.59974115,"prestress concrete girder",1.97,0.83,3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,11130000909182,1,65,1960,33.119890990000002,-95.633946699999996,"prestress concrete girder",2.21,0.62,5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,11130001002257,1,65,1960,33.143432820000001,-95.565022319999997,"prestress concrete girder",2.21,0.62,5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,11130061001032,1,65,1963,33.167265790000002,-95.331653430000003,"prestress concrete girder",2.21,0.88,3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,11170000913464,1,80,2010,33.119150269999999,-96.096550969999996,"prestress concrete girder",2.4500000000000002,2.08,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,10920004701354,1,90,1991,33.809258450000002,-96.534839849999997,"prestress concrete girder",2.16,0.8,4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,10920004701399,1,130,1997,33.822096639999998,-96.533172609999994,"prestress concrete girder",1.76,0.74,4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,10920004713180,1,60,2003,33.421414660000003,-96.588870889999995,"steel girder",1.27,0.74,4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,10920004718228,1,115,1981,33.655548899999999,-96.612261899999993,"prestress concrete girder",1.93,0.82,3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,10920004718237,1,75,1981,33.670461619999998,-96.61018009,"prestress concrete girder",2.21,0.93,2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,10920004718273,1,105,1988,33.771738569999997,-96.584954920000001,"prestress concrete girder",2.0099999999999998,0.74,4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,10920004718323,1,150,2014,33.680877959999997,-96.607618759999994,"prestress concrete girder",2.16,1.84,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,11130001002259,1,55,2013,33.146070289999997,-95.552161810000001,"prestress concrete special",2.4,2.4,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,11130061001022,1,65,1963,33.162037400000003,-95.405220909999997,"prestress concrete girder",2.21,0.78,4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,11170000913329,1,90,1974,33.135761440000003,-96.073214609999994,"prestress concrete girder",1.76,0.74,4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,11170000913466,1,85,2011,33.096425600000003,-96.109876330000006,"prestress concrete girder",2.4700000000000002,2.4700000000000002,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,11170013602115,1,105,2002,33.26792949,-95.904937009999998,"prestress concrete girder",2.0099999999999998,0.84,3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,11170013602116,1,105,2002,33.267936839999997,-95.904509970000007,"prestress concrete girder",2.0099999999999998,0.74,4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,11390004509156,1,60,1978,33.660717069999997,-95.599174529999999,"prestress concrete girder",1.55,0.57999999999999996,5]

{"sheet":"Sheet3","index":2,"n_rows":6554,"n_cols":61,"rows_kept":1125,"cut":true,"hidden":true,"merged":[[1,7,1,9],[1,10,1,12],[1,13,1,15],[1,16,1,18],[0,7,0,15],[1,19,1,21],[1,22,1,24],[0,16,0,24],[0,25,0,33],[0,34,0,42],[1,25,1,27],[1,28,1,30],[1,31,1,33],[1,34,1,36],[1,37,1,39],[1,40,1,42],[0,43,0,51],[0,52,0,60],[1,43,1,45],[1,46,1,48],[1,49,1,51],[1,52,1,54],[1,55,1,57],[1,58,1,60]],"bounds":{"rows_first":500,"rows_last":125,"rows_between":500,"halvings":2}}
[null,null,null,null,null,null,null,"2 TRUCK",null,null,null,null,null,null,null,null,"3 TRUCK",null,null,null,null,null,null,null,null,"2 TRUCK",null,null,null,null,null,null,null,null,"3 TRUCK",null,null,null,null,null,null,null,null,"2 TRUCK ALDOT",null,null,null,null,null,null,null,null,"3 TRUCK ALDOT"]
[null,null,null,null,null,null,null,"C5 30 FEET",null,null,"C5 40 FEET",null,null,"C5 50 FEET",null,null,"C5 30 FEET",null,null,"C5 40 FEET",null,null,"C5 50 FEET",null,null,"3S230 FEET",null,null,"3S2 40 FEET",null,null,"3S2 50 FEET",null,null,"3S2 30 FEET",null,null,"3S2 40 FEET",null,null,"3S2 50 FEET",null,null,"ALDOT 30 FEET",null,null,"ALDOT 40 FEET",null,null,"ALDOT 50 FEET",null,null,"ALDOT 30 FEET",null,null,"ALDOT 40 FEET",null,null,"ALDOT 50 FEET"]
["BRDG_ID","STATE_HWY_DEPT_DIST","LENGTH MAX SPAN","YEAR MAX","LAT_DD","LONG_DD","bridge_type","operator_rating","NET_RATING","PRIORITY_INDEX","operator_rating","NET_RATING","PRIORITY_INDEX","operator_rating","NET_RATING","PRIORITY_INDEX","operator_rating","NET_RATING","PRIORITY_INDEX","operator_rating","NET_RATING","PRIORITY_INDEX","operator_rating","NET_RATING","PRIORITY_INDEX","operator_rating","NET_RATING","PRIORITY_INDEX","operator_rating","NET_RATING","PRIORITY_INDEX","operator_rating","NET_RATING","PRIORITY_INDEX","operator_rating","NET_RATING","PRIORITY_INDEX","operator_rating","NET_RATING","PRIORITY_INDEX","operator_rating","NET_RATING","PRIORITY_INDEX","operator_rating","NET_RATING","PRIORITY_INDEX","operator_rating","NET_RATING","PRIORITY_INDEX","operator_rating","NET_RATING","PRIORITY_INDEX","operator_rating","NET_RATING","PRIORITY_INDEX","operator_rating","NET_RATING","PRIORITY_INDEX","operator_rating","NET_RATING","PRIORITY_INDEX"]
["010600013603132","01",60,2016,33.301048520000002,-95.848313689999998,"prestress concrete girder",2.4,2.4,1,2.4,2.4,1,2.4,2.4,1,2.4,2.4,1,2.4,2.4,1,2.4,2.4,1,3.1,3.1,1,3.1,3.1,1,3.1,3.1,1,3.1,3.1,1,3.1,3.1,1,3.1,3.1,1,2.77,2.77,1,2.77,2.77,1,2.77,2.77,1,2.77,2.77,1,2.77,2.77,1,2.77,2.77,1]
["010810061002077","01",65,1963,33.161074759999998,-95.131828130000002,"prestress concrete girder",2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3]
["010810061002192","01",70,2004,33.162128500000001,-95.234763200000003,"prestress concrete girder",2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1]
["010920004701353","01",90,1991,33.809254449999997,-96.534633850000006,"prestress concrete girder",2.16,0.8,4,2.17,0.8,4,2.17,0.8,4,2.16,0.8,4,2.17,0.8,4,2.17,0.8,4,2.63,0.98,2,2.63,0.98,2,2.63,0.98,2,2.63,0.98,2,2.63,0.98,2,2.63,0.98,2,2.36,0.88,3,2.36,0.88,3,2.36,0.88,3,2.36,0.88,3,2.36,0.88,3,2.36,0.88,3]
["010920004703424","01",100,2005,33.553323499999998,-96.60645882,"prestress concrete girder",2.4300000000000002,2.0699999999999998,1,2.5499999999999998,2.17,1,2.5499999999999998,2.17,1,2.4300000000000002,2.0699999999999998,1,2.5499999999999998,2.17,1,2.5499999999999998,2.17,1,2.91,2.4700000000000002,1,3.05,2.59,1,3.05,2.59,1,2.91,2.4700000000000002,1,3.05,2.59,1,3.05,2.59,1,2.62,2.23,1,2.74,2.33,1,2.74,2.33,1,2.62,2.23,1,2.74,2.33,1,2.74,2.33,1]
["010920004718235","01",115,1981,33.662234769999998,-96.611564990000005,"prestress concrete girder",1.93,0.82,3,2.08,0.88,3,2.13,0.89,3,1.93,0.82,3,2.08,0.88,3,2.13,0.89,3,2.27,0.95,2,2.4700000000000002,1.04,1,2.5299999999999998,1.06,1,2.27,0.95,2,2.4700000000000002,1.04,1,2.5299999999999998,1.06,1,2.04,0.86,3,2.23,0.94,2,2.27,0.95,2,2.04,0.86,3,2.23,0.94,2,2.27,0.95,2]
["010920004718250","01",100,1984,33.721130610000003,-96.585726170000001,"prestress concrete girder",2.0499999999999998,0.86,3,2.15,0.9,3,2.15,0.9,3,2.0499999999999998,0.86,3,2.15,0.9,3,2.15,0.9,3,2.46,1.04,1,2.58,1.0900000000000001,1,2.58,1.0900000000000001,1,2.46,1.04,1,2.58,1.0900000000000001,1,2.58,1.0900000000000001,1,2.2200000000000002,0.94,2,2.3199999999999998,0.98,2,2.3199999999999998,0.98,2,2.2200000000000002,0.94,2,2.3199999999999998,0.98,2,2.3199999999999998,0.98,2]
["010920004718290","01",110,1991,33.789012100000001,-96.572018740000004,"prestress concrete girder",1.97,0.74,4,2.12,0.79,4,2.14,0.8,4,1.97,0.74,4,2.12,0.79,4,2.14,0.8,4,2.3199999999999998,0.86,3,2.54,0.95,2,2.54,0.95,2,2.3199999999999998,0.86,3,2.54,0.95,2,2.54,0.95,2,2.09,0.77,4,2.2799999999999998,0.85,3,2.2799999999999998,0.85,3,2.09,0.77,4,2.2799999999999998,0.85,3,2.2799999999999998,0.85,3]
["011130001002109","01",60,1962,33.147367930000001,-95.525239979999995,"prestress concrete girder",2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.84,1,2,2.84,1,2,2.84,1,2,2.84,1,2,2.84,1,2,2.84,1,2,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3]
["011130001002113","01",70,1962,33.146665120000002,-95.494113920000004,"prestress concrete girder",2.23,0.63,5,2.23,0.63,5,2.23,0.63,5,2.23,0.63,5,2.23,0.63,5,2.23,0.63,5,2.8,0.79,4,2.8,0.79,4,2.8,0.79,4,2.8,0.79,4,2.8,0.79,4,2.8,0.79,4,2.5099999999999998,0.71,4,2.5099999999999998,0.71,4,2.5099999999999998,0.71,4,2.5099999999999998,0.71,4,2.5099999999999998,0.71,4,2.5099999999999998,0.71,4]
["011130001002114","01",65,1987,33.137207930000002,-95.572434580000007,"prestress concrete girder",2.25,0.67,5,2.25,0.67,5,2.25,0.67,5,2.25,0.67,5,2.25,0.67,5,2.25,0.67,5,2.86,0.85,3,2.86,0.85,3,2.86,0.85,3,2.86,0.85,3,2.86,0.85,3,2.86,0.85,3,2.56,0.76,4,2.56,0.76,4,2.56,0.76,4,2.56,0.76,4,2.56,0.76,4,2.56,0.76,4]
["011170000913284","01",85,1965,33.129451230000001,-95.991146650000005,"steel girder",1.38,0.64,5,1.35,0.62,5,1.38,0.64,5,1.35,0.62,5,1.35,0.62,5,1.38,0.64,5,1.59,0.73,4,1.59,0.73,4,1.64,0.76,4,1.59,0.73,4,1.59,0.73,4,1.64,0.76,4,1.43,0.66,5,1.42,0.65,5,1.47,0.68,5,1.42,0.65,5,1.42,0.65,5,1.47,0.68,5]
["011170000913327","01",80,1974,33.119496900000001,-96.096575470000005,"prestress concrete girder",2.19,0.92,2,2.19,0.92,2,2.19,0.92,2,2.2000000000000002,0.93,2,2.2000000000000002,0.93,2,2.2000000000000002,0.93,2,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1]
["011170000913462","01",120,2011,33.088757289999997,-96.125096099999993,"prestress concrete girder",2.33,1.98,1,2.5499999999999998,2.17,1,2.66,2.2599999999999998,1,2.33,1.98,1,2.5499999999999998,2.17,1,2.66,2.2599999999999998,1,2.77,2.35,1,3.01,2.56,1,3.14,2.67,1,2.77,2.35,1,3.01,2.56,1,3.14,2.67,1,2.4900000000000002,2.12,1,2.71,2.2999999999999998,1,2.82,2.4,1,2.4900000000000002,2.12,1,2.71,2.2999999999999998,1,2.82,2.4,1]
["011170013602117","01",110,2002,33.273424919999997,-95.898135530000005,"prestress concrete girder",1.97,0.83,3,2.12,0.89,3,2.14,0.9,3,1.97,0.83,3,2.12,0.89,3,2.14,0.9,3,2.3199999999999998,0.98,2,2.54,1.07,1,2.54,1.07,1,2.3199999999999998,0.98,2,2.54,1.07,1,2.54,1.07,1,2.09,0.88,3,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.09,0.88,3,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2]
["011170013602118","01",110,2002,33.273323089999998,-95.897783419999996,"prestress concrete girder",1.97,0.83,3,2.12,0.89,3,2.14,0.9,3,1.97,0.83,3,2.12,0.89,3,2.14,0.9,3,2.3199999999999998,0.98,2,2.54,1.07,1,2.54,1.07,1,2.3199999999999998,0.98,2,2.54,1.07,1,2.54,1.07,1,2.09,0.88,3,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.09,0.88,3,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2]
["021270001403495","02",90,2008,32.486131710000002,-97.28001313,"prestress concrete girder",2.4900000000000002,2.12,1,2.5,2.13,1,2.5,2.13,1,2.4900000000000002,2.12,1,2.5,2.13,1,2.5,2.13,1,3.02,2.57,1,3.02,2.57,1,3.02,2.57,1,3.02,2.57,1,3.02,2.57,1,3.02,2.57,1,2.72,2.31,1,2.72,2.31,1,2.72,2.31,1,2.72,2.31,1,2.72,2.31,1,2.72,2.31,1]
["021820031403132","02",65,1970,32.52444216,-98.338068930000006,"prestress concrete girder",2.21,0.88,3,2.21,0.88,3,2.21,0.88,3,2.21,0.88,3,2.21,0.88,3,2.21,0.88,3,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.52,1,2,2.52,1,2,2.52,1,2,2.52,1,2,2.52,1,2,2.52,1,2]
["021820031403134","02",95,1970,32.533469119999999,-98.319217399999999,"prestress concrete girder",2.33,0.94,2,2.39,0.95,2,2.39,0.95,2,2.33,0.94,2,2.39,0.95,2,2.39,0.95,2,2.83,1.1299999999999999,1,2.88,1.1499999999999999,1,2.88,1.1499999999999999,1,2.83,1.1299999999999999,1,2.88,1.1499999999999999,1,2.88,1.1499999999999999,1,2.5499999999999998,1.02,1,2.59,1.04,1,2.59,1.04,1,2.5499999999999998,1.02,1,2.59,1.04,1,2.59,1.04,1]
["021820031403135","02",95,1970,32.533626130000002,-98.318419379999995,"prestress concrete girder",2.33,0.94,2,2.39,0.95,2,2.39,0.95,2,2.33,0.94,2,2.39,0.95,2,2.39,0.95,2,2.83,1.1299999999999999,1,2.88,1.1499999999999999,1,2.88,1.1499999999999999,1,2.83,1.1299999999999999,1,2.88,1.1499999999999999,1,2.88,1.1499999999999999,1,2.5499999999999998,1.02,1,2.59,1.04,1,2.59,1.04,1,2.5499999999999998,1.02,1,2.59,1.04,1,2.59,1.04,1]
["021840000803274","02",100,1978,32.747486909999999,-97.674147230000003,"prestress concrete girder",2.0499999999999998,0.86,3,2.15,0.9,3,2.15,0.9,3,2.0499999999999998,0.86,3,2.15,0.9,3,2.15,0.9,3,2.46,1.04,1,2.58,1.0900000000000001,1,2.58,1.0900000000000001,1,2.46,1.04,1,2.58,1.0900000000000001,1,2.58,1.0900000000000001,1,2.2200000000000002,0.94,2,2.3199999999999998,0.98,2,2.3199999999999998,0.98,2,2.2200000000000002,0.94,2,2.3199999999999998,0.98,2,2.3199999999999998,0.98,2]
["021840000803276","02",75,1978,32.739883229999997,-97.652071460000002,"prestress concrete girder",2.21,0.93,2,2.21,0.93,2,2.21,0.93,2,2.21,0.93,2,2.21,0.93,2,2.21,0.93,2,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.46,1.04,1,2.46,1.04,1,2.46,1.04,1,2.46,1.04,1,2.46,1.04,1,2.46,1.04,1]
["021840031401083","02",145,2008,32.66499314,-98.033445589999999,"steel girder",1.77,1.5,1,1.95,1.66,1,2.12,1.8,1,1.7,1.44,1,1.73,1.47,1,1.81,1.54,1,2.11,1.79,1,2.3199999999999998,1.97,1,2.46,2.09,1,1.88,1.6,1,1.97,1.67,1,2.12,1.8,1,1.9,1.62,1,2.09,1.78,1,2.21,1.88,1,1.69,1.44,1,1.78,1.51,1,1.91,1.62,1]
["021840031407064","02",50,1969,32.728121180000002,-97.85005452,"prestress concrete girder",2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.99,1.06,1,2.99,1.06,1,2.99,1.06,1,2.99,1.06,1,2.99,1.06,1,2.99,1.06,1,2.67,0.94,2,2.67,0.94,2,2.67,0.94,2,2.67,0.94,2,2.67,0.94,2,2.67,0.94,2]
["021840031407232","02",100,2017,32.746110000000002,-97.73527,"prestress concrete girder",2.4300000000000002,2.4300000000000002,1,2.5499999999999998,2.5499999999999998,1,2.5499999999999998,2.5499999999999998,1,2.4300000000000002,2.4300000000000002,1,2.5499999999999998,2.5499999999999998,1,2.5499999999999998,2.5499999999999998,1,2.91,2.91,1,3.05,3.05,1,3.05,3.05,1,2.91,2.91,1,3.05,3.05,1,3.05,3.05,1,2.62,2.62,1,2.74,2.74,1,2.74,2.74,1,2.62,2.62,1,2.74,2.74,1,2.74,2.74,1]
["022200000812357","02",125,1991,32.667374129999999,-97.352541840000001,"prestress concrete girder",1.81,0.77,4,2,0.84,3,2.12,0.89,3,1.81,0.77,4,2,0.84,3,2.12,0.89,3,2.16,0.91,2,2.35,0.99,2,2.5,1.05,1,2.16,0.91,2,2.35,0.99,2,2.5,1.05,1,1.95,0.82,3,2.12,0.89,3,2.25,0.94,2,1.95,0.82,3,2.12,0.89,3,2.25,0.94,2]
["022200000812464","02",115,2013,32.682657999999996,-97.400466999999992,"prestress concrete girder",2.38,2.02,1,2.56,2.1800000000000002,1,2.63,2.2400000000000002,1,2.38,2.02,1,2.56,2.1800000000000002,1,2.63,2.2400000000000002,1,2.8,2.38,1,3.05,2.59,1,3.12,2.65,1,2.8,2.38,1,3.05,2.59,1,3.12,2.65,1,2.52,2.14,1,2.75,2.34,1,2.8,2.38,1,2.52,2.14,1,2.75,2.34,1,2.8,2.38,1]
["022200000813092","02",75,1988,32.662990000000001,-97.244659999999996,"steel girder",1.29,0.84,3,1.31,0.86,3,1.38,0.9,3,1.29,0.84,3,1.31,0.86,3,1.38,0.9,3,1.53,1,2,1.58,1.04,1,1.7,1.1100000000000001,1,1.53,1,2,1.58,1.04,1,1.7,1.1100000000000001,1,1.37,0.89,3,1.41,0.93,2,1.52,0.99,2,1.37,0.89,3,1.41,0.93,2,1.52,0.99,2]
["022200000813093","02",75,1988,32.662612799999998,-97.244588530000001,"steel girder",1.29,0.84,3,1.31,0.86,3,1.38,0.9,3,1.29,0.84,3,1.31,0.86,3,1.38,0.9,3,1.53,1,2,1.58,1.04,1,1.7,1.1100000000000001,1,1.53,1,2,1.58,1.04,1,1.7,1.1100000000000001,1,1.37,0.89,3,1.41,0.93,2,1.52,0.99,2,1.37,0.89,3,1.41,0.93,2,1.52,0.99,2]
["022200000813100","02",75,1963,32.734791710000003,-97.224728450000001,"steel girder",1.29,0.59,5,1.31,0.61,5,1.38,0.64,5,1.29,0.59,5,1.31,0.61,5,1.38,0.64,5,1.53,0.71,4,1.58,0.73,4,1.7,0.79,4,1.53,0.71,4,1.58,0.73,4,1.7,0.79,4,1.37,0.63,5,1.41,0.65,5,1.52,0.7,5,1.37,0.63,5,1.41,0.65,5,1.52,0.7,5]
["022200000813104","02",65,1963,32.72944055,-97.225054150000005,"steel girder",1.25,0.72,4,1.33,0.77,4,1.51,0.87,3,1.25,0.72,4,1.33,0.77,4,1.51,0.87,3,1.54,0.89,3,1.68,0.97,2,1.93,1.1200000000000001,1,1.54,0.89,3,1.68,0.97,2,1.93,1.1200000000000001,1,1.38,0.8,4,1.51,0.87,3,1.73,1,2,1.38,0.8,4,1.51,0.87,3,1.73,1,2]
["022200000813126","02",90,1963,32.780898000000001,-97.212408999999994,"steel girder",1.43,0.83,3,1.39,0.8,4,1.4,0.81,3,1.36,0.79,4,1.39,0.8,4,1.4,0.81,3,1.64,0.95,2,1.62,0.94,2,1.64,0.95,2,1.61,0.93,2,1.62,0.94,2,1.64,0.95,2,1.47,0.85,3,1.45,0.84,3,1.47,0.85,3,1.45,0.84,3,1.45,0.84,3,1.47,0.85,3]
["022200000813343","02",60,1988,32.661484799999997,-97.260043999999994,"prestress concrete girder",2.2799999999999998,0.85,3,2.2799999999999998,0.85,3,2.2799999999999998,0.85,3,2.2799999999999998,0.85,3,2.2799999999999998,0.85,3,2.2799999999999998,0.85,3,2.94,1.1000000000000001,1,2.94,1.1000000000000001,1,2.94,1.1000000000000001,1,2.94,1.1000000000000001,1,2.94,1.1000000000000001,1,2.94,1.1000000000000001,1,2.64,0.98,2,2.64,0.98,2,2.64,0.98,2,2.64,0.98,2,2.64,0.98,2,2.64,0.98,2]
["022200000813416","02",155,2001,32.831981999999996,-97.207526000000001,"steel girder",1.33,0.87,3,1.47,0.96,2,1.62,1.06,1,1.28,0.84,3,1.47,0.96,2,1.62,1.06,1,1.56,1.02,1,1.73,1.1299999999999999,1,1.91,1.25,1,1.55,1.01,1,1.73,1.1299999999999999,1,1.91,1.25,1,1.4,0.92,2,1.56,1.02,1,1.72,1.1200000000000001,1,1.39,0.91,2,1.56,1.02,1,1.72,1.1200000000000001,1]
["022200000813419","02",120,2002,32.831899219999997,-97.207738030000002,"prestress concrete girder",1.87,0.79,4,2.04,0.86,3,2.13,0.89,3,1.87,0.79,4,2.04,0.86,3,2.13,0.89,3,2.2200000000000002,0.94,2,2.41,1.01,1,2.5099999999999998,1.05,1,2.2200000000000002,0.94,2,2.41,1.01,1,2.5099999999999998,1.05,1,1.99,0.84,3,2.17,0.91,2,2.2599999999999998,0.95,2,1.99,0.84,3,2.17,0.91,2,2.2599999999999998,0.95,2]
["022200000813421","02",180,1990,32.666959310000003,-97.318359790000002,"Multi Span Long",0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1]
["022200000813429","02",125,1990,32.667121299999998,-97.320555859999999,"prestress concrete girder",1.81,0.68,5,2,0.74,4,2.12,0.79,4,1.81,0.68,5,2,0.74,4,2.12,0.79,4,2.16,0.8,4,2.35,0.87,3,2.5,0.93,2,2.16,0.8,4,2.35,0.87,3,2.5,0.93,2,1.95,0.73,4,2.12,0.79,4,2.25,0.83,3,1.95,0.73,4,2.12,0.79,4,2.25,0.83,3]
["022200000813430","02",125,1990,32.667221290000001,-97.320554860000001,"prestress concrete girder",1.81,0.68,5,2,0.74,4,2.12,0.79,4,1.81,0.68,5,2,0.74,4,2.12,0.79,4,2.16,0.8,4,2.35,0.87,3,2.5,0.93,2,2.16,0.8,4,2.35,0.87,3,2.5,0.93,2,1.95,0.73,4,2.12,0.79,4,2.25,0.83,3,1.95,0.73,4,2.12,0.79,4,2.25,0.83,3]
["022200000814201","02",75,1973,32.836388069999998,-97.3629186,"prestress concrete girder",2.2599999999999998,0.8,4,2.2599999999999998,0.8,4,2.2599999999999998,0.8,4,2.2599999999999998,0.8,4,2.2599999999999998,0.8,4,2.2599999999999998,0.8,4,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3]
["022200000814204","02",140,1973,32.838313040000003,-97.358761490000006,"steel girder",1.67,1.1000000000000001,1,1.84,1.21,1,1.96,1.28,1,1.52,0.99,2,1.57,1.03,1,1.66,1.0900000000000001,1,2,1.31,1,2.2000000000000002,1.44,1,2.1800000000000002,1.43,1,1.69,1.1100000000000001,1,1.79,1.17,1,1.94,1.27,1,1.8,1.18,1,1.98,1.29,1,1.96,1.28,1,1.52,0.99,2,1.61,1.05,1,1.75,1.1499999999999999,1]
["022200000814205","02",140,1973,32.837996050000001,-97.358714489999997,"steel girder",1.67,1.1000000000000001,1,1.84,1.21,1,1.96,1.28,1,1.52,0.99,2,1.57,1.03,1,1.66,1.0900000000000001,1,2,1.31,1,2.2000000000000002,1.44,1,2.1800000000000002,1.43,1,1.69,1.1100000000000001,1,1.79,1.17,1,1.94,1.27,1,1.8,1.18,1,1.98,1.29,1,1.96,1.28,1,1.52,0.99,2,1.61,1.05,1,1.75,1.1499999999999999,1]
["022200000814261","02",75,1977,32.798074620000001,-97.440621710000002,"prestress concrete girder",2.21,0.93,2,2.21,0.93,2,2.21,0.93,2,2.21,0.93,2,2.21,0.93,2,2.21,0.93,2,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.46,1.04,1,2.46,1.04,1,2.46,1.04,1,2.46,1.04,1,2.46,1.04,1,2.46,1.04,1]
["022200000814488","02",110,2014,32.840510999999999,-97.24430799999999,"prestress concrete girder",2.4,2.04,1,2.58,2.19,1,2.6,2.21,1,2.4,2.04,1,2.58,2.19,1,2.6,2.21,1,2.83,2.41,1,3.09,2.63,1,3.09,2.63,1,2.83,2.41,1,3.09,2.63,1,3.09,2.63,1,2.54,2.16,1,2.78,2.36,1,2.78,2.36,1,2.54,2.16,1,2.78,2.36,1,2.78,2.36,1]
["022200000814490","02",95,2014,32.838561999999996,-97.227587,"prestress concrete girder",2.4500000000000002,2.08,1,2.52,2.14,1,2.52,2.14,1,2.4500000000000002,2.08,1,2.52,2.14,1,2.52,2.14,1,2.98,2.5299999999999998,1,3.04,2.58,1,3.04,2.58,1,2.98,2.5299999999999998,1,3.04,2.58,1,3.04,2.58,1,2.68,2.2799999999999998,1,2.73,2.3199999999999998,1,2.73,2.3199999999999998,1,2.68,2.2799999999999998,1,2.73,2.3199999999999998,1,2.73,2.3199999999999998,1]
["022200000814499","02",130,2013,32.839886999999997,-97.279407999999989,"prestress concrete girder",2.2599999999999998,1.92,1,2.54,2.16,1,2.69,2.29,1,2.2599999999999998,1.92,1,2.54,2.16,1,2.69,2.29,1,2.71,2.2999999999999998,1,2.96,2.52,1,3.19,2.71,1,2.71,2.2999999999999998,1,2.96,2.52,1,3.19,2.71,1,2.44,2.0699999999999998,1,2.66,2.2599999999999998,1,2.87,2.44,1,2.44,2.0699999999999998,1,2.66,2.2599999999999998,1,2.87,2.44,1]
["022200000814514","02",190,2014,32.82808,-97.205736999999999,"steel girder",2.1,1.79,1,2.27,1.93,1,2.4500000000000002,2.08,1,1.85,1.57,1,2.13,1.81,1,2.44,2.0699999999999998,1,2.4300000000000002,2.0699999999999998,1,2.63,2.2400000000000002,1,2.85,2.42,1,2.25,1.91,1,2.5499999999999998,2.17,1,2.85,2.42,1,2.19,1.86,1,2.36,2.0099999999999998,1,2.56,2.1800000000000002,1,2.02,1.72,1,2.2999999999999998,1.95,1,2.56,2.1800000000000002,1]
["022200000814521","02",130,2014,32.839549999999996,-97.300309999999996,"prestress concrete girder",2.2599999999999998,1.36,1,2.54,1.52,1,2.69,1.61,1,2.2599999999999998,1.36,1,2.54,1.52,1,2.69,1.61,1,2.71,1.63,1,2.96,1.78,1,3.19,1.91,1,2.71,1.63,1,2.96,1.78,1,3.19,1.91,1,2.44,1.46,1,2.66,1.6,1,2.87,1.72,1,2.44,1.46,1,2.66,1.6,1,2.87,1.72,1]
["022200000814525","02",100,2014,32.833773999999998,-97.199612999999999,"prestress concrete girder",2.4300000000000002,2.0699999999999998,1,2.5499999999999998,2.17,1,2.5499999999999998,2.17,1,2.4300000000000002,2.0699999999999998,1,2.5499999999999998,2.17,1,2.5499999999999998,2.17,1,2.91,2.4700000000000002,1,3.05,2.59,1,3.05,2.59,1,2.91,2.4700000000000002,1,3.05,2.59,1,3.05,2.59,1,2.62,2.23,1,2.74,2.33,1,2.74,2.33,1,2.62,2.23,1,2.74,2.33,1,2.74,2.33,1]
["022200000815227","02",110,1976,32.766132069999998,-97.476823730000007,"prestress concrete girder",1.97,0.74,4,2.12,0.79,4,2.14,0.8,4,1.97,0.74,4,2.12,0.79,4,2.14,0.8,4,2.3199999999999998,0.86,3,2.54,0.95,2,2.54,0.95,2,2.3199999999999998,0.86,3,2.54,0.95,2,2.54,0.95,2,2.09,0.77,4,2.2799999999999998,0.85,3,2.2799999999999998,0.85,3,2.09,0.77,4,2.2799999999999998,0.85,3,2.2799999999999998,0.85,3]
["022200000815228","02",110,1976,32.766123069999999,-97.476923740000004,"prestress concrete girder",1.97,0.83,3,2.12,0.89,3,2.14,0.9,3,1.97,0.83,3,2.12,0.89,3,2.14,0.9,3,2.3199999999999998,0.98,2,2.54,1.07,1,2.54,1.07,1,2.3199999999999998,0.98,2,2.54,1.07,1,2.54,1.07,1,2.09,0.88,3,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.09,0.88,3,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2]
["022200000815294","02",120,1982,32.724467330000003,-97.480525810000003,"prestress concrete girder",1.87,0.7,5,2.04,0.76,4,2.13,0.79,4,1.87,0.7,5,2.04,0.76,4,2.13,0.79,4,2.2200000000000002,0.83,3,2.41,0.89,3,2.5099999999999998,0.93,2,2.2200000000000002,0.83,3,2.41,0.89,3,2.5099999999999998,0.93,2,1.99,0.74,4,2.17,0.8,4,2.2599999999999998,0.84,3,1.99,0.74,4,2.17,0.8,4,2.2599999999999998,0.84,3]
["022200000815300","02",130,1982,32.711785820000003,-97.477470699999998,"prestress concrete girder",1.76,0.65,5,1.97,0.74,4,2.1,0.78,4,1.76,0.65,5,1.97,0.74,4,2.1,0.78,4,2.11,0.78,4,2.2999999999999998,0.86,3,2.48,0.92,2,2.11,0.78,4,2.2999999999999998,0.86,3,2.48,0.92,2,1.9,0.71,4,2.0699999999999998,0.77,4,2.23,0.83,3,1.9,0.71,4,2.0699999999999998,0.77,4,2.23,0.83,3]
["022200000816251","02",120,1995,32.683077310000002,-97.400239319999997,"prestress concrete girder",1.87,0.56000000000000005,5,2.04,0.61,5,2.13,0.63,5,1.87,0.56000000000000005,5,2.04,0.61,5,2.13,0.63,5,2.2200000000000002,0.66,5,2.41,0.71,4,2.5099999999999998,0.74,4,2.2200000000000002,0.66,5,2.41,0.71,4,2.5099999999999998,0.74,4,1.99,0.59,5,2.17,0.64,5,2.2599999999999998,0.67,5,1.99,0.59,5,2.17,0.64,5,2.2599999999999998,0.67,5]
["022200001415331","02",80,1970,32.927565909999998,-97.361185849999998,"prestress concrete girder",2.29,0.81,3,2.29,0.81,3,2.29,0.81,3,2.29,0.81,3,2.29,0.81,3,2.29,0.81,3,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3]
["022200001415383","02",75,1976,32.960245200000003,-97.407217090000003,"prestress concrete girder",2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2]
["022200001416189","02",55,1961,32.76793095,-97.317912050000004,"concrete bridge",1.62,0.48,5,1.88,0.56000000000000005,5,2.2400000000000002,0.67,5,1.62,0.48,5,1.89,0.56000000000000005,5,2.2400000000000002,0.67,5,2.11,0.62,5,2.34,0.7,5,2.75,0.82,3,2.11,0.62,5,2.35,0.7,5,2.75,0.82,3,1.88,0.56000000000000005,5,2.11,0.62,5,2.48,0.74,4,1.88,0.56000000000000005,5,2.11,0.62,5,2.48,0.74,4]
["022200001416391","02",85,1981,32.712954689999997,-97.32056197,"prestress concrete girder",2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.39,1,2,2.39,1,2,2.39,1,2,2.39,1,2,2.39,1,2,2.39,1,2]
["022200001416408","02",70,1988,32.718581489999998,-97.320547980000001,"prestress concrete girder",2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1]
["022200001416457","02",120,2001,32.861300450000002,-97.314812399999994,"prestress concrete girder",1.87,0.79,4,2.04,0.86,3,2.13,0.89,3,1.87,0.79,4,2.04,0.86,3,2.13,0.89,3,2.2200000000000002,0.94,2,2.41,1.01,1,2.5099999999999998,1.05,1,2.2200000000000002,0.94,2,2.41,1.01,1,2.5099999999999998,1.05,1,1.99,0.84,3,2.17,0.91,2,2.2599999999999998,0.95,2,1.99,0.84,3,2.17,0.91,2,2.2599999999999998,0.95,2]
["022200001416459","02",95,2001,32.86280678,-97.315094619999996,"prestress concrete girder",2.1,0.88,3,2.16,0.91,2,2.16,0.91,2,2.1,0.88,3,2.16,0.91,2,2.16,0.91,2,2.5499999999999998,1.07,1,2.6,1.1000000000000001,1,2.6,1.1000000000000001,1,2.5499999999999998,1.07,1,2.6,1.1000000000000001,1,2.6,1.1000000000000001,1,2.2999999999999998,0.97,2,2.34,0.99,2,2.34,0.99,2,2.2999999999999998,0.97,2,2.34,0.99,2,2.34,0.99,2]
["022200001416478","02",125,2000,32.745887549999999,-97.318856740000001,"steel girder",1.47,0.96,2,1.63,1.07,1,1.73,1.1299999999999999,1,1.48,0.97,2,1.63,1.07,1,1.73,1.1299999999999999,1,1.76,1.1599999999999999,1,1.92,1.26,1,2.04,1.33,1,1.76,1.1599999999999999,1,1.92,1.26,1,2.04,1.33,1,1.59,1.04,1,1.72,1.1200000000000001,1,1.83,1.2,1,1.59,1.04,1,1.72,1.1200000000000001,1,1.83,1.2,1]
["022200001416539","02",130,2014,32.872954669999999,-97.317529339999993,"prestress concrete girder",2.2599999999999998,1.92,1,2.54,2.16,1,2.69,2.29,1,2.2599999999999998,1.92,1,2.54,2.16,1,2.69,2.29,1,2.71,2.2999999999999998,1,2.96,2.52,1,3.19,2.71,1,2.71,2.2999999999999998,1,2.96,2.52,1,3.19,2.71,1,2.44,2.0699999999999998,1,2.66,2.2599999999999998,1,2.87,2.44,1,2.44,2.0699999999999998,1,2.66,2.2599999999999998,1,2.87,2.44,1]
["022200001416541","02",95,2014,32.862609999999997,-97.315419999999989,"prestress concrete girder",2.4500000000000002,2.4500000000000002,1,2.52,2.52,1,2.52,2.52,1,2.4500000000000002,2.4500000000000002,1,2.52,2.52,1,2.52,2.52,1,2.98,2.98,1,3.04,3.04,1,3.04,3.04,1,2.98,2.98,1,3.04,3.04,1,3.04,3.04,1,2.68,2.68,1,2.73,2.73,1,2.73,2.73,1,2.68,2.68,1,2.73,2.73,1,2.73,2.73,1]
["022200001416573","02",90,2016,32.840409999999999,-97.31259,"prestress concrete girder",2.4900000000000002,2.4900000000000002,1,2.5,2.5,1,2.5,2.5,1,2.4900000000000002,2.4900000000000002,1,2.5,2.5,1,2.5,2.5,1,3.02,3.02,1,3.02,3.02,1,3.02,3.02,1,3.02,3.02,1,3.02,3.02,1,3.02,3.02,1,2.72,2.72,1,2.72,2.72,1,2.72,2.72,1,2.72,2.72,1,2.72,2.72,1,2.72,2.72,1]
["022200001416593","02",235,2016,32.808720000000001,-97.314889999999991,"steel girder",2.15,2.15,1,2.2799999999999998,2.2799999999999998,1,2.41,2.41,1,1.74,1.74,1,1.92,1.92,1,2.15,2.15,1,2.46,2.46,1,2.61,2.61,1,2.77,2.77,1,2.06,2.06,1,2.29,2.29,1,2.58,2.58,1,2.2200000000000002,2.2200000000000002,1,2.35,2.35,1,2.4900000000000002,2.4900000000000002,1,1.85,1.85,1,2.06,2.06,1,2.3199999999999998,2.3199999999999998,1]
["022200001416601","02",120,2016,32.760259999999995,-97.318269999999998,"prestress concrete girder",2.33,2.33,1,2.5499999999999998,2.5499999999999998,1,2.66,2.66,1,2.33,2.33,1,2.5499999999999998,2.5499999999999998,1,2.66,2.66,1,2.77,2.77,1,3.01,3.01,1,3.14,3.14,1,2.77,2.77,1,3.01,3.01,1,3.14,3.14,1,2.4900000000000002,2.4900000000000002,1,2.71,2.71,1,2.82,2.82,1,2.4900000000000002,2.4900000000000002,1,2.71,2.71,1,2.82,2.82,1]
["022200001416619","02",145,2016,32.790100000000002,-97.321389999999994,"prestress concrete girder",2.1800000000000002,2.1800000000000002,1,2.42,2.42,1,2.67,2.67,1,2.16,2.16,1,2.42,2.42,1,2.67,2.67,1,2.57,2.57,1,2.89,2.89,1,3.11,3.11,1,2.57,2.57,1,2.89,2.89,1,3.11,3.11,1,2.31,2.31,1,2.6,2.6,1,2.8,2.8,1,2.31,2.31,1,2.6,2.6,1,2.8,2.8,1]
["022200001416628","02",270,2018,32.769103999999999,-97.318517999999997,"Multi Span Long","Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1]
["022200008112077","02",60,1990,32.975274669999997,-97.308354730000005,"prestress concrete girder",2.2799999999999998,0.85,3,2.2799999999999998,0.85,3,2.2799999999999998,0.85,3,2.2799999999999998,0.85,3,2.2799999999999998,0.85,3,2.2799999999999998,0.85,3,2.94,1.1000000000000001,1,2.94,1.1000000000000001,1,2.94,1.1000000000000001,1,2.94,1.1000000000000001,1,2.94,1.1000000000000001,1,2.94,1.1000000000000001,1,2.64,0.98,2,2.64,0.98,2,2.64,0.98,2,2.64,0.98,2,2.64,0.98,2,2.64,0.98,2]
["022200008112222","02",80,1997,32.974902900000004,-97.307721650000005,"prestress concrete girder",2.19,0.92,2,2.19,0.92,2,2.19,0.92,2,2.2000000000000002,0.93,2,2.2000000000000002,0.93,2,2.2000000000000002,0.93,2,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1]
["022200008112223","02",65,1997,32.975041390000001,-97.307861149999994,"prestress concrete girder",2.25,0.94,2,2.25,0.94,2,2.25,0.94,2,2.25,0.94,2,2.25,0.94,2,2.25,0.94,2,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.56,1.08,1,2.56,1.08,1,2.56,1.08,1,2.56,1.08,1,2.56,1.08,1,2.56,1.08,1]
["022200009402067","02",125,1974,32.836086000000002,-97.035613999999995,"prestress concrete girder",1.81,0.68,5,2,0.74,4,2.12,0.79,4,1.81,0.68,5,2,0.74,4,2.12,0.79,4,2.16,0.8,4,2.35,0.87,3,2.5,0.93,2,2.16,0.8,4,2.35,0.87,3,2.5,0.93,2,1.95,0.73,4,2.12,0.79,4,2.25,0.83,3,1.95,0.73,4,2.12,0.79,4,2.25,0.83,3]
["022200009402069","02",80,1974,32.836449270000003,-97.040001110000006,"prestress concrete girder",2.19,0.92,2,2.19,0.92,2,2.19,0.92,2,2.2000000000000002,0.93,2,2.2000000000000002,0.93,2,2.2000000000000002,0.93,2,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1]
["022200035303433","02",140,2012,32.922412999999999,-97.07819099999999,"prestress concrete girder",2.2000000000000002,1.87,1,2.46,2.09,1,2.68,2.2799999999999998,1,2.19,1.86,1,2.46,2.09,1,2.68,2.2799999999999998,1,2.61,2.2200000000000002,1,2.92,2.48,1,3.13,2.66,1,2.61,2.2200000000000002,1,2.92,2.48,1,3.13,2.66,1,2.34,1.99,1,2.62,2.23,1,2.81,2.39,1,2.34,1.99,1,2.62,2.23,1,2.81,2.39,1]
["022200036401411","02",120,2001,32.833436249999998,-97.202588950000006,"prestress concrete girder",1.87,0.79,4,2.04,0.86,3,2.13,0.89,3,1.87,0.79,4,2.04,0.86,3,2.13,0.89,3,2.2200000000000002,0.94,2,2.41,1.01,1,2.5099999999999998,1.05,1,2.2200000000000002,0.94,2,2.41,1.01,1,2.5099999999999998,1.05,1,1.99,0.84,3,2.17,0.91,2,2.2599999999999998,0.95,2,1.99,0.84,3,2.17,0.91,2,2.2599999999999998,0.95,2]
["022200036401674","02",100,2014,32.839257789999998,-97.189158219999996,"prestress concrete girder",2.4300000000000002,2.0699999999999998,1,2.5499999999999998,2.17,1,2.5499999999999998,2.17,1,2.4300000000000002,2.0699999999999998,1,2.5499999999999998,2.17,1,2.5499999999999998,2.17,1,2.91,2.4700000000000002,1,3.05,2.59,1,3.05,2.59,1,2.91,2.4700000000000002,1,3.05,2.59,1,3.05,2.59,1,2.62,2.23,1,2.74,2.33,1,2.74,2.33,1,2.62,2.23,1,2.74,2.33,1,2.74,2.33,1]
["022200036401688","02",115,2014,32.839273999999996,-97.150579999999991,"prestress concrete girder",2.38,2.38,1,2.56,2.56,1,2.63,2.63,1,2.38,2.38,1,2.56,2.56,1,2.63,2.63,1,2.8,2.8,1,3.05,3.05,1,3.12,3.12,1,2.8,2.8,1,3.05,3.05,1,3.12,3.12,1,2.52,2.52,1,2.75,2.75,1,2.8,2.8,1,2.52,2.52,1,2.75,2.75,1,2.8,2.8,1]
["022200050402470","02",75,2014,32.645273869999997,-97.416461650000002,"prestress concrete girder",2.4300000000000002,2.4300000000000002,1,2.4300000000000002,2.4300000000000002,1,2.4300000000000002,2.4300000000000002,1,2.4300000000000002,2.4300000000000002,1,2.4300000000000002,2.4300000000000002,1,2.4300000000000002,2.4300000000000002,1,3.01,3.01,1,3.01,3.01,1,3.01,3.01,1,3.01,3.01,1,3.01,3.01,1,3.01,3.01,1,2.7,2.7,1,2.7,2.7,1,2.7,2.7,1,2.7,2.7,1,2.7,2.7,1,2.7,2.7,1]
["022200050402483","02",115,2014,32.688259080000002,-97.410461889999993,"prestress concrete girder",2.38,2.38,1,2.56,2.56,1,2.63,2.63,1,2.38,2.38,1,2.56,2.56,1,2.63,2.63,1,2.8,2.8,1,3.05,3.05,1,3.12,3.12,1,2.8,2.8,1,3.05,3.05,1,3.12,3.12,1,2.52,2.52,1,2.75,2.75,1,2.8,2.8,1,2.52,2.52,1,2.75,2.75,1,2.8,2.8,1]
["022200106801117","02",60,1989,32.734697320000002,-97.418681960000001,"concrete bridge",1.55,0.57999999999999996,5,1.73,0.65,5,2.04,0.76,4,1.55,0.57999999999999996,5,1.73,0.65,5,2.04,0.76,4,1.98,0.74,4,2.2200000000000002,0.83,3,2.5299999999999998,0.94,2,1.98,0.74,4,2.2200000000000002,0.83,3,2.5299999999999998,0.94,2,1.77,0.66,5,1.99,0.74,4,2.27,0.84,3,1.77,0.66,5,1.99,0.74,4,2.27,0.84,3]
["022200106801126","02",65,1965,32.737812810000001,-97.483503920000004,"prestress concrete girder",2.21,0.88,3,2.21,0.88,3,2.21,0.88,3,2.21,0.88,3,2.21,0.88,3,2.21,0.88,3,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.52,1,2,2.52,1,2,2.52,1,2,2.52,1,2,2.52,1,2,2.52,1,2]
["022200106801138","02",85,1975,32.720816249999999,-97.533515489999999,"prestress concrete girder",2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.39,1,2,2.39,1,2,2.39,1,2,2.39,1,2,2.39,1,2,2.39,1,2]
["022200106801289","02",125,2000,32.742838669999998,-97.339774129999995,"prestress concrete girder",1.81,0.77,4,2,0.84,3,2.12,0.89,3,1.81,0.77,4,2,0.84,3,2.12,0.89,3,2.16,0.91,2,2.35,0.99,2,2.5,1.05,1,2.16,0.91,2,2.35,0.99,2,2.5,1.05,1,1.95,0.82,3,2.12,0.89,3,2.25,0.94,2,1.95,0.82,3,2.12,0.89,3,2.25,0.94,2]
["022200106801293","02",150,2000,32.742476600000003,-97.338980680000006,"steel girder",1.33,0.87,3,1.47,0.96,2,1.63,1.07,1,1.3,0.85,3,1.47,0.96,2,1.63,1.07,1,1.56,1.02,1,1.75,1.1499999999999999,1,1.9,1.24,1,1.56,1.02,1,1.75,1.1499999999999999,1,1.9,1.24,1,1.4,0.92,2,1.57,1.03,1,1.71,1.1200000000000001,1,1.4,0.92,2,1.57,1.03,1,1.71,1.1200000000000001,1]
["022200106801483","02",120,2000,32.745164889999998,-97.335661610000002,"prestress concrete girder",1.87,0.79,4,2.04,0.86,3,2.13,0.89,3,1.87,0.79,4,2.04,0.86,3,2.13,0.89,3,2.2200000000000002,0.94,2,2.41,1.01,1,2.5099999999999998,1.05,1,2.2200000000000002,0.94,2,2.41,1.01,1,2.5099999999999998,1.05,1,1.99,0.84,3,2.17,0.91,2,2.2599999999999998,0.95,2,1.99,0.84,3,2.17,0.91,2,2.2599999999999998,0.95,2]
["022200106801563","02",100,2017,32.729340000000001,-97.50376,"prestress concrete girder",2.4300000000000002,2.4300000000000002,1,2.5499999999999998,2.5499999999999998,1,2.5499999999999998,2.5499999999999998,1,2.4300000000000002,2.4300000000000002,1,2.5499999999999998,2.5499999999999998,1,2.5499999999999998,2.5499999999999998,1,2.91,2.91,1,3.05,3.05,1,3.05,3.05,1,2.91,2.91,1,3.05,3.05,1,3.05,3.05,1,2.62,2.62,1,2.74,2.74,1,2.74,2.74,1,2.62,2.62,1,2.74,2.74,1,2.74,2.74,1]
["022200106802037","02",70,1957,32.759694619999998,-97.190884280000006,"concrete bridge",1.54,0.46,5,1.6,0.47,5,1.75,0.52,5,1.54,0.46,5,1.61,0.48,5,1.75,0.52,5,1.87,0.56000000000000005,5,1.97,0.59,5,2.2000000000000002,0.65,5,1.87,0.56000000000000005,5,1.97,0.59,5,2.2000000000000002,0.65,5,1.67,0.5,5,1.77,0.53,5,1.97,0.59,5,1.67,0.5,5,1.77,0.53,5,1.97,0.59,5]
["022200106802047","02",95,1957,32.760225630000001,-97.158411340000001,"steel girder",1.49,0.69,5,1.44,0.67,5,1.43,0.66,5,1.38,0.64,5,1.44,0.67,5,1.43,0.66,5,1.7,0.79,4,1.66,0.77,4,1.66,0.77,4,1.61,0.74,4,1.66,0.77,4,1.66,0.77,4,1.53,0.71,4,1.49,0.69,5,1.49,0.69,5,1.45,0.67,5,1.49,0.69,5,1.49,0.69,5]
["022200106802058","02",105,1957,32.760007999999999,-97.057631000000001,"steel girder",1.63,0.95,2,1.55,0.89,3,1.52,0.88,3,1.37,0.79,4,1.49,0.86,3,1.52,0.88,3,1.83,1.06,1,1.76,1.02,1,1.73,1,2,1.6,0.92,2,1.73,1,2,1.73,1,2,1.65,0.95,2,1.58,0.92,2,1.56,0.9,3,1.44,0.83,3,1.56,0.9,3,1.56,0.9,3]
["022200106802271","02",90,1957,32.746354590000003,-97.308668679999997,"steel girder",2.2799999999999998,1.51,1,2.29,1.52,1,2.29,1.52,1,2.2799999999999998,1.51,1,2.29,1.52,1,2.29,1.52,1,2.77,1.83,1,2.77,1.83,1,2.77,1.83,1,2.77,1.83,1,2.77,1.83,1,2.77,1.83,1,2.4900000000000002,1.64,1,2.4900000000000002,1.64,1,2.4900000000000002,1.64,1,2.4900000000000002,1.64,1,2.4900000000000002,1.64,1,2.4900000000000002,1.64,1]
["022200106802284","02",50,1997,32.760402829999997,-97.239857819999997,"prestress concrete girder",2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,3.2,1.34,1,3.2,1.34,1,3.2,1.34,1,3.2,1.34,1,3.2,1.34,1,3.2,1.34,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1]
["022200106802286","02",110,1997,32.75993991,-97.15066161,"prestress concrete girder",1.97,0.83,3,2.12,0.89,3,2.14,0.9,3,1.97,0.83,3,2.12,0.89,3,2.14,0.9,3,2.3199999999999998,0.98,2,2.54,1.07,1,2.54,1.07,1,2.3199999999999998,0.98,2,2.54,1.07,1,2.54,1.07,1,2.09,0.88,3,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.09,0.88,3,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2]
["022200106802288","02",90,1997,32.759646330000002,-97.136661939999996,"prestress concrete girder",2.16,0.91,2,2.17,0.91,2,2.17,0.91,2,2.16,0.91,2,2.17,0.91,2,2.17,0.91,2,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2]
["022200106802302","02",90,2000,32.757987550000003,-97.261736330000005,"prestress concrete girder",2.16,0.91,2,2.17,0.91,2,2.17,0.91,2,2.16,0.91,2,2.17,0.91,2,2.17,0.91,2,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2]
["022200106802332","02",85,1983,32.760729999999995,-97.217649999999992,"prestress concrete girder",2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.66,0.99,2,2.66,0.99,2,2.66,0.99,2,2.66,0.99,2,2.66,0.99,2,2.66,0.99,2,2.39,0.89,3,2.39,0.89,3,2.39,0.89,3,2.39,0.89,3,2.39,0.89,3,2.39,0.89,3]
["022200106802376","02",200,1991,32.760327580000002,-97.212127899999999,"Multi Span Long",0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1]
["022200106802551","02",120,2017,32.759659999999997,-97.063629999999989,"prestress concrete girder",2.33,2.33,1,2.5499999999999998,2.5499999999999998,1,2.66,2.66,1,2.33,2.33,1,2.5499999999999998,2.5499999999999998,1,2.66,2.66,1,2.77,2.77,1,3.01,3.01,1,3.14,3.14,1,2.77,2.77,1,3.01,3.01,1,3.14,3.14,1,2.4900000000000002,2.4900000000000002,1,2.71,2.71,1,2.82,2.82,1,2.4900000000000002,2.4900000000000002,1,2.71,2.71,1,2.82,2.82,1]
["022200106802554","02",120,2017,32.759219999999999,-97.062939999999998,"prestress concrete girder",2.33,2.33,1,2.5499999999999998,2.5499999999999998,1,2.66,2.66,1,2.33,2.33,1,2.5499999999999998,2.5499999999999998,1,2.66,2.66,1,2.77,2.77,1,3.01,3.01,1,3.14,3.14,1,2.77,2.77,1,3.01,3.01,1,3.14,3.14,1,2.4900000000000002,2.4900000000000002,1,2.71,2.71,1,2.82,2.82,1,2.4900000000000002,2.4900000000000002,1,2.71,2.71,1,2.82,2.82,1]
["022200106802557","02",70,2017,32.759920000000001,-97.066019999999995,"prestress concrete girder",2.42,2.42,1,2.42,2.42,1,2.42,2.42,1,2.42,2.42,1,2.42,2.42,1,2.42,2.42,1,3.03,3.03,1,3.03,3.03,1,3.03,3.03,1,3.03,3.03,1,3.03,3.03,1,3.03,3.03,1,2.71,2.71,1,2.71,2.71,1,2.71,2.71,1,2.71,2.71,1,2.71,2.71,1,2.71,2.71,1]
["022200106802567","02",215,2017,32.756239999999998,-97.063180000000003,"Multi Span Long","Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1]
["022200106802568","02",245,2017,32.75685,-97.063200000000009,"Multi Span Long","Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1]
["022200226602092","02",70,1992,32.860750510000003,-97.06488195,"prestress concrete girder",2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1]
["022200237405232","02",100,1973,32.668797580000003,-97.231164140000004,"prestress concrete girder",2.3199999999999998,0.82,3,2.4300000000000002,0.86,3,2.4300000000000002,0.86,3,2.3199999999999998,0.82,3,2.4300000000000002,0.86,3,2.4300000000000002,0.86,3,2.78,0.98,2,2.91,1.03,1,2.91,1.03,1,2.78,0.98,2,2.91,1.03,1,2.91,1.03,1,2.5099999999999998,0.89,3,2.62,0.92,2,2.62,0.92,2,2.5099999999999998,0.89,3,2.62,0.92,2,2.62,0.92,2]
["022200237405275","02",65,1974,32.674475409999999,-97.157766499999994,"prestress concrete girder",2.25,0.94,2,2.25,0.94,2,2.25,0.94,2,2.25,0.94,2,2.25,0.94,2,2.25,0.94,2,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.56,1.08,1,2.56,1.08,1,2.56,1.08,1,2.56,1.08,1,2.56,1.08,1,2.56,1.08,1]
["022200237405279","02",110,2010,32.675396300000003,-97.134816229999998,"prestress concrete girder",2.4,1.8,1,2.58,1.94,1,2.6,1.95,1,2.4,1.8,1,2.58,1.94,1,2.6,1.95,1,2.83,2.12,1,3.09,2.3199999999999998,1,3.09,2.3199999999999998,1,2.83,2.12,1,3.09,2.3199999999999998,1,3.09,2.3199999999999998,1,2.54,1.91,1,2.78,2.09,1,2.78,2.09,1,2.54,1.91,1,2.78,2.09,1,2.78,2.09,1]
["022200237405289","02",85,1975,32.677106639999998,-97.063053190000005,"prestress concrete girder",2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.66,0.99,2,2.66,0.99,2,2.66,0.99,2,2.66,0.99,2,2.66,0.99,2,2.66,0.99,2,2.39,0.89,3,2.39,0.89,3,2.39,0.89,3,2.39,0.89,3,2.39,0.89,3,2.39,0.89,3]
["022490001306059","02",55,1981,33.368745689999997,-97.705333600000003,"prestress concrete girder",2.31,0.97,2,2.31,0.97,2,2.31,0.97,2,2.31,0.97,2,2.31,0.97,2,2.31,0.97,2,3.05,1.28,1,3.05,1.28,1,3.05,1.28,1,3.05,1.28,1,3.05,1.28,1,3.05,1.28,1,2.73,1.1499999999999999,1,2.73,1.1499999999999999,1,2.73,1.1499999999999999,1,2.73,1.1499999999999999,1,2.73,1.1499999999999999,1,2.73,1.1499999999999999,1]
["022490001306068","02",85,1977,33.387199080000002,-97.72017898,"prestress concrete girder",2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.39,1,2,2.39,1,2,2.39,1,2,2.39,1,2,2.39,1,2,2.39,1,2]
["022490001308053","02",85,1972,33.055765919999999,-97.478637759999998,"prestress concrete girder",2.3199999999999998,0.82,3,2.3199999999999998,0.82,3,2.3199999999999998,0.82,3,2.3199999999999998,0.82,3,2.3199999999999998,0.82,3,2.3199999999999998,0.82,3,2.83,1,2,2.83,1,2,2.83,1,2,2.83,1,2,2.83,1,2,2.83,1,2,2.54,0.89,3,2.54,0.89,3,2.54,0.89,3,2.54,0.89,3,2.54,0.89,3,2.54,0.89,3]
["030390004402111","03",75,1997,33.880830330000002,-98.410636929999995,"prestress concrete girder",2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2]
["030490019401001","03",110,1984,33.727054580000001,-97.159869720000003,"steel girder",1.71,0.99,2,1.62,0.94,2,1.57,0.91,2,1.37,0.79,4,1.5,0.87,3,1.56,0.9,3,1.91,1.1000000000000001,1,1.82,1.05,1,1.78,1.03,1,1.59,0.92,2,1.74,1.01,1,1.78,1.03,1,1.72,0.99,2,1.64,0.95,2,1.6,0.92,2,1.43,0.83,3,1.57,0.91,2,1.6,0.92,2]
["030490019402035","03",65,2013,33.640689719999997,-97.155807479999993,"prestress concrete girder",2.4,2.04,1,2.4,2.04,1,2.4,2.04,1,2.4,2.04,1,2.4,2.04,1,2.4,2.04,1,3.05,2.59,1,3.05,2.59,1,3.05,2.59,1,3.05,2.59,1,3.05,2.59,1,3.05,2.59,1,2.74,2.33,1,2.74,2.33,1,2.74,2.33,1,2.74,2.33,1,2.74,2.33,1,2.74,2.33,1]
["031690001305051","03",95,1972,33.437717480000003,-97.762650579999999,"prestress concrete girder",2.33,0.94,2,2.39,0.95,2,2.39,0.95,2,2.33,0.94,2,2.39,0.95,2,2.39,0.95,2,2.83,1.1299999999999999,1,2.88,1.1499999999999999,1,2.88,1.1499999999999999,1,2.83,1.1299999999999999,1,2.88,1.1499999999999999,1,2.88,1.1499999999999999,1,2.5499999999999998,1.02,1,2.59,1.04,1,2.59,1.04,1,2.5499999999999998,1.02,1,2.59,1.04,1,2.59,1.04,1]
["031690022403052","03",115,1977,33.541779759999997,-97.844273689999994,"prestress concrete girder",1.93,0.82,3,2.08,0.88,3,2.13,0.89,3,1.93,0.82,3,2.08,0.88,3,2.13,0.89,3,2.27,0.95,2,2.4700000000000002,1.04,1,2.5299999999999998,1.06,1,2.27,0.95,2,2.4700000000000002,1.04,1,2.5299999999999998,1.06,1,2.04,0.86,3,2.23,0.94,2,2.27,0.95,2,2.04,0.86,3,2.23,0.94,2,2.27,0.95,2]
["032430004308120","03",80,1968,34.044204829999998,-98.917545540000006,"prestress concrete girder",2.29,0.81,3,2.29,0.81,3,2.29,0.81,3,2.29,0.81,3,2.29,0.81,3,2.29,0.81,3,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3]
["032430004309075","03",45,1961,33.965869429999998,-98.690545470000004,"concrete bridge",1.87,0.79,4,2.35,0.99,2,2.42,1.02,1,1.87,0.79,4,2.35,0.99,2,2.42,1.02,1,2.35,0.99,2,2.56,1.08,1,2.56,1.08,1,2.35,0.99,2,2.56,1.08,1,2.56,1.08,1,2.12,0.89,3,2.2999999999999998,0.97,2,2.2999999999999998,0.97,2,2.12,0.89,3,2.2999999999999998,0.97,2,2.2999999999999998,0.97,2]
["032430004309095","03",80,1961,33.944929639999998,-98.525490759999997,"concrete bridge",1.63,0.61,5,1.63,0.61,5,1.68,0.62,5,1.63,0.61,5,1.63,0.61,5,1.68,0.62,5,1.91,0.71,4,1.93,0.72,4,2.0299999999999998,0.75,4,1.91,0.71,4,1.93,0.72,4,2.0299999999999998,0.75,4,1.71,0.64,5,1.73,0.65,5,1.82,0.68,5,1.71,0.64,5,1.73,0.65,5,1.82,0.68,5]
["032430004309200","03",65,2001,33.91011151,-98.502710640000004,"steel girder",1.25,0.82,3,1.33,0.87,3,1.51,0.99,2,1.25,0.82,3,1.33,0.87,3,1.51,0.99,2,1.54,1.01,1,1.68,1.1000000000000001,1,1.93,1.27,1,1.54,1.01,1,1.68,1.1000000000000001,1,1.93,1.27,1,1.38,0.9,3,1.51,0.99,2,1.73,1.1299999999999999,1,1.38,0.9,3,1.51,0.99,2,1.73,1.1299999999999999,1]
["032430004401084","03",120,2001,33.898120759999998,-98.492340600000006,"prestress concrete special",1.87,0.7,0,2.04,0.76,0,2.13,0.79,0,1.87,0.7,0,2.04,0.76,0,2.13,0.79,0,2.2200000000000002,0.83,0,2.41,0.89,0,2.5099999999999998,0.93,0,2.2200000000000002,0.83,0,2.41,0.89,0,2.5099999999999998,0.93,0,1.99,0.74,0,2.17,0.8,0,2.2599999999999998,0.84,0,1.99,0.74,0,2.17,0.8,0,2.2599999999999998,0.84,0]
["032430004401120","03",130,1972,33.885975119999998,-98.448637169999998,"prestress concrete girder",2.23,0.79,4,2.5,0.88,3,2.66,0.94,2,2.23,0.79,4,2.5,0.88,3,2.66,0.94,2,2.68,0.95,2,2.92,1.03,1,3.14,1.1100000000000001,1,2.68,0.95,2,2.92,1.03,1,3.14,1.1100000000000001,1,2.4,0.85,3,2.63,0.93,2,2.83,1,2,2.4,0.85,3,2.63,0.93,2,2.83,1,2]
["032430015604060","03",80,2009,33.872504929999998,-98.569698970000005,"prestress concrete girder",2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1]
["032430015604061","03",80,2009,33.872306930000001,-98.569769969999996,"prestress concrete girder",2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1]
["032430015604080","03",75,1988,33.885495859999999,-98.528226720000006,"prestress concrete girder",2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2]
["032430015604086","03",100,1990,33.890721839999998,-98.511815220000003,"prestress concrete special",1.91,0.81,0,1.83,0.77,0,1.8,0.76,0,1.69,0.71,0,1.8,0.76,0,1.8,0.76,0,2.16,0.91,0,2.09,0.88,0,2.08,0.88,0,2,0.84,0,2.08,0.88,0,2.08,0.88,0,1.94,0.82,0,1.88,0.79,0,1.87,0.79,0,1.8,0.76,0,1.87,0.79,0,1.87,0.79,0]
["032430015604105","03",95,2003,33.880824660000002,-98.541144099999997,"prestress concrete girder",2.1,0.88,3,2.16,0.91,2,2.16,0.91,2,2.1,0.88,3,2.16,0.91,2,2.16,0.91,2,2.5499999999999998,1.07,1,2.6,1.1000000000000001,1,2.6,1.1000000000000001,1,2.5499999999999998,1.07,1,2.6,1.1000000000000001,1,2.6,1.1000000000000001,1,2.2999999999999998,0.97,2,2.34,0.99,2,2.34,0.99,2,2.2999999999999998,0.97,2,2.34,0.99,2,2.34,0.99,2]
["032430015607031","03",65,1964,33.969169110000003,-98.531405019999994,"prestress concrete girder",2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3]
["032430015607043","03",75,1964,34.091374510000001,-98.557459109999996,"prestress concrete girder",2.2599999999999998,0.8,4,2.2599999999999998,0.8,4,2.2599999999999998,0.8,4,2.2599999999999998,0.8,4,2.2599999999999998,0.8,4,2.2599999999999998,0.8,4,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3]
["032430015607096","03",115,1961,33.942722709999998,-98.521703630000005,"concrete bridge",2.16,0.8,4,2.06,0.77,4,1.99,0.74,4,1.7,0.63,5,1.86,0.69,5,1.96,0.73,4,2.44,0.91,2,2.3199999999999998,0.86,3,2.25,0.83,3,1.94,0.72,4,2.16,0.8,4,2.2400000000000002,0.83,3,2.19,0.81,3,2.08,0.77,4,2.02,0.75,4,1.75,0.65,5,1.94,0.72,4,2.0099999999999998,0.74,4]
["032430015607203","03",70,2009,33.952366480000002,-98.526499810000004,"prestress concrete girder",2.42,2.06,1,2.42,2.06,1,2.42,2.06,1,2.42,2.06,1,2.42,2.06,1,2.42,2.06,1,3.03,2.58,1,3.03,2.58,1,3.03,2.58,1,3.03,2.58,1,3.03,2.58,1,3.03,2.58,1,2.71,2.2999999999999998,1,2.71,2.2999999999999998,1,2.71,2.2999999999999998,1,2.71,2.2999999999999998,1,2.71,2.2999999999999998,1,2.71,2.2999999999999998,1]
["032440004305101","03",45,1985,34.178618999999998,-99.322806999999997,"concrete bridge",2.42,0.72,4,2.42,0.72,4,2.42,0.72,4,2.4300000000000002,0.72,4,2.42,0.72,4,2.42,0.72,4,3.23,0.96,2,3.23,0.96,2,3.23,0.96,2,3.23,0.96,2,3.23,0.96,2,3.23,0.96,2,2.92,0.87,3,2.92,0.87,3,2.92,0.87,3,2.92,0.87,3,2.92,0.87,3,2.92,0.87,3]
["040330027504092","04",85,1971,35.206704999999999,-101.16981,"prestress concrete girder",2.3199999999999998,0.82,3,2.3199999999999998,0.82,3,2.3199999999999998,0.82,3,2.3199999999999998,0.82,3,2.3199999999999998,0.82,3,2.3199999999999998,0.82,3,2.83,1,2,2.83,1,2,2.83,1,2,2.83,1,2,2.83,1,2,2.83,1,2,2.54,0.89,3,2.54,0.89,3,2.54,0.89,3,2.54,0.89,3,2.54,0.89,3,2.54,0.89,3]
["040330027504121","04",90,1978,35.213128999999995,-101.116822,"prestress concrete girder",2.16,0.8,4,2.17,0.8,4,2.17,0.8,4,2.16,0.8,4,2.17,0.8,4,2.17,0.8,4,2.63,0.98,2,2.63,0.98,2,2.63,0.98,2,2.63,0.98,2,2.63,0.98,2,2.63,0.98,2,2.36,0.88,3,2.36,0.88,3,2.36,0.88,3,2.36,0.88,3,2.36,0.88,3,2.36,0.88,3]
["040330027504122","04",90,1978,35.212652999999996,-101.11746599999999,"prestress concrete girder",2.16,0.91,2,2.17,0.91,2,2.17,0.91,2,2.16,0.91,2,2.17,0.91,2,2.17,0.91,2,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2]
["040910027511145","04",75,1984,35.226698999999996,-100.58721300000001,"prestress concrete girder",2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2]
["040910027511146","04",75,1984,35.226408999999997,-100.587874,"prestress concrete girder",2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2]
["041800009003036","04",75,1969,35.263525229999999,-102.74441349,"steel girder",1.29,0.59,5,1.31,0.61,5,1.38,0.64,5,1.29,0.59,5,1.31,0.61,5,1.38,0.64,5,1.53,0.71,4,1.58,0.73,4,1.7,0.79,4,1.53,0.71,4,1.58,0.73,4,1.7,0.79,4,1.37,0.63,5,1.41,0.65,5,1.52,0.7,5,1.37,0.63,5,1.41,0.65,5,1.52,0.7,5]
["041800022603023","04",80,2005,35.513930950000002,-102.25943267,"prestress concrete girder",2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1]
["041880016810133","04",65,1998,35.191275999999995,-101.837765,"steel girder",1.25,0.72,4,1.33,0.77,4,1.51,0.87,3,1.25,0.72,4,1.33,0.77,4,1.51,0.87,3,1.54,0.89,3,1.68,0.97,2,1.93,1.1200000000000001,1,1.54,0.89,3,1.68,0.97,2,1.93,1.1200000000000001,1,1.38,0.8,4,1.51,0.87,3,1.73,1,2,1.38,0.8,4,1.51,0.87,3,1.73,1,2]
["041880027501036","04",95,1966,35.191320159999997,-101.88397299,"steel girder",1.49,0.86,3,1.44,0.83,3,1.43,0.83,3,1.38,0.8,4,1.44,0.83,3,1.43,0.83,3,1.7,0.98,2,1.66,0.96,2,1.66,0.96,2,1.61,0.93,2,1.66,0.96,2,1.66,0.96,2,1.53,0.89,3,1.49,0.86,3,1.49,0.86,3,1.45,0.84,3,1.49,0.86,3,1.49,0.86,3]
["041880027501128","04",80,1969,35.187152410000003,-101.96817634,"prestress concrete girder",2.29,0.81,3,2.29,0.81,3,2.29,0.81,3,2.29,0.81,3,2.29,0.81,3,2.29,0.81,3,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3]
["041910006717106","04",100,1981,34.837711779999999,-101.84814686999999,"prestress concrete girder",2.0499999999999998,0.76,4,2.15,0.8,4,2.15,0.8,4,2.0499999999999998,0.76,4,2.15,0.8,4,2.15,0.8,4,2.46,0.92,2,2.58,0.96,2,2.58,0.96,2,2.46,0.92,2,2.58,0.96,2,2.58,0.96,2,2.2200000000000002,0.83,3,2.3199999999999998,0.86,3,2.3199999999999998,0.86,3,2.2200000000000002,0.83,3,2.3199999999999998,0.86,3,2.3199999999999998,0.86,3]
["041910006717139","04",120,1986,34.979564009999997,-101.88045871,"prestress concrete girder",1.87,0.7,5,2.04,0.76,4,2.13,0.79,4,1.87,0.7,5,2.04,0.76,4,2.13,0.79,4,2.2200000000000002,0.83,3,2.41,0.89,3,2.5099999999999998,0.93,2,2.2200000000000002,0.83,3,2.41,0.89,3,2.5099999999999998,0.93,2,1.99,0.74,4,2.17,0.8,4,2.2599999999999998,0.84,3,1.99,0.74,4,2.17,0.8,4,2.2599999999999998,0.84,3]
["041910016809027","04",75,1990,35.175359290000003,-101.85508003,"steel girder",1.29,0.74,4,1.31,0.76,4,1.38,0.8,4,1.29,0.74,4,1.31,0.76,4,1.38,0.8,4,1.53,0.89,3,1.58,0.92,2,1.7,0.98,2,1.53,0.89,3,1.58,0.92,2,1.7,0.98,2,1.37,0.79,4,1.41,0.82,3,1.52,0.88,3,1.37,0.79,4,1.41,0.82,3,1.52,0.88,3]
["041910016809040","04",60,1990,35.169959390000002,-101.86597951,"steel girder",1.27,0.74,4,1.41,0.82,3,1.66,0.96,2,1.27,0.74,4,1.41,0.82,3,1.66,0.96,2,1.61,0.93,2,1.81,1.04,1,2.06,1.19,1,1.61,0.93,2,1.81,1.04,1,2.06,1.19,1,1.44,0.83,3,1.62,0.94,2,1.85,1.07,1,1.44,0.83,3,1.62,0.94,2,1.85,1.07,1]
["041910016809056","04",80,1985,35.146466770000004,-101.88666655999999,"prestress concrete girder",2.19,0.65,5,2.19,0.65,5,2.19,0.65,5,2.2000000000000002,0.65,5,2.2000000000000002,0.65,5,2.2000000000000002,0.65,5,2.7,0.8,4,2.7,0.8,4,2.7,0.8,4,2.7,0.8,4,2.7,0.8,4,2.7,0.8,4,2.42,0.72,4,2.42,0.72,4,2.42,0.72,4,2.42,0.72,4,2.42,0.72,4,2.42,0.72,4]
["041910016809070","04",70,1990,35.176635259999998,-101.84847876000001,"steel girder",1.26,0.73,4,1.31,0.76,4,1.43,0.83,3,1.26,0.73,4,1.31,0.76,4,1.43,0.83,3,1.52,0.88,3,1.61,0.93,2,1.79,1.04,1,1.52,0.88,3,1.61,0.93,2,1.79,1.04,1,1.36,0.79,4,1.44,0.83,3,1.61,0.93,2,1.36,0.79,4,1.44,0.83,3,1.61,0.93,2]
["041910016809166","04",80,2011,35.043258559999998,-101.9187706,"prestress concrete girder",2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1]
["050860005305085","05",70,1987,33.038558020000004,-101.19863699,"prestress concrete girder",2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1]
["050960006704051","05",60,1967,34.18752525,-101.74977065,"prestress concrete girder",2.2000000000000002,0.62,5,2.2000000000000002,0.62,5,2.2000000000000002,0.62,5,2.2000000000000002,0.62,5,2.2000000000000002,0.62,5,2.2000000000000002,0.62,5,2.84,0.8,4,2.84,0.8,4,2.84,0.8,4,2.84,0.8,4,2.84,0.8,4,2.84,0.8,4,2.5499999999999998,0.72,4,2.5499999999999998,0.72,4,2.5499999999999998,0.72,4,2.5499999999999998,0.72,4,2.5499999999999998,0.72,4,2.5499999999999998,0.72,4]
["050960006704053","05",65,1986,34.21009858,-101.7355726,"prestress concrete girder",2.25,0.67,5,2.25,0.67,5,2.25,0.67,5,2.25,0.67,5,2.25,0.67,5,2.25,0.67,5,2.86,0.85,3,2.86,0.85,3,2.86,0.85,3,2.86,0.85,3,2.86,0.85,3,2.86,0.85,3,2.56,0.76,4,2.56,0.76,4,2.56,0.76,4,2.56,0.76,4,2.56,0.76,4,2.56,0.76,4]
["051520005301073","05",55,1966,33.420032390000003,-101.64286416,"prestress concrete girder",2.19,0.77,4,2.19,0.77,4,2.19,0.77,4,2.19,0.77,4,2.19,0.77,4,2.19,0.77,4,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.59,0.92,2,2.59,0.92,2,2.59,0.92,2,2.59,0.92,2,2.59,0.92,2,2.59,0.92,2]
["051520005301191","05",115,2017,33.415050000000001,-101.63444,"prestress concrete girder",2.38,2.02,1,2.56,2.1800000000000002,1,2.63,2.2400000000000002,1,2.38,2.02,1,2.56,2.1800000000000002,1,2.63,2.2400000000000002,1,2.8,2.38,1,3.05,2.59,1,3.12,2.65,1,2.8,2.38,1,3.05,2.59,1,3.12,2.65,1,2.52,2.14,1,2.75,2.34,1,2.8,2.38,1,2.52,2.14,1,2.75,2.34,1,2.8,2.38,1]
["051520006707073","05",115,1978,33.643261379999998,-101.83577131,"prestress concrete girder",2.16,0.91,2,2.06,0.87,3,1.99,0.84,3,1.7,0.71,4,1.86,0.78,4,1.96,0.82,3,2.44,1.03,1,2.3199999999999998,0.98,2,2.25,0.94,2,1.94,0.82,3,2.16,0.91,2,2.2400000000000002,0.94,2,2.19,0.92,2,2.08,0.88,3,2.02,0.85,3,1.75,0.74,4,1.94,0.82,3,2.0099999999999998,0.84,3]
["051520006711183","05",130,1989,33.536839919999998,-101.84445321,"steel girder",1.7,0.98,2,1.88,1.0900000000000001,1,1.81,1.04,1,1.45,0.84,3,1.54,0.89,3,1.65,0.95,2,2.0499999999999998,1.19,1,2.12,1.22,1,2.02,1.17,1,1.63,0.95,2,1.77,1.02,1,1.9,1.1000000000000001,1,1.84,1.07,1,1.9,1.1000000000000001,1,1.82,1.05,1,1.47,0.85,3,1.59,0.92,2,1.71,0.99,2]
["051520006711187","05",115,1990,33.5801783,-101.84009503999999,"prestress concrete girder",1.93,0.72,4,2.08,0.77,4,2.13,0.79,4,1.93,0.72,4,2.08,0.77,4,2.13,0.79,4,2.27,0.84,3,2.4700000000000002,0.92,2,2.5299999999999998,0.94,2,2.27,0.84,3,2.4700000000000002,0.92,2,2.5299999999999998,0.94,2,2.04,0.76,4,2.23,0.83,3,2.27,0.84,3,2.04,0.76,4,2.23,0.83,3,2.27,0.84,3]
["051520006711207","05",135,1992,33.577842330000003,-101.84071501,"prestress concrete girder",1.71,0.64,5,1.92,0.71,4,2.06,0.77,4,1.71,0.64,5,1.92,0.71,4,2.06,0.77,4,2.04,0.76,4,2.2599999999999998,0.84,3,2.42,0.9,3,2.04,0.76,4,2.2599999999999998,0.84,3,2.42,0.9,3,1.83,0.68,5,2.0299999999999998,0.75,4,2.1800000000000002,0.81,3,1.83,0.68,5,2.0299999999999998,0.75,4,2.1800000000000002,0.81,3]
["051520006711212","05",85,2013,33.591785039999998,-101.84019825,"prestress concrete girder",2.4700000000000002,2.4700000000000002,1,2.4700000000000002,2.4700000000000002,1,2.4700000000000002,2.4700000000000002,1,2.4700000000000002,2.4700000000000002,1,2.4700000000000002,2.4700000000000002,1,2.4700000000000002,2.4700000000000002,1,3.01,3.01,1,3.01,3.01,1,3.01,3.01,1,3.01,3.01,1,3.01,3.01,1,3.01,3.01,1,2.71,2.71,1,2.71,2.71,1,2.71,2.71,1,2.71,2.71,1,2.71,2.71,1,2.71,2.71,1]
["051520006801015","05",60,1970,33.519704160000003,-101.84417684,"prestress concrete girder",2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.84,1,2,2.84,1,2,2.84,1,2,2.84,1,2,2.84,1,2,2.84,1,2,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3]
["051520006801088","05",260,1988,33.53066201,-101.84423507,"Multi Span Long",0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1]
["051520038001023","05",215,2009,33.577668959999997,-101.90145895000001,"Multi Span Long","Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1]
["051520078301094","05",115,2005,33.548810349999997,-101.93782127,"prestress concrete girder",2.38,2.02,1,2.56,2.1800000000000002,1,2.63,2.2400000000000002,1,2.38,2.02,1,2.56,2.1800000000000002,1,2.63,2.2400000000000002,1,2.8,2.38,1,3.05,2.59,1,3.12,2.65,1,2.8,2.38,1,3.05,2.59,1,3.12,2.65,1,2.52,2.14,1,2.75,2.34,1,2.8,2.38,1,2.52,2.14,1,2.75,2.34,1,2.8,2.38,1]
["051520078301099","05",115,2006,33.538634109999997,-101.93098171,"prestress concrete girder",2.38,2.02,1,2.56,2.1800000000000002,1,2.63,2.2400000000000002,1,2.38,2.02,1,2.56,2.1800000000000002,1,2.63,2.2400000000000002,1,2.8,2.38,1,3.05,2.59,1,3.12,2.65,1,2.8,2.38,1,3.05,2.59,1,3.12,2.65,1,2.52,2.14,1,2.75,2.34,1,2.8,2.38,1,2.52,2.14,1,2.75,2.34,1,2.8,2.38,1]
["052190006702118","05",105,1983,34.719752530000001,-101.84615488999999,"prestress concrete girder",2.0099999999999998,0.59,5,2.15,0.64,5,2.15,0.64,5,2.0099999999999998,0.59,5,2.15,0.64,5,2.15,0.64,5,2.39,0.71,4,2.56,0.76,4,2.56,0.76,4,2.39,0.71,4,2.56,0.76,4,2.56,0.76,4,2.15,0.64,5,2.2999999999999998,0.68,5,2.2999999999999998,0.68,5,2.15,0.64,5,2.2999999999999998,0.68,5,2.2999999999999998,0.68,5]
["052190006703136","05",105,1986,34.369135810000003,-101.76656909,"prestress concrete girder",2.0099999999999998,0.59,5,2.15,0.64,5,2.15,0.64,5,2.0099999999999998,0.59,5,2.15,0.64,5,2.15,0.64,5,2.39,0.71,4,2.56,0.76,4,2.56,0.76,4,2.39,0.71,4,2.56,0.76,4,2.56,0.76,4,2.15,0.64,5,2.2999999999999998,0.68,5,2.2999999999999998,0.68,5,2.15,0.64,5,2.2999999999999998,0.68,5,2.2999999999999998,0.68,5]
["052190006703148","05",70,1987,34.450937410000002,-101.7763994,"prestress concrete girder",2.23,0.83,3,2.23,0.83,3,2.23,0.83,3,2.23,0.83,3,2.23,0.83,3,2.23,0.83,3,2.79,1.04,1,2.79,1.04,1,2.79,1.04,1,2.79,1.04,1,2.79,1.04,1,2.79,1.04,1,2.5,0.93,2,2.5,0.93,2,2.5,0.93,2,2.5,0.93,2,2.5,0.93,2,2.5,0.93,2]
["060690000407069","06",70,1969,31.8139839,-102.40617537,"prestress concrete girder",2.23,0.79,4,2.23,0.79,4,2.23,0.79,4,2.23,0.79,4,2.23,0.79,4,2.23,0.79,4,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3]
["060690000407088","06",105,2002,31.787195910000001,-102.47897096,"prestress concrete girder",2.0099999999999998,0.74,4,2.15,0.8,4,2.15,0.8,4,2.0099999999999998,0.74,4,2.15,0.8,4,2.15,0.8,4,2.39,0.89,3,2.56,0.95,2,2.56,0.95,2,2.39,0.89,3,2.56,0.95,2,2.56,0.95,2,2.15,0.8,4,2.2999999999999998,0.86,3,2.2999999999999998,0.86,3,2.15,0.8,4,2.2999999999999998,0.86,3,2.2999999999999998,0.86,3]
["060690000513004","06",105,2007,31.85551289,-102.31632096,"prestress concrete girder",2.41,2.0499999999999998,1,2.57,2.1800000000000002,1,2.57,2.1800000000000002,1,2.41,2.0499999999999998,1,2.57,2.1800000000000002,1,2.57,2.1800000000000002,1,2.87,2.44,1,3.07,2.61,1,3.07,2.61,1,2.87,2.44,1,3.07,2.61,1,3.07,2.61,1,2.58,2.19,1,2.76,2.35,1,2.76,2.35,1,2.58,2.19,1,2.76,2.35,1,2.76,2.35,1]
["060690000513176","06",95,1966,31.837082599999999,-102.33653314999999,"steel girder",1.49,0.86,3,1.44,0.83,3,1.43,0.83,3,1.38,0.8,4,1.44,0.83,3,1.43,0.83,3,1.7,0.98,2,1.66,0.96,2,1.66,0.96,2,1.61,0.93,2,1.66,0.96,2,1.66,0.96,2,1.53,0.89,3,1.49,0.86,3,1.49,0.86,3,1.45,0.84,3,1.49,0.86,3,1.49,0.86,3]
["060690000513186","06",50,1966,31.86612526,-102.30216599000001,"prestress concrete girder",2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.99,1.06,1,2.99,1.06,1,2.99,1.06,1,2.99,1.06,1,2.99,1.06,1,2.99,1.06,1,2.67,0.94,2,2.67,0.94,2,2.67,0.94,2,2.67,0.94,2,2.67,0.94,2,2.67,0.94,2]
["061560000504206","06",70,1968,32.138476930000003,-101.80588028,"steel girder",1.26,0.82,3,1.31,0.86,3,1.43,0.94,2,1.26,0.82,3,1.31,0.86,3,1.43,0.94,2,1.52,0.99,2,1.61,1.05,1,1.79,1.17,1,1.52,0.99,2,1.61,1.05,1,1.79,1.17,1,1.36,0.89,3,1.44,0.94,2,1.61,1.05,1,1.36,0.89,3,1.44,0.94,2,1.61,1.05,1]
["061650000515273","06",75,2016,32.00453985,-102.01327399,"prestress concrete girder",2.4300000000000002,1.82,1,2.4300000000000002,1.82,1,2.4300000000000002,1.82,1,2.4300000000000002,1.82,1,2.4300000000000002,1.82,1,2.4300000000000002,1.82,1,3.01,2.2599999999999998,1,3.01,2.2599999999999998,1,3.01,2.2599999999999998,1,3.01,2.2599999999999998,1,3.01,2.2599999999999998,1,3.01,2.2599999999999998,1,2.7,2.0299999999999998,1,2.7,2.0299999999999998,1,2.7,2.0299999999999998,1,2.7,2.0299999999999998,1,2.7,2.0299999999999998,1,2.7,2.0299999999999998,1]
["061860014002103","06",100,1975,30.86313715,-102.58744866000001,"prestress concrete girder",2.0499999999999998,0.86,3,2.15,0.9,3,2.15,0.9,3,2.0499999999999998,0.86,3,2.15,0.9,3,2.15,0.9,3,2.46,1.04,1,2.58,1.0900000000000001,1,2.58,1.0900000000000001,1,2.46,1.04,1,2.58,1.0900000000000001,1,2.58,1.0900000000000001,1,2.2200000000000002,0.94,2,2.3199999999999998,0.98,2,2.3199999999999998,0.98,2,2.2200000000000002,0.94,2,2.3199999999999998,0.98,2,2.3199999999999998,0.98,2]
["061860044107087","06",110,1971,30.900390940000001,-103.05546698000001,"prestress concrete girder",2.31,0.82,3,2.5,0.88,3,2.5099999999999998,0.89,3,2.3199999999999998,0.82,3,2.5,0.88,3,2.5099999999999998,0.89,3,2.73,0.96,2,2.99,1.06,1,2.99,1.06,1,2.73,0.96,2,2.99,1.06,1,2.99,1.06,1,2.46,0.87,3,2.69,0.95,2,2.69,0.95,2,2.46,0.87,3,2.69,0.95,2,2.69,0.95,2]
["061860044107177","06",65,1982,30.941569999999999,-103.33327,"prestress concrete girder",2.25,0.94,2,2.25,0.94,2,2.25,0.94,2,2.25,0.94,2,2.25,0.94,2,2.25,0.94,2,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.56,1.08,1,2.56,1.08,1,2.56,1.08,1,2.56,1.08,1,2.56,1.08,1,2.56,1.08,1]
["061950000305089","06",90,1969,31.096262339999999,-104.04874647,"steel girder",1.43,0.83,3,1.39,0.8,4,1.4,0.81,3,1.36,0.79,4,1.39,0.8,4,1.4,0.81,3,1.64,0.95,2,1.62,0.94,2,1.64,0.95,2,1.61,0.93,2,1.62,0.94,2,1.64,0.95,2,1.47,0.85,3,1.45,0.84,3,1.47,0.85,3,1.45,0.84,3,1.45,0.84,3,1.47,0.85,3]
["061950000306076","06",60,1968,31.361473480000001,-103.6863644,"prestress concrete girder",2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.84,1,2,2.84,1,2,2.84,1,2,2.84,1,2,2.84,1,2,2.84,1,2,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3]
["061950000307057","06",50,1966,31.399716940000001,-103.52364149,"prestress concrete girder",2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.99,1.2,1,2.99,1.2,1,2.99,1.2,1,2.99,1.2,1,2.99,1.2,1,2.99,1.2,1,2.67,1.06,1,2.67,1.06,1,2.67,1.06,1,2.67,1.06,1,2.67,1.06,1,2.67,1.06,1]
["061950000307058","06",60,1966,31.399578959999999,-103.52176142,"prestress concrete girder",2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.84,1.1299999999999999,1,2.84,1.1299999999999999,1,2.84,1.1299999999999999,1,2.84,1.1299999999999999,1,2.84,1.1299999999999999,1,2.84,1.1299999999999999,1,2.5499999999999998,1.02,1,2.5499999999999998,1.02,1,2.5499999999999998,1.02,1,2.5499999999999998,1.02,1,2.5499999999999998,1.02,1,2.5499999999999998,1.02,1]
["061950000307085","06",55,1968,31.401927530000002,-103.56968026,"prestress concrete girder",2.19,0.88,3,2.19,0.88,3,2.19,0.88,3,2.19,0.88,3,2.19,0.88,3,2.19,0.88,3,2.89,1.1599999999999999,1,2.89,1.1599999999999999,1,2.89,1.1599999999999999,1,2.89,1.1599999999999999,1,2.89,1.1599999999999999,1,2.89,1.1599999999999999,1,2.59,1.04,1,2.59,1.04,1,2.59,1.04,1,2.59,1.04,1,2.59,1.04,1,2.59,1.04,1]
["061950044105148","06",75,1975,30.979789759999999,-103.58714849,"prestress concrete girder",2.21,0.93,2,2.21,0.93,2,2.21,0.93,2,2.21,0.93,2,2.21,0.93,2,2.21,0.93,2,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.46,1.04,1,2.46,1.04,1,2.46,1.04,1,2.46,1.04,1,2.46,1.04,1,2.46,1.04,1]
["061950044109115","06",60,1974,31.028689119999999,-103.89955573,"prestress concrete girder",2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1]
["062380000402064","06",90,1968,31.471591999999998,-103.337188,"steel girder",1.43,0.83,3,1.39,0.8,4,1.4,0.81,3,1.36,0.79,4,1.39,0.8,4,1.4,0.81,3,1.64,0.95,2,1.62,0.94,2,1.64,0.95,2,1.61,0.93,2,1.62,0.94,2,1.64,0.95,2,1.47,0.85,3,1.45,0.84,3,1.47,0.85,3,1.45,0.84,3,1.45,0.84,3,1.47,0.85,3]
["062380000404035","06",70,1965,31.57272601,-102.9097678,"prestress concrete girder",2.23,0.79,4,2.23,0.79,4,2.23,0.79,4,2.23,0.79,4,2.23,0.79,4,2.23,0.79,4,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3]
["062380000404083","06",80,1982,31.615910999999997,-102.811573,"prestress concrete girder",2.19,0.92,2,2.19,0.92,2,2.19,0.92,2,2.2000000000000002,0.93,2,2.2000000000000002,0.93,2,2.2000000000000002,0.93,2,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1]
["070480003504049","07",110,2009,31.184899860000002,-99.841339989999994,"prestress concrete girder",2.4,2.04,1,2.58,2.19,1,2.6,2.21,1,2.4,2.04,1,2.58,2.19,1,2.6,2.21,1,2.83,2.41,1,3.09,2.63,1,3.09,2.63,1,2.83,2.41,1,3.09,2.63,1,3.09,2.63,1,2.54,2.16,1,2.78,2.36,1,2.78,2.36,1,2.54,2.16,1,2.78,2.36,1,2.78,2.36,1]
["070530014101109","07",100,1976,30.705664160000001,-101.20170566,"prestress concrete girder",2.0499999999999998,0.86,3,2.15,0.9,3,2.15,0.9,3,2.0499999999999998,0.86,3,2.15,0.9,3,2.15,0.9,3,2.46,1.04,1,2.58,1.0900000000000001,1,2.58,1.0900000000000001,1,2.46,1.04,1,2.58,1.0900000000000001,1,2.58,1.0900000000000001,1,2.2200000000000002,0.94,2,2.3199999999999998,0.98,2,2.3199999999999998,0.98,2,2.2200000000000002,0.94,2,2.3199999999999998,0.98,2,2.3199999999999998,0.98,2]
["071340014108152","07",70,1978,30.46958678,-100.11355229999999,"prestress concrete girder",2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1]
["071340014108163","07",65,1978,30.4835989,-100.04940452,"prestress concrete girder",1.53,0.56999999999999995,5,1.64,0.61,5,1.86,0.69,5,1.53,0.56999999999999995,5,1.64,0.61,5,1.86,0.69,5,1.9,0.71,4,2.0699999999999998,0.77,4,2.37,0.88,3,1.9,0.71,4,2.0699999999999998,0.77,4,2.37,0.88,3,1.7,0.63,5,1.85,0.69,5,2.12,0.79,4,1.7,0.63,5,1.85,0.69,5,2.13,0.79,4]
["071340014108164","07",115,1978,30.48231577,-100.06803234,"prestress concrete girder",1.93,0.82,3,2.08,0.88,3,2.13,0.89,3,1.93,0.82,3,2.08,0.88,3,2.13,0.89,3,2.27,0.95,2,2.4700000000000002,1.04,1,2.5299999999999998,1.06,1,2.27,0.95,2,2.4700000000000002,1.04,1,2.5299999999999998,1.06,1,2.04,0.86,3,2.23,0.94,2,2.27,0.95,2,2.04,0.86,3,2.23,0.94,2,2.27,0.95,2]
["071340014109120","07",60,1975,30.502403739999998,-99.948564559999994,"prestress concrete girder",2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1]
["071340014109134","07",105,1975,30.526915580000001,-99.84241299,"prestress concrete girder",2.0099999999999998,0.84,3,2.15,0.9,3,2.15,0.9,3,2.0099999999999998,0.84,3,2.15,0.9,3,2.15,0.9,3,2.39,1,2,2.56,1.08,1,2.56,1.08,1,2.39,1,2,2.56,1.08,1,2.56,1.08,1,2.15,0.9,3,2.2999999999999998,0.97,2,2.2999999999999998,0.97,2,2.15,0.9,3,2.2999999999999998,0.97,2,2.2999999999999998,0.97,2]
["071340014201057","07",65,1968,30.352178949999999,-99.592646349999995,"prestress concrete girder",2.21,0.88,3,2.21,0.88,3,2.21,0.88,3,2.21,0.88,3,2.21,0.88,3,2.21,0.88,3,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.52,1,2,2.52,1,2,2.52,1,2,2.52,1,2,2.52,1,2,2.52,1,2]
["071340014201063","07",60,1967,30.306022609999999,-99.552976180000002,"prestress concrete girder",2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.84,1.1299999999999999,1,2.84,1.1299999999999999,1,2.84,1.1299999999999999,1,2.84,1.1299999999999999,1,2.84,1.1299999999999999,1,2.84,1.1299999999999999,1,2.5499999999999998,1.02,1,2.5499999999999998,1.02,1,2.5499999999999998,1.02,1,2.5499999999999998,1.02,1,2.5499999999999998,1.02,1,2.5499999999999998,1.02,1]
["071340014201093","07",110,1969,30.43891116,-99.713194709999996,"prestress concrete girder",2.31,0.55000000000000004,5,2.5,0.59,5,2.5099999999999998,0.59,5,2.3199999999999998,0.55000000000000004,5,2.5,0.59,5,2.5099999999999998,0.59,5,2.73,0.64,5,2.99,0.71,4,2.99,0.71,4,2.73,0.64,5,2.99,0.71,4,2.99,0.71,4,2.46,0.57999999999999996,5,2.69,0.63,5,2.69,0.63,5,2.46,0.57999999999999996,5,2.69,0.63,5,2.69,0.63,5]
["072000003405046","07",170,2016,31.743515420000001,-99.939516209999994,"steel girder",1.72,1.29,1,1.87,1.4,1,2.02,1.52,1,1.67,1.25,1,1.76,1.32,1,1.77,1.33,1,2.02,1.52,1,2.21,1.66,1,2.4,1.8,1,1.98,1.48,1,1.99,1.49,1,2.0299999999999998,1.52,1,1.82,1.37,1,1.98,1.48,1,2.15,1.61,1,1.78,1.34,1,1.79,1.34,1,1.82,1.37,1]
["072180014102064","07",45,1969,30.64962367,-100.91400591,"concrete bridge",2.4,0.85,3,2.4,0.85,3,2.4,0.85,3,2.41,0.85,3,2.4,0.85,3,2.4,0.85,3,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1]
["072180014102071","07",60,1969,30.62591952,-100.85006799,"prestress concrete girder",2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.84,1.1299999999999999,1,2.84,1.1299999999999999,1,2.84,1.1299999999999999,1,2.84,1.1299999999999999,1,2.84,1.1299999999999999,1,2.84,1.1299999999999999,1,2.5499999999999998,1.02,1,2.5499999999999998,1.02,1,2.5499999999999998,1.02,1,2.5499999999999998,1.02,1,2.5499999999999998,1.02,1,2.5499999999999998,1.02,1]
["072180014103086","07",95,1969,30.582766240000002,-100.65792613000001,"prestress concrete girder",2.33,0.94,2,2.39,0.95,2,2.39,0.95,2,2.33,0.94,2,2.39,0.95,2,2.39,0.95,2,2.83,1.1299999999999999,1,2.88,1.1499999999999999,1,2.88,1.1499999999999999,1,2.83,1.1299999999999999,1,2.88,1.1499999999999999,1,2.88,1.1499999999999999,1,2.5499999999999998,1.02,1,2.59,1.04,1,2.59,1.04,1,2.5499999999999998,1.02,1,2.59,1.04,1,2.59,1.04,1]
["072180014107139","07",80,1978,30.443913009999999,-100.21398159,"prestress concrete girder",2.19,0.81,3,2.19,0.81,3,2.19,0.81,3,2.2000000000000002,0.82,3,2.2000000000000002,0.82,3,2.2000000000000002,0.82,3,2.7,1.01,1,2.7,1.01,1,2.7,1.01,1,2.7,1.01,1,2.7,1.01,1,2.7,1.01,1,2.42,0.9,3,2.42,0.9,3,2.42,0.9,3,2.42,0.9,3,2.42,0.9,3,2.42,0.9,3]
["072260007002059","07",80,1972,31.41495527,-100.43940644,"prestress concrete girder",2.29,0.92,2,2.29,0.92,2,2.29,0.92,2,2.29,0.92,2,2.29,0.92,2,2.29,0.92,2,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.52,1,2,2.52,1,2,2.52,1,2,2.52,1,2,2.52,1,2,2.52,1,2]
["072260007706083","07",80,2003,31.442533780000002,-100.49836765000001,"prestress concrete girder",2.19,0.92,2,2.19,0.92,2,2.19,0.92,2,2.2000000000000002,0.93,2,2.2000000000000002,0.93,2,2.2000000000000002,0.93,2,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1]
["072260007706084","07",80,2003,31.441785020000001,-100.49850480000001,"prestress concrete girder",2.19,0.92,2,2.19,0.92,2,2.19,0.92,2,2.2000000000000002,0.93,2,2.2000000000000002,0.93,2,2.2000000000000002,0.93,2,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1]
["072260015802078","07",100,1990,31.478957269999999,-100.38780594000001,"prestress concrete girder",2.0499999999999998,0.86,3,2.15,0.9,3,2.15,0.9,3,2.0499999999999998,0.86,3,2.15,0.9,3,2.15,0.9,3,2.46,1.04,1,2.58,1.0900000000000001,1,2.58,1.0900000000000001,1,2.46,1.04,1,2.58,1.0900000000000001,1,2.58,1.0900000000000001,1,2.2200000000000002,0.94,2,2.3199999999999998,0.98,2,2.3199999999999998,0.98,2,2.2200000000000002,0.94,2,2.3199999999999998,0.98,2,2.3199999999999998,0.98,2]
["080300000607282","08",45,1965,32.41531647,-99.508220640000005,"concrete bridge",1.87,0.7,5,2.35,0.87,3,2.42,0.9,3,1.87,0.7,5,2.35,0.87,3,2.42,0.9,3,2.35,0.87,3,2.56,0.95,2,2.56,0.95,2,2.35,0.87,3,2.56,0.95,2,2.56,0.95,2,2.12,0.79,4,2.2999999999999998,0.86,3,2.2999999999999998,0.86,3,2.12,0.79,4,2.2999999999999998,0.86,3,2.2999999999999998,0.86,3]
["080300000607286","08",45,1964,32.412044389999998,-99.489680140000004,"concrete bridge",1.87,0.79,4,2.35,0.99,2,2.42,1.02,1,1.87,0.79,4,2.35,0.99,2,2.42,1.02,1,2.35,0.99,2,2.56,1.08,1,2.56,1.08,1,2.35,0.99,2,2.56,1.08,1,2.56,1.08,1,2.12,0.89,3,2.2999999999999998,0.97,2,2.2999999999999998,0.97,2,2.12,0.89,3,2.2999999999999998,0.97,2,2.2999999999999998,0.97,2]
["080300000701087","08",45,1965,32.391414589999997,-99.345091929999995,"concrete bridge",1.87,0.7,5,2.35,0.87,3,2.42,0.9,3,1.87,0.7,5,2.35,0.87,3,2.42,0.9,3,2.35,0.87,3,2.56,0.95,2,2.56,0.95,2,2.35,0.87,3,2.56,0.95,2,2.56,0.95,2,2.12,0.79,4,2.2999999999999998,0.86,3,2.2999999999999998,0.86,3,2.12,0.79,4,2.2999999999999998,0.86,3,2.2999999999999998,0.86,3]
["080300000701089","08",45,1965,32.385799079999998,-99.298513310000004,"concrete bridge",1.87,0.79,4,2.35,0.99,2,2.42,1.02,1,1.87,0.79,4,2.35,0.99,2,2.42,1.02,1,2.35,0.99,2,2.56,1.08,1,2.56,1.08,1,2.35,0.99,2,2.56,1.08,1,2.56,1.08,1,2.12,0.89,3,2.2999999999999998,0.97,2,2.2999999999999998,0.97,2,2.12,0.89,3,2.2999999999999998,0.97,2,2.2999999999999998,0.97,2]
["080300000702112","08",50,1983,32.377095599999997,-99.164940709999996,"steel girder",1.43,0.83,3,1.66,0.96,2,1.93,1.1200000000000001,1,1.43,0.83,3,1.66,0.96,2,1.93,1.1200000000000001,1,1.81,1.04,1,2.06,1.19,1,2.2599999999999998,1.31,1,1.81,1.04,1,2.06,1.19,1,2.2599999999999998,1.31,1,1.62,0.94,2,1.86,1.07,1,2.04,1.18,1,1.62,0.94,2,1.86,1.07,1,2.04,1.18,1]
["081150000505016","08",85,1980,32.224352570000001,-101.56296322999999,"steel girder",1.38,0.8,4,1.35,0.78,4,1.38,0.8,4,1.35,0.78,4,1.35,0.78,4,1.38,0.8,4,1.59,0.92,2,1.59,0.92,2,1.64,0.95,2,1.59,0.92,2,1.59,0.92,2,1.64,0.95,2,1.43,0.83,3,1.42,0.82,3,1.47,0.85,3,1.42,0.82,3,1.42,0.82,3,1.47,0.85,3]
["081150000505067","08",45,1958,32.176730319999997,-101.65920023,"concrete bridge",1.87,0.7,5,2.35,0.87,3,2.42,0.9,3,1.87,0.7,5,2.35,0.87,3,2.42,0.9,3,2.35,0.87,3,2.56,0.95,2,2.56,0.95,2,2.35,0.87,3,2.56,0.95,2,2.56,0.95,2,2.12,0.79,4,2.2999999999999998,0.86,3,2.2999999999999998,0.86,3,2.12,0.79,4,2.2999999999999998,0.86,3,2.2999999999999998,0.86,3]
["081150000506084","08",45,1959,32.2747867,-101.37051235,"concrete bridge",1.87,0.7,5,2.35,0.87,3,2.42,0.9,3,1.87,0.7,5,2.35,0.87,3,2.42,0.9,3,2.35,0.87,3,2.56,0.95,2,2.56,0.95,2,2.35,0.87,3,2.56,0.95,2,2.56,0.95,2,2.12,0.79,4,2.2999999999999998,0.86,3,2.2999999999999998,0.86,3,2.12,0.79,4,2.2999999999999998,0.86,3,2.2999999999999998,0.86,3]
["081150000506126","08",55,1991,32.262408499999999,-101.4549693,"steel girder",1.32,0.61,5,1.53,0.71,4,1.82,0.84,3,1.32,0.61,5,1.54,0.71,4,1.82,0.84,3,1.72,0.79,4,1.91,0.88,3,2.2400000000000002,1.03,1,1.72,0.79,4,1.91,0.88,3,2.2400000000000002,1.03,1,1.53,0.71,4,1.72,0.79,4,2.02,0.94,2,1.53,0.71,4,1.72,0.79,4,2.02,0.94,2]
["081680000508050","08",45,1957,32.356779979999999,-101.00613848,"concrete bridge",1.87,0.7,5,2.35,0.87,3,2.42,0.9,3,1.87,0.7,5,2.35,0.87,3,2.42,0.9,3,2.35,0.87,3,2.56,0.95,2,2.56,0.95,2,2.35,0.87,3,2.56,0.95,2,2.56,0.95,2,2.12,0.79,4,2.2999999999999998,0.86,3,2.2999999999999998,0.86,3,2.12,0.79,4,2.2999999999999998,0.86,3,2.2999999999999998,0.86,3]
["081680000508053","08",45,1957,32.376010960000002,-100.97609294999999,"concrete bridge",1.87,0.79,4,2.35,0.99,2,2.42,1.02,1,1.87,0.79,4,2.35,0.99,2,2.42,1.02,1,2.35,0.99,2,2.56,1.08,1,2.56,1.08,1,2.35,0.99,2,2.56,1.08,1,2.56,1.08,1,2.12,0.89,3,2.2999999999999998,0.97,2,2.2999999999999998,0.97,2,2.12,0.89,3,2.2999999999999998,0.97,2,2.2999999999999998,0.97,2]
["081680000508059","08",45,1957,32.392180349999997,-100.92733330999999,"concrete bridge",1.87,0.7,5,2.35,0.87,3,2.42,0.9,3,1.87,0.7,5,2.35,0.87,3,2.42,0.9,3,2.35,0.87,3,2.56,0.95,2,2.56,0.95,2,2.35,0.87,3,2.56,0.95,2,2.56,0.95,2,2.12,0.79,4,2.2999999999999998,0.86,3,2.2999999999999998,0.86,3,2.12,0.79,4,2.2999999999999998,0.86,3,2.2999999999999998,0.86,3]
["081680000508094","08",100,1990,32.399416029999998,-100.89381757,"prestress concrete girder",2.0499999999999998,0.76,4,2.15,0.8,4,2.15,0.8,4,2.0499999999999998,0.76,4,2.15,0.8,4,2.15,0.8,4,2.46,0.92,2,2.58,0.96,2,2.58,0.96,2,2.46,0.92,2,2.58,0.96,2,2.58,0.96,2,2.2200000000000002,0.83,3,2.3199999999999998,0.86,3,2.3199999999999998,0.86,3,2.2200000000000002,0.83,3,2.3199999999999998,0.86,3,2.3199999999999998,0.86,3]
["081680000508101","08",65,1962,32.407858189999999,-100.84345906,"steel girder",1.25,0.57999999999999996,5,1.33,0.61,5,1.51,0.7,5,1.25,0.57999999999999996,5,1.33,0.61,5,1.51,0.7,5,1.54,0.71,4,1.68,0.77,4,1.93,0.89,3,1.54,0.71,4,1.68,0.77,4,1.93,0.89,3,1.38,0.64,5,1.51,0.7,5,1.73,0.8,4,1.38,0.64,5,1.51,0.7,5,1.73,0.8,4]
["081680000601159","08",45,1958,32.415117940000002,-100.71317474,"concrete bridge",1.87,0.7,5,2.35,0.87,3,2.42,0.9,3,1.87,0.7,5,2.35,0.87,3,2.42,0.9,3,2.35,0.87,3,2.56,0.95,2,2.56,0.95,2,2.35,0.87,3,2.56,0.95,2,2.56,0.95,2,2.12,0.79,4,2.2999999999999998,0.86,3,2.2999999999999998,0.86,3,2.12,0.79,4,2.2999999999999998,0.86,3,2.2999999999999998,0.86,3]
["081770000602304","08",45,1967,32.41571519,-100.63523843999999,"concrete bridge",1.87,0.79,4,2.35,0.99,2,2.42,1.02,1,1.87,0.79,4,2.35,0.99,2,2.42,1.02,1,2.35,0.99,2,2.56,1.08,1,2.56,1.08,1,2.35,0.99,2,2.56,1.08,1,2.56,1.08,1,2.12,0.89,3,2.2999999999999998,0.97,2,2.2999999999999998,0.97,2,2.12,0.89,3,2.2999999999999998,0.97,2,2.2999999999999998,0.97,2]
["081770000602340","08",130,2013,32.445662689999999,-100.50721668,"prestress concrete girder",2.2599999999999998,2.2599999999999998,1,2.54,2.54,1,2.69,2.69,1,2.2599999999999998,2.2599999999999998,1,2.54,2.54,1,2.69,2.69,1,2.71,2.71,1,2.96,2.96,1,3.19,3.19,1,2.71,2.71,1,2.96,2.96,1,3.19,3.19,1,2.44,2.44,1,2.66,2.66,1,2.87,2.87,1,2.44,2.44,1,2.66,2.66,1,2.87,2.87,1]
["081770000603176","08",65,1959,32.488562829999999,-100.18073351,"prestress concrete girder",2.21,0.62,5,2.21,0.62,5,2.21,0.62,5,2.21,0.62,5,2.21,0.62,5,2.21,0.62,5,2.81,0.79,4,2.81,0.79,4,2.81,0.79,4,2.81,0.79,4,2.81,0.79,4,2.81,0.79,4,2.52,0.71,4,2.52,0.71,4,2.52,0.71,4,2.52,0.71,4,2.52,0.71,4,2.52,0.71,4]
["081770000603320","08",125,1997,32.494297690000003,-100.14826357,"prestress concrete girder",1.81,0.77,4,2,0.84,3,2.12,0.89,3,1.81,0.77,4,2,0.84,3,2.12,0.89,3,2.16,0.91,2,2.35,0.99,2,2.5,1.05,1,2.16,0.91,2,2.35,0.99,2,2.5,1.05,1,1.95,0.82,3,2.12,0.89,3,2.25,0.94,2,1.95,0.82,3,2.12,0.89,3,2.25,0.94,2]
["081770000603337","08",70,1999,32.489732600000004,-100.23748409,"prestress concrete girder",2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1]
["082080005308094","08",65,2004,32.748413890000002,-100.92508056,"prestress concrete girder",2.25,1.1100000000000001,1,2.25,1.1100000000000001,1,2.25,1.1100000000000001,1,2.25,1.1100000000000001,1,2.25,1.1100000000000001,1,2.25,1.1100000000000001,1,2.86,1.42,1,2.86,1.42,1,2.86,1.42,1,2.86,1.42,1,2.86,1.42,1,2.86,1.42,1,2.56,1.27,1,2.56,1.27,1,2.56,1.27,1,2.56,1.27,1,2.56,1.27,1,2.56,1.27,1]
["082210000604121","08",45,1958,32.477714429999999,-100.01137724,"concrete bridge",1.87,0.7,5,2.35,0.87,3,2.42,0.9,3,1.87,0.7,5,2.35,0.87,3,2.42,0.9,3,2.35,0.87,3,2.56,0.95,2,2.56,0.95,2,2.35,0.87,3,2.56,0.95,2,2.56,0.95,2,2.12,0.79,4,2.2999999999999998,0.86,3,2.2999999999999998,0.86,3,2.12,0.79,4,2.2999999999999998,0.86,3,2.2999999999999998,0.86,3]
["082210000605193","08",65,1961,32.459702030000003,-99.854985920000004,"concrete bridge",1.53,0.46,5,1.64,0.49,5,1.86,0.55000000000000004,5,1.53,0.46,5,1.64,0.49,5,1.86,0.55000000000000004,5,1.9,0.56000000000000005,5,2.0699999999999998,0.61,5,2.37,0.7,5,1.9,0.56000000000000005,5,2.0699999999999998,0.61,5,2.37,0.7,5,1.7,0.5,5,1.85,0.55000000000000004,5,2.12,0.63,5,1.7,0.5,5,1.85,0.55000000000000004,5,2.13,0.63,5]
["082210000605213","08",65,1961,32.471217760000002,-99.805051710000001,"concrete bridge",1.53,0.56999999999999995,5,1.64,0.61,5,1.86,0.69,5,1.53,0.56999999999999995,5,1.64,0.61,5,1.86,0.69,5,1.9,0.71,4,2.0699999999999998,0.77,4,2.37,0.88,3,1.9,0.71,4,2.0699999999999998,0.77,4,2.37,0.88,3,1.7,0.63,5,1.85,0.69,5,2.12,0.79,4,1.7,0.63,5,1.85,0.69,5,2.13,0.79,4]
["082210000605325","08",100,2008,32.48193552,-99.770703679999997,"prestress concrete girder",2.4300000000000002,2.0699999999999998,1,2.5499999999999998,2.17,1,2.5499999999999998,2.17,1,2.4300000000000002,2.0699999999999998,1,2.5499999999999998,2.17,1,2.5499999999999998,2.17,1,2.91,2.4700000000000002,1,3.05,2.59,1,3.05,2.59,1,2.91,2.4700000000000002,1,3.05,2.59,1,3.05,2.59,1,2.62,2.23,1,2.74,2.33,1,2.74,2.33,1,2.62,2.23,1,2.74,2.33,1,2.74,2.33,1]
["082210000606186","08",50,1990,32.46094403,-99.67735295,"steel girder",1.43,0.83,3,1.66,0.96,2,1.93,1.1200000000000001,1,1.43,0.83,3,1.66,0.96,2,1.93,1.1200000000000001,1,1.81,1.04,1,2.06,1.19,1,2.2599999999999998,1.31,1,1.81,1.04,1,2.06,1.19,1,2.2599999999999998,1.31,1,1.62,0.94,2,1.86,1.07,1,2.04,1.18,1,1.62,0.94,2,1.86,1.07,1,2.04,1.18,1]
["082210000606195","08",80,1961,32.4904096,-99.731218979999994,"steel girder",1.33,0.77,4,1.33,0.77,4,1.37,0.79,4,1.33,0.77,4,1.33,0.77,4,1.37,0.79,4,1.55,0.89,3,1.57,0.91,2,1.65,0.95,2,1.55,0.89,3,1.57,0.91,2,1.65,0.95,2,1.39,0.8,4,1.41,0.82,3,1.48,0.86,3,1.39,0.8,4,1.41,0.82,3,1.48,0.86,3]
["082210000618333","08",115,2010,32.45357817,-99.808181050000002,"prestress concrete girder",2.38,2.02,1,2.56,2.1800000000000002,1,2.63,2.2400000000000002,1,2.38,2.02,1,2.56,2.1800000000000002,1,2.63,2.2400000000000002,1,2.8,2.38,1,3.05,2.59,1,3.12,2.65,1,2.8,2.38,1,3.05,2.59,1,3.12,2.65,1,2.52,2.14,1,2.75,2.34,1,2.8,2.38,1,2.52,2.14,1,2.75,2.34,1,2.8,2.38,1]
["082210000618341","08",140,2015,32.456773210000001,-99.842427929999999,"prestress concrete girder",2.2000000000000002,1.87,1,2.46,2.09,1,2.68,2.2799999999999998,1,2.19,1.86,1,2.46,2.09,1,2.68,2.2799999999999998,1,2.61,2.2200000000000002,1,2.92,2.48,1,3.13,2.66,1,2.61,2.2200000000000002,1,2.92,2.48,1,3.13,2.66,1,2.34,1.99,1,2.62,2.23,1,2.81,2.39,1,2.34,1.99,1,2.62,2.23,1,2.81,2.39,1]
["082210003306079","08",90,1970,32.475252920000003,-99.775260079999995,"prestress concrete girder",2.35,0.83,3,2.36,0.83,3,2.36,0.83,3,2.35,0.83,3,2.36,0.83,3,2.36,0.83,3,2.85,1.01,1,2.85,1.01,1,2.85,1.01,1,2.85,1.01,1,2.85,1.01,1,2.85,1.01,1,2.56,0.9,3,2.56,0.9,3,2.56,0.9,3,2.56,0.9,3,2.56,0.9,3,2.56,0.9,3]
["082210003401064","08",90,2003,32.412847139999997,-99.775065479999995,"prestress concrete girder",2.16,0.91,2,2.17,0.91,2,2.17,0.91,2,2.16,0.91,2,2.17,0.91,2,2.17,0.91,2,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2]
["090140001504709","09",95,2016,31.128257999999999,-97.334700999999995,"prestress concrete special",2.4500000000000002,2.4500000000000002,0,2.52,2.52,0,2.52,2.52,0,2.4500000000000002,2.4500000000000002,0,2.52,2.52,0,2.52,2.52,0,2.98,2.98,0,3.04,3.04,0,3.04,3.04,0,2.98,2.98,0,3.04,3.04,0,3.04,3.04,0,2.68,2.68,0,2.73,2.73,0,2.73,2.73,0,2.68,2.68,0,2.73,2.73,0,2.73,2.73,0]
["090140001506531","09",140,2012,31.015671999999999,-97.483354999999989,"prestress concrete girder",2.2000000000000002,1.87,1,2.46,2.09,1,2.68,2.2799999999999998,1,2.19,1.86,1,2.46,2.09,1,2.68,2.2799999999999998,1,2.61,2.2200000000000002,1,2.92,2.48,1,3.13,2.66,1,2.61,2.2200000000000002,1,2.92,2.48,1,3.13,2.66,1,2.34,1.99,1,2.62,2.23,1,2.81,2.39,1,2.34,1.99,1,2.62,2.23,1,2.81,2.39,1]
["090140001506532","09",120,2016,31.001800000000003,-97.492000000000004,"prestress concrete girder",2.33,1.98,1,2.5499999999999998,2.17,1,2.66,2.2599999999999998,1,2.33,1.98,1,2.5499999999999998,2.17,1,2.66,2.2599999999999998,1,2.77,2.35,1,3.01,2.56,1,3.14,2.67,1,2.77,2.35,1,3.01,2.56,1,3.14,2.67,1,2.4900000000000002,2.12,1,2.71,2.2999999999999998,1,2.82,2.4,1,2.4900000000000002,2.12,1,2.71,2.2999999999999998,1,2.82,2.4,1]
["090140001507393","09",115,2008,30.917009999999998,-97.54755999999999,"prestress concrete special",2.38,2.02,0,2.56,2.1800000000000002,0,2.63,2.2400000000000002,0,2.38,2.02,0,2.56,2.1800000000000002,0,2.63,2.2400000000000002,0,2.8,2.38,0,3.05,2.59,0,3.12,2.65,0,2.8,2.38,0,3.05,2.59,0,3.12,2.65,0,2.52,2.14,0,2.75,2.34,0,2.8,2.38,0,2.52,2.14,0,2.75,2.34,0,2.8,2.38,0]
["090140001507545","09",135,2016,30.935433,-97.540115999999998,"prestress concrete girder",2.23,2.23,1,2.4900000000000002,2.4900000000000002,1,2.68,2.68,1,2.23,2.23,1,2.4900000000000002,2.4900000000000002,1,2.68,2.68,1,2.65,2.65,1,2.94,2.94,1,3.15,3.15,1,2.65,2.65,1,2.94,2.94,1,3.15,3.15,1,2.39,2.39,1,2.65,2.65,1,2.84,2.84,1,2.39,2.39,1,2.65,2.65,1,2.84,2.84,1]
["090140001507550","09",135,2016,30.954065,-97.53725399999999,"prestress concrete girder",2.23,2.23,1,2.4900000000000002,2.4900000000000002,1,2.68,2.68,1,2.23,2.23,1,2.4900000000000002,2.4900000000000002,1,2.68,2.68,1,2.65,2.65,1,2.94,2.94,1,3.15,3.15,1,2.65,2.65,1,2.94,2.94,1,3.15,3.15,1,2.39,2.39,1,2.65,2.65,1,2.84,2.84,1,2.39,2.39,1,2.65,2.65,1,2.84,2.84,1]
["090140001514371","09",65,1976,31.044843310000001,-97.467568270000001,"prestress concrete special",1.53,0.65,0,1.64,0.69,0,1.86,0.78,0,1.53,0.65,0,1.64,0.69,0,1.86,0.78,0,1.9,0.8,0,2.0699999999999998,0.87,0,2.37,0.99,0,1.9,0.8,0,2.0699999999999998,0.87,0,2.37,0.99,0,1.7,0.71,0,1.85,0.78,0,2.12,0.89,0,1.7,0.71,0,1.85,0.78,0,2.13,0.89,0]
["090140001514372","09",50,1977,31.06729,-97.42770999999999,"concrete bridge",1.75,0.65,5,2.04,0.76,4,2.37,0.88,3,1.75,0.65,5,2.04,0.76,4,2.37,0.88,3,2.2200000000000002,0.83,3,2.5299999999999998,0.94,2,2.77,1.03,1,2.2200000000000002,0.83,3,2.5299999999999998,0.94,2,2.77,1.03,1,1.99,0.74,4,2.2799999999999998,0.85,3,2.5,0.93,2,1.99,0.74,4,2.2799999999999998,0.85,3,2.5,0.93,2]
["090140001514397","09",105,2009,31.091235480000002,-97.387550509999997,"prestress concrete girder",2.41,2.0499999999999998,1,2.57,2.1800000000000002,1,2.57,2.1800000000000002,1,2.41,2.0499999999999998,1,2.57,2.1800000000000002,1,2.57,2.1800000000000002,1,2.87,2.44,1,3.07,2.61,1,3.07,2.61,1,2.87,2.44,1,3.07,2.61,1,3.07,2.61,1,2.58,2.19,1,2.76,2.35,1,2.76,2.35,1,2.58,2.19,1,2.76,2.35,1,2.76,2.35,1]
["090140001514482","09",90,2008,31.09069667,-97.387664400000006,"prestress concrete girder",2.4900000000000002,1.87,1,2.5,1.88,1,2.5,1.88,1,2.4900000000000002,1.87,1,2.5,1.88,1,2.5,1.88,1,3.02,2.27,1,3.02,2.27,1,3.02,2.27,1,3.02,2.27,1,3.02,2.27,1,3.02,2.27,1,2.72,2.04,1,2.72,2.04,1,2.72,2.04,1,2.72,2.04,1,2.72,2.04,1,2.72,2.04,1]
["090140023103068","09",90,2015,31.09479,-97.732309999999998,"prestress concrete girder",2.4900000000000002,2.12,1,2.5,2.13,1,2.5,2.13,1,2.4900000000000002,2.12,1,2.5,2.13,1,2.5,2.13,1,3.02,2.57,1,3.02,2.57,1,3.02,2.57,1,3.02,2.57,1,3.02,2.57,1,3.02,2.57,1,2.72,2.31,1,2.72,2.31,1,2.72,2.31,1,2.72,2.31,1,2.72,2.31,1,2.72,2.31,1]
["090140023103093","09",90,2015,31.109133069999999,-97.747709389999997,"prestress concrete girder",2.4900000000000002,2.12,1,2.5,2.13,1,2.5,2.13,1,2.4900000000000002,2.12,1,2.5,2.13,1,2.5,2.13,1,3.02,2.57,1,3.02,2.57,1,3.02,2.57,1,3.02,2.57,1,3.02,2.57,1,3.02,2.57,1,2.72,2.31,1,2.72,2.31,1,2.72,2.31,1,2.72,2.31,1,2.72,2.31,1,2.72,2.31,1]
["090140023103098","09",105,1976,31.083376179999998,-97.639244680000004,"prestress concrete girder",2.0099999999999998,0.84,3,2.15,0.9,3,2.15,0.9,3,2.0099999999999998,0.84,3,2.15,0.9,3,2.15,0.9,3,2.39,1,2,2.56,1.08,1,2.56,1.08,1,2.39,1,2,2.56,1.08,1,2.56,1.08,1,2.15,0.9,3,2.2999999999999998,0.97,2,2.2999999999999998,0.97,2,2.15,0.9,3,2.2999999999999998,0.97,2,2.2999999999999998,0.97,2]
["090140023104128","09",95,1978,31.054756789999999,-97.506625060000005,"prestress concrete girder",1.83,0.68,5,1.77,0.66,5,1.76,0.65,5,1.69,0.63,5,1.77,0.66,5,1.76,0.65,5,2.09,0.77,4,2.0299999999999998,0.75,4,2.04,0.76,4,1.98,0.74,4,2.0299999999999998,0.75,4,2.04,0.76,4,1.87,0.7,5,1.82,0.68,5,1.83,0.68,5,1.78,0.66,5,1.82,0.68,5,1.83,0.68,5]
["090500023119379","09",125,2015,31.095939999999999,-97.905500000000004,"prestress concrete special",2.29,2.29,0,2.54,2.54,0,2.69,2.69,0,2.2999999999999998,2.2999999999999998,0,2.54,2.54,0,2.69,2.69,0,2.74,2.74,0,2.98,2.98,0,3.17,3.17,0,2.74,2.74,0,2.98,2.98,0,3.17,3.17,0,2.4700000000000002,2.4700000000000002,0,2.68,2.68,0,2.85,2.85,0,2.4700000000000002,2.4700000000000002,0,2.68,2.68,0,2.85,2.85,0]
["090500023119386","09",340,2015,31.120700000000003,-97.858409999999992,"Multi Span Long","Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1]
["091100001423284","09",45,1965,32.242339549999997,-97.157935850000001,"concrete bridge",2.4,0.68,5,2.4,0.68,5,2.4,0.68,5,2.41,0.68,5,2.4,0.68,5,2.4,0.68,5,3.2,0.9,3,3.2,0.9,3,3.2,0.9,3,3.2,0.9,3,3.2,0.9,3,3.2,0.9,3,2.89,0.82,3,2.89,0.82,3,2.89,0.82,3,2.89,0.82,3,2.89,0.82,3,2.89,0.82,3]
["091100001423287","09",50,1965,32.230121949999997,-97.15398562,"concrete bridge",1.75,0.74,4,2.04,0.86,3,2.37,0.99,2,1.75,0.74,4,2.04,0.86,3,2.37,0.99,2,2.2200000000000002,0.94,2,2.5299999999999998,1.06,1,2.77,1.1599999999999999,1,2.2200000000000002,0.94,2,2.5299999999999998,1.06,1,2.77,1.1599999999999999,1,1.99,0.84,3,2.2799999999999998,0.96,2,2.5,1.05,1,1.99,0.84,3,2.2799999999999998,0.96,2,2.5,1.05,1]
["091100001424479","09",110,2001,32.017165040000002,-97.095773620000003,"prestress concrete girder",1.97,0.83,3,2.12,0.89,3,2.14,0.9,3,1.97,0.83,3,2.12,0.89,3,2.14,0.9,3,2.3199999999999998,0.98,2,2.54,1.07,1,2.54,1.07,1,2.3199999999999998,0.98,2,2.54,1.07,1,2.54,1.07,1,2.09,0.88,3,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.09,0.88,3,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2]
["091610001408519","09",125,2014,31.753933329999999,-97.104383330000005,"prestress concrete special",2.29,1.95,0,2.54,2.16,0,2.69,2.29,0,2.2999999999999998,1.95,0,2.54,2.16,0,2.69,2.29,0,2.74,2.33,0,2.98,2.5299999999999998,0,3.17,2.69,0,2.74,2.33,0,2.98,2.5299999999999998,0,3.17,2.69,0,2.4700000000000002,2.1,0,2.68,2.2799999999999998,0,2.85,2.42,0,2.4700000000000002,2.1,0,2.68,2.2799999999999998,0,2.85,2.42,0]
["091610001408520","09",125,2013,31.787649999999999,-97.103039999999993,"prestress concrete special",2.29,1.95,0,2.54,2.16,0,2.69,2.29,0,2.2999999999999998,1.95,0,2.54,2.16,0,2.69,2.29,0,2.74,2.33,0,2.98,2.5299999999999998,0,3.17,2.69,0,2.74,2.33,0,2.98,2.5299999999999998,0,3.17,2.69,0,2.4700000000000002,2.1,0,2.68,2.2799999999999998,0,2.85,2.42,0,2.4700000000000002,2.1,0,2.68,2.2799999999999998,0,2.85,2.42,0]
["091610001501099","09",115,2006,31.492972430000002,-97.151965739999994,"prestress concrete special",2.38,2.02,0,2.56,2.1800000000000002,0,2.63,2.2400000000000002,0,2.38,2.02,0,2.56,2.1800000000000002,0,2.63,2.2400000000000002,0,2.8,2.38,0,3.05,2.59,0,3.12,2.65,0,2.8,2.38,0,3.05,2.59,0,3.12,2.65,0,2.52,2.14,0,2.75,2.34,0,2.8,2.38,0,2.52,2.14,0,2.75,2.34,0,2.8,2.38,0]
["091610001501260","09",80,1991,31.534234609999999,-97.129908499999999,"concrete bridge",1.63,0.49,5,1.63,0.49,5,1.68,0.5,5,1.63,0.49,5,1.63,0.49,5,1.68,0.5,5,1.91,0.56999999999999995,5,1.93,0.57999999999999996,5,2.0299999999999998,0.6,5,1.91,0.56999999999999995,5,1.93,0.57999999999999996,5,2.0299999999999998,0.6,5,1.71,0.51,5,1.73,0.52,5,1.82,0.54,5,1.71,0.51,5,1.73,0.52,5,1.82,0.54,5]
["091610001501264","09",75,1966,31.550359270000001,-97.122945729999998,"concrete bridge",1.58,0.47,5,1.61,0.48,5,1.7,0.5,5,1.58,0.47,5,1.61,0.48,5,1.7,0.5,5,1.88,0.56000000000000005,5,1.93,0.57999999999999996,5,2.08,0.62,5,1.88,0.56000000000000005,5,1.93,0.57999999999999996,5,2.08,0.62,5,1.68,0.5,5,1.73,0.52,5,1.87,0.56000000000000005,5,1.68,0.5,5,1.73,0.52,5,1.87,0.56000000000000005,5]
["091610001501285","09",55,1970,31.560200340000002,-97.117288250000001,"concrete bridge",1.62,0.48,5,1.88,0.56000000000000005,5,2.2400000000000002,0.67,5,1.62,0.48,5,1.89,0.56000000000000005,5,2.2400000000000002,0.67,5,2.11,0.62,5,2.34,0.7,5,2.75,0.82,3,2.11,0.62,5,2.35,0.7,5,2.75,0.82,3,1.88,0.56000000000000005,5,2.11,0.62,5,2.48,0.74,4,1.88,0.56000000000000005,5,2.11,0.62,5,2.48,0.74,4]
["091610001501312","09",155,1971,31.524603989999999,-97.135024380000004,"steel girder",1.65,0.76,4,1.8,0.83,3,1.96,0.91,2,1.63,0.76,4,1.64,0.76,4,1.69,0.78,4,1.96,0.91,2,2.15,1,2,2.33,1.07,1,1.81,0.83,3,1.86,0.86,3,1.96,0.91,2,1.76,0.82,3,1.93,0.89,3,2.1,0.97,2,1.63,0.76,4,1.68,0.77,4,1.76,0.82,3]
["091610001501318","09",80,1972,31.604717919999999,-97.106508219999995,"prestress concrete girder",2.29,0.92,2,2.29,0.92,2,2.29,0.92,2,2.29,0.92,2,2.29,0.92,2,2.29,0.92,2,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.52,1,2,2.52,1,2,2.52,1,2,2.52,1,2,2.52,1,2,2.52,1,2]
["091610001501319","09",80,1972,31.604623,-97.106090379999998,"prestress concrete girder",2.29,0.92,2,2.29,0.92,2,2.29,0.92,2,2.29,0.92,2,2.29,0.92,2,2.29,0.92,2,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.52,1,2,2.52,1,2,2.52,1,2,2.52,1,2,2.52,1,2,2.52,1,2]
["091610001501540","09",125,2013,31.650373999999999,-97.099949999999993,"prestress concrete special",2.29,2.29,0,2.54,2.54,0,2.69,2.69,0,2.2999999999999998,2.2999999999999998,0,2.54,2.54,0,2.69,2.69,0,2.74,2.74,0,2.98,2.98,0,3.17,3.17,0,2.74,2.74,0,2.98,2.98,0,3.17,3.17,0,2.4700000000000002,2.4700000000000002,0,2.68,2.68,0,2.85,2.85,0,2.4700000000000002,2.4700000000000002,0,2.68,2.68,0,2.85,2.85,0]
["091610001501671","09",115,2011,31.471933,-97.16401599999999,"prestress concrete special",2.38,2.02,0,2.56,2.1800000000000002,0,2.63,2.2400000000000002,0,2.38,2.02,0,2.56,2.1800000000000002,0,2.63,2.2400000000000002,0,2.8,2.38,0,3.05,2.59,0,3.12,2.65,0,2.8,2.38,0,3.05,2.59,0,3.12,2.65,0,2.52,2.14,0,2.75,2.34,0,2.8,2.38,0,2.52,2.14,0,2.75,2.34,0,2.8,2.38,0]
["091610025809452","09",135,2018,31.494273,-97.13376199999999,"prestress concrete girder",2.23,2.23,1,2.4900000000000002,2.4900000000000002,1,2.68,2.68,1,2.23,2.23,1,2.4900000000000002,2.4900000000000002,1,2.68,2.68,1,2.65,2.65,1,2.94,2.94,1,3.15,3.15,1,2.65,2.65,1,2.94,2.94,1,3.15,3.15,1,2.39,2.39,1,2.65,2.65,1,2.84,2.84,1,2.39,2.39,1,2.65,2.65,1,2.84,2.84,1]
["100930049507254","10",65,1966,32.432351310000001,-94.902343939999994,"prestress concrete girder",2.21,0.88,3,2.21,0.88,3,2.21,0.88,3,2.21,0.88,3,2.21,0.88,3,2.21,0.88,3,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.52,1,2,2.52,1,2,2.52,1,2,2.52,1,2,2.52,1,2,2.52,1,2]
["100930049507256","10",65,1966,32.432515039999998,-94.86232545,"prestress concrete girder",2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3]
["100930049507279","10",70,1967,32.434541129999999,-94.82449287,"steel girder",1.26,0.73,4,1.31,0.76,4,1.43,0.83,3,1.26,0.73,4,1.31,0.76,4,1.43,0.83,3,1.52,0.88,3,1.61,0.93,2,1.79,1.04,1,1.52,0.88,3,1.61,0.93,2,1.79,1.04,1,1.36,0.79,4,1.44,0.83,3,1.61,0.93,2,1.36,0.79,4,1.44,0.83,3,1.61,0.93,2]
["100930049507280","10",45,1987,32.435120410000003,-94.820715010000001,"concrete bridge",2.42,0.72,4,2.42,0.72,4,2.42,0.72,4,2.4300000000000002,0.72,4,2.42,0.72,4,2.42,0.72,4,3.23,0.96,2,3.23,0.96,2,3.23,0.96,2,3.23,0.96,2,3.23,0.96,2,3.23,0.96,2,2.92,0.87,3,2.92,0.87,3,2.92,0.87,3,2.92,0.87,3,2.92,0.87,3,2.92,0.87,3]
["102120049505177","10",95,1964,32.441196470000001,-95.134088329999997,"steel girder",1.49,0.69,5,1.44,0.67,5,1.43,0.66,5,1.38,0.64,5,1.44,0.67,5,1.43,0.66,5,1.7,0.79,4,1.66,0.77,4,1.66,0.77,4,1.61,0.74,4,1.66,0.77,4,1.66,0.77,4,1.53,0.71,4,1.49,0.69,5,1.49,0.69,5,1.45,0.67,5,1.49,0.69,5,1.49,0.69,5]
["102120049506239","10",65,1966,32.436103539999998,-94.989605510000004,"prestress concrete girder",2.21,0.62,5,2.21,0.62,5,2.21,0.62,5,2.21,0.62,5,2.21,0.62,5,2.21,0.62,5,2.81,0.79,4,2.81,0.79,4,2.81,0.79,4,2.81,0.79,4,2.81,0.79,4,2.81,0.79,4,2.52,0.71,4,2.52,0.71,4,2.52,0.71,4,2.52,0.71,4,2.52,0.71,4,2.52,0.71,4]
["102340049502010","10",60,1963,32.647848250000003,-96.065736630000004,"steel girder",1.27,0.59,5,1.41,0.65,5,1.66,0.77,4,1.27,0.59,5,1.41,0.65,5,1.66,0.77,4,1.61,0.74,4,1.81,0.83,3,2.06,0.95,2,1.61,0.74,4,1.81,0.83,3,2.06,0.95,2,1.44,0.67,5,1.62,0.75,4,1.85,0.85,3,1.44,0.67,5,1.62,0.75,4,1.85,0.85,3]
["102340049502312","10",95,2000,32.577976069999998,-95.854865200000006,"prestress concrete girder",2.1,0.88,3,2.16,0.91,2,2.16,0.91,2,2.1,0.88,3,2.16,0.91,2,2.16,0.91,2,2.5499999999999998,1.07,1,2.6,1.1000000000000001,1,2.6,1.1000000000000001,1,2.5499999999999998,1.07,1,2.6,1.1000000000000001,1,2.6,1.1000000000000001,1,2.2999999999999998,0.97,2,2.34,0.99,2,2.34,0.99,2,2.2999999999999998,0.97,2,2.34,0.99,2,2.34,0.99,2]
["102340049503001","10",75,2005,32.506284600000001,-95.643205429999995,"prestress concrete girder",2.4300000000000002,2.0699999999999998,1,2.4300000000000002,2.0699999999999998,1,2.4300000000000002,2.0699999999999998,1,2.4300000000000002,2.0699999999999998,1,2.4300000000000002,2.0699999999999998,1,2.4300000000000002,2.0699999999999998,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1]
["102340049503096","10",45,1962,32.512184779999998,-95.674905809999998,"steel girder",1.52,0.7,5,1.92,0.89,3,1.97,0.91,2,1.52,0.7,5,1.92,0.89,3,1.97,0.91,2,1.92,0.89,3,2.08,0.96,2,2.08,0.96,2,1.92,0.89,3,2.08,0.96,2,2.08,0.96,2,1.73,0.8,4,1.87,0.86,3,1.87,0.86,3,1.73,0.8,4,1.87,0.86,3,1.87,0.86,3]
["111740017601141","11",70,1938,31.601716999999997,-94.657181999999992,"steel girder",2.14,1.42,1,2.14,1.42,1,2.14,1.42,1,2.14,1.42,1,2.14,1.42,1,2.14,1.42,1,2.69,1.78,1,2.69,1.78,1,2.69,1.78,1,2.69,1.78,1,2.69,1.78,1,2.69,1.78,1,2.41,1.59,1,2.41,1.59,1,2.41,1.59,1,2.41,1.59,1,2.41,1.59,1,2.41,1.59,1]
["111870017605085","11",110,1980,30.735196819999999,-94.930775179999998,"prestress concrete girder",1.97,0.74,4,2.12,0.79,4,2.14,0.8,4,1.97,0.74,4,2.12,0.79,4,2.14,0.8,4,2.3199999999999998,0.86,3,2.54,0.95,2,2.54,0.95,2,2.3199999999999998,0.86,3,2.54,0.95,2,2.54,0.95,2,2.09,0.77,4,2.2799999999999998,0.85,3,2.2799999999999998,0.85,3,2.09,0.77,4,2.2799999999999998,0.85,3,2.2799999999999998,0.85,3]
["120800002712050","12",145,2007,29.560938999999998,-95.691254000000001,"steel girder",2.1800000000000002,1.85,1,2.42,2.06,1,2.67,2.27,1,2.16,1.84,1,2.42,2.06,1,2.67,2.27,1,2.57,2.1800000000000002,1,2.89,2.46,1,3.11,2.64,1,2.57,2.1800000000000002,1,2.89,2.46,1,3.11,2.64,1,2.31,1.96,1,2.6,2.21,1,2.8,2.38,1,2.31,1.96,1,2.6,2.21,1,2.8,2.38,1]
["120800002712189","12",135,1984,29.542415200000001,-95.756732650000004,"prestress concrete girder",1.71,0.72,4,1.92,0.81,3,2.06,0.87,3,1.71,0.72,4,1.92,0.81,3,2.06,0.87,3,2.04,0.86,3,2.2599999999999998,0.95,2,2.42,1.02,1,2.04,0.86,3,2.2599999999999998,0.95,2,2.42,1.02,1,1.83,0.77,4,2.0299999999999998,0.85,3,2.1800000000000002,0.92,2,1.83,0.77,4,2.0299999999999998,0.85,3,2.1800000000000002,0.92,2]
["120800002712309","12",125,2004,29.621317340000001,-95.601503730000005,"prestress concrete special",1.81,0.77,0,2,0.84,0,2.12,0.89,0,1.81,0.77,0,2,0.84,0,2.12,0.89,0,2.16,0.91,0,2.35,0.99,0,2.5,1.05,0,2.16,0.91,0,2.35,0.99,0,2.5,1.05,0,1.95,0.82,0,2.12,0.89,0,2.25,0.94,0,1.95,0.82,0,2.12,0.89,0,2.25,0.94,0]
["120800008909005","12",50,2002,29.526072800000001,-95.871091559999996,"prestress concrete girder",2.36,1.17,1,2.36,1.17,1,2.36,1.17,1,2.36,1.17,1,2.36,1.17,1,2.36,1.17,1,3.2,1.58,1,3.2,1.58,1,3.2,1.58,1,3.2,1.58,1,3.2,1.58,1,3.2,1.58,1,2.86,1.42,1,2.86,1.42,1,2.86,1.42,1,2.86,1.42,1,2.86,1.42,1,2.86,1.42,1]
["120800008909208","12",120,2008,29.44589367,-95.999907899999997,"prestress concrete special",2.33,1.98,0,2.5499999999999998,2.17,0,2.66,2.2599999999999998,0,2.33,1.98,0,2.5499999999999998,2.17,0,2.66,2.2599999999999998,0,2.77,2.35,0,3.01,2.56,0,3.14,2.67,0,2.77,2.35,0,3.01,2.56,0,3.14,2.67,0,2.4900000000000002,2.12,0,2.71,2.2999999999999998,0,2.82,2.4,0,2.4900000000000002,2.12,0,2.71,2.2999999999999998,0,2.82,2.4,0]
["120800008909210","12",120,2010,29.483917989999998,-95.937680709999995,"prestress concrete special",2.33,1.98,0,2.5499999999999998,2.17,0,2.66,2.2599999999999998,0,2.33,1.98,0,2.5499999999999998,2.17,0,2.66,2.2599999999999998,0,2.77,2.35,0,3.01,2.56,0,3.14,2.67,0,2.77,2.35,0,3.01,2.56,0,3.14,2.67,0,2.4900000000000002,2.12,0,2.71,2.2999999999999998,0,2.82,2.4,0,2.4900000000000002,2.12,0,2.71,2.2999999999999998,0,2.82,2.4,0]
["120800008909212","12",120,2008,29.493930809999998,-95.911785089999995,"prestress concrete special",2.33,1.98,0,2.5499999999999998,2.17,0,2.66,2.2599999999999998,0,2.33,1.98,0,2.5499999999999998,2.17,0,2.66,2.2599999999999998,0,2.77,2.35,0,3.01,2.56,0,3.14,2.67,0,2.77,2.35,0,3.01,2.56,0,3.14,2.67,0,2.4900000000000002,2.12,0,2.71,2.2999999999999998,0,2.82,2.4,0,2.4900000000000002,2.12,0,2.71,2.2999999999999998,0,2.82,2.4,0]
["120850050001124","12",50,1965,29.285194180000001,-94.863323500000007,"prestress concrete girder",2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.99,1.06,1,2.99,1.06,1,2.99,1.06,1,2.99,1.06,1,2.99,1.06,1,2.99,1.06,1,2.67,0.94,2,2.67,0.94,2,2.67,0.94,2,2.67,0.94,2,2.67,0.94,2,2.67,0.94,2]
["120850050001132","12",60,1987,29.306997330000002,-94.905960370000003,"steel girder",1.86,0.86,3,1.86,0.86,3,1.86,0.86,3,1.86,0.86,3,1.86,0.86,3,1.86,0.86,3,2.4,1.1100000000000001,1,2.4,1.1100000000000001,1,2.4,1.1100000000000001,1,2.4,1.1100000000000001,1,2.4,1.1100000000000001,1,2.4,1.1100000000000001,1,2.15,1,2,2.15,1,2,2.15,1,2,2.15,1,2,2.15,1,2,2.15,1,2]
["121020002713123","12",60,1975,29.747486469999998,-95.360400900000002,"steel girder",1.27,0.74,4,1.41,0.82,3,1.66,0.96,2,1.27,0.74,4,1.41,0.82,3,1.66,0.96,2,1.61,0.93,2,1.81,1.04,1,2.06,1.19,1,1.61,0.93,2,1.81,1.04,1,2.06,1.19,1,1.44,0.83,3,1.62,0.94,2,1.85,1.07,1,1.44,0.83,3,1.62,0.94,2,1.85,1.07,1]
["121020002713200","12",115,1988,29.661178289999999,-95.557697829999995,"prestress concrete girder",1.93,0.82,3,2.08,0.88,3,2.13,0.89,3,1.93,0.82,3,2.08,0.88,3,2.13,0.89,3,2.27,0.95,2,2.4700000000000002,1.04,1,2.5299999999999998,1.06,1,2.27,0.95,2,2.4700000000000002,1.04,1,2.5299999999999998,1.06,1,2.04,0.86,3,2.23,0.94,2,2.27,0.95,2,2.04,0.86,3,2.23,0.94,2,2.27,0.95,2]
["121020002713233","12",175,1974,29.7434686,-95.361785949999998,"steel girder",1.65,0.95,2,1.78,1.03,1,1.92,1.1100000000000001,1,1.57,0.91,2,1.77,1.02,1,1.79,1.04,1,1.93,1.1200000000000001,1,2.1,1.22,1,2.27,1.31,1,1.9,1.1000000000000001,1,2.0099999999999998,1.1599999999999999,1,2.04,1.18,1,1.73,1,2,1.88,1.0900000000000001,1,2.04,1.18,1,1.71,0.99,2,1.81,1.04,1,1.83,1.06,1]
["121020002713248","12",80,1992,29.680903489999999,-95.536779159999995,"prestress concrete girder",2.19,0.92,2,2.19,0.92,2,2.19,0.92,2,2.2000000000000002,0.93,2,2.2000000000000002,0.93,2,2.2000000000000002,0.93,2,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1]
["121020002713251","12",115,1992,29.68807421,-95.530744960000007,"prestress concrete girder",1.93,0.72,4,2.08,0.77,4,2.13,0.79,4,1.93,0.72,4,2.08,0.77,4,2.13,0.79,4,2.27,0.84,3,2.4700000000000002,0.92,2,2.5299999999999998,0.94,2,2.27,0.84,3,2.4700000000000002,0.92,2,2.5299999999999998,0.94,2,2.04,0.76,4,2.23,0.83,3,2.27,0.84,3,2.04,0.76,4,2.23,0.83,3,2.27,0.84,3]
["121020002713260","12",210,1990,29.662638250000001,-95.55905885,"Multi Span Long",0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1]
["121020002713274","12",130,1992,29.692034060000001,-95.527012830000004,"prestress concrete girder",1.76,0.65,5,1.97,0.74,4,2.1,0.78,4,1.76,0.65,5,1.97,0.74,4,2.1,0.78,4,2.11,0.78,4,2.2999999999999998,0.86,3,2.48,0.92,2,2.11,0.78,4,2.2999999999999998,0.86,3,2.48,0.92,2,1.9,0.71,4,2.0699999999999998,0.77,4,2.23,0.83,3,1.9,0.71,4,2.0699999999999998,0.77,4,2.23,0.83,3]
["121020002713373","12",280,1998,29.658745790000001,-95.555855179999995,"Multi Span Long",0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1]
["121020005006150","12",115,1994,29.96290291,-95.687890940000003,"prestress concrete girder",1.93,0.72,4,2.08,0.77,4,2.13,0.79,4,1.93,0.72,4,2.08,0.77,4,2.13,0.79,4,2.27,0.84,3,2.4700000000000002,0.92,2,2.5299999999999998,0.94,2,2.27,0.84,3,2.4700000000000002,0.92,2,2.5299999999999998,0.94,2,2.04,0.76,4,2.23,0.83,3,2.27,0.84,3,2.04,0.76,4,2.23,0.83,3,2.27,0.84,3]
["121020005006461","12",270,2013,29.995350999999999,-95.768648999999996,"Multi Span Long","Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1]
["121020005009083","12",90,1988,29.867987999999997,-95.543549999999996,"prestress concrete girder",2.16,0.8,4,2.17,0.8,4,2.17,0.8,4,2.16,0.8,4,2.17,0.8,4,2.17,0.8,4,2.63,0.98,2,2.63,0.98,2,2.63,0.98,2,2.63,0.98,2,2.63,0.98,2,2.63,0.98,2,2.36,0.88,3,2.36,0.88,3,2.36,0.88,3,2.36,0.88,3,2.36,0.88,3,2.36,0.88,3]
["121020005009117","12",115,2016,29.876766310000001,-95.563110690000002,"prestress concrete girder",2.38,1.79,1,2.56,1.92,1,2.63,1.97,1,2.38,1.79,1,2.56,1.92,1,2.63,1.97,1,2.8,2.1,1,3.05,2.29,1,3.12,2.34,1,2.8,2.1,1,3.05,2.29,1,3.12,2.34,1,2.52,1.89,1,2.75,2.06,1,2.8,2.1,1,2.52,1.89,1,2.75,2.06,1,2.8,2.1,1]
["121020005009120","12",130,1990,29.87244441,-95.553128430000001,"prestress concrete girder",1.76,0.65,5,1.97,0.74,4,2.1,0.78,4,1.76,0.65,5,1.97,0.74,4,2.1,0.78,4,2.11,0.78,4,2.2999999999999998,0.86,3,2.48,0.92,2,2.11,0.78,4,2.2999999999999998,0.86,3,2.48,0.92,2,1.9,0.71,4,2.0699999999999998,0.77,4,2.23,0.83,3,1.9,0.71,4,2.0699999999999998,0.77,4,2.23,0.83,3]
["121020005009146","12",90,1988,29.871005999999998,-95.549875999999998,"steel weathered girder",1.76,1.02,1,1.77,1.02,1,1.77,1.02,1,1.76,1.02,1,1.77,1.02,1,1.77,1.02,1,2.14,1.24,1,2.14,1.24,1,2.14,1.24,1,2.14,1.24,1,2.14,1.24,1,2.14,1.24,1,1.92,1.1100000000000001,1,1.92,1.1100000000000001,1,1.92,1.1100000000000001,1,1.92,1.1100000000000001,1,1.92,1.1100000000000001,1,1.92,1.1100000000000001,1]
["121020005009177","12",225,2016,29.872387,-95.552253999999991,"Multi Span Long","Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1]
["121020005009488","12",160,2016,29.859396999999998,-95.52377899999999,"steel girder",2.13,1.81,1,2.34,1.99,1,2.58,2.19,1,2.02,1.72,1,2.34,1.99,1,2.58,2.19,1,2.4900000000000002,2.12,1,2.76,2.35,1,3.06,2.6,1,2.4500000000000002,2.08,1,2.76,2.35,1,3.06,2.6,1,2.2400000000000002,1.9,1,2.48,2.11,1,2.75,2.34,1,2.2000000000000002,1.87,1,2.48,2.11,1,2.75,2.34,1]
["121020005009498","12",155,2017,29.823658999999999,-95.472949,"steel girder",2.14,2.14,1,2.36,2.36,1,2.61,2.61,1,2.06,2.06,1,2.36,2.36,1,2.61,2.61,1,2.5099999999999998,2.5099999999999998,1,2.79,2.79,1,3.08,3.08,1,2.5,2.5,1,2.79,2.79,1,3.08,3.08,1,2.2599999999999998,2.2599999999999998,1,2.5099999999999998,2.5099999999999998,1,2.77,2.77,1,2.25,2.25,1,2.5099999999999998,2.5099999999999998,1,2.77,2.77,1]
["121020011005137","12",95,1991,30.105483549999999,-95.435617309999998,"steel weathered girder",1.49,0.98,2,1.44,0.94,2,1.43,0.94,2,1.38,0.9,3,1.44,0.94,2,1.43,0.94,2,1.7,1.1100000000000001,1,1.66,1.0900000000000001,1,1.66,1.0900000000000001,1,1.61,1.05,1,1.66,1.0900000000000001,1,1.66,1.0900000000000001,1,1.53,1,2,1.49,0.98,2,1.49,0.98,2,1.45,0.95,2,1.49,0.98,2,1.49,0.98,2]
["121020011005160","12",80,1998,30.04736553,-95.430463489999994,"prestress concrete girder",2.19,0.92,2,2.19,0.92,2,2.19,0.92,2,2.2000000000000002,0.93,2,2.2000000000000002,0.93,2,2.2000000000000002,0.93,2,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1]
["121020011005180","12",125,2002,30.075168009999999,-95.43636952,"prestress concrete girder",1.81,0.77,4,2,0.84,3,2.12,0.89,3,1.81,0.77,4,2,0.84,3,2.12,0.89,3,2.16,0.91,2,2.35,0.99,2,2.5,1.05,1,2.16,0.91,2,2.35,0.99,2,2.5,1.05,1,1.95,0.82,3,2.12,0.89,3,2.25,0.94,2,1.95,0.82,3,2.12,0.89,3,2.25,0.94,2]
["121020011006114","12",70,1989,29.931807939999999,-95.411261850000002,"prestress concrete girder",2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1]
["121020011006283","12",85,1995,29.940317690000001,-95.413431840000001,"prestress concrete girder",2.1800000000000002,0.65,5,2.1800000000000002,0.65,5,2.1800000000000002,0.65,5,2.1800000000000002,0.65,5,2.1800000000000002,0.65,5,2.1800000000000002,0.65,5,2.66,0.79,4,2.66,0.79,4,2.66,0.79,4,2.66,0.79,4,2.66,0.79,4,2.66,0.79,4,2.39,0.71,4,2.39,0.71,4,2.39,0.71,4,2.39,0.71,4,2.39,0.71,4,2.39,0.71,4]
["121020011006292","12",225,1997,29.949137660000002,-95.417397019999996,"Multi Span Long",0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1]
["121020011006384","12",310,2003,29.9379542,-95.412376510000001,"Multi Span Long",0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1]
["121020017706134","12",85,2000,30.025607279999999,-95.25887195,"prestress concrete girder",2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.66,0.99,2,2.66,0.99,2,2.66,0.99,2,2.66,0.99,2,2.66,0.99,2,2.66,0.99,2,2.39,0.89,3,2.39,0.89,3,2.39,0.89,3,2.39,0.89,3,2.39,0.89,3,2.39,0.89,3]
["121020017706228","12",80,2002,30.020793189999999,-95.260878219999995,"prestress concrete girder",2.19,0.92,2,2.19,0.92,2,2.19,0.92,2,2.2000000000000002,0.93,2,2.2000000000000002,0.93,2,2.2000000000000002,0.93,2,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1]
["121020017706229","12",110,1999,30.034779820000001,-95.256516430000005,"prestress concrete special",1.97,0.59,0,2.12,0.63,0,2.14,0.64,0,1.97,0.59,0,2.12,0.63,0,2.14,0.64,0,2.3199999999999998,0.69,0,2.54,0.76,0,2.54,0.76,0,2.3199999999999998,0.69,0,2.54,0.76,0,2.54,0.76,0,2.09,0.62,0,2.2799999999999998,0.68,0,2.2799999999999998,0.68,0,2.09,0.62,0,2.2799999999999998,0.68,0,2.2799999999999998,0.68,0]
["121020017707185","12",95,1995,29.91844386,-95.306947940000001,"prestress concrete girder",2.1,0.88,3,2.16,0.91,2,2.16,0.91,2,2.1,0.88,3,2.16,0.91,2,2.16,0.91,2,2.5499999999999998,1.07,1,2.6,1.1000000000000001,1,2.6,1.1000000000000001,1,2.5499999999999998,1.07,1,2.6,1.1000000000000001,1,2.6,1.1000000000000001,1,2.2999999999999998,0.97,2,2.34,0.99,2,2.34,0.99,2,2.2999999999999998,0.97,2,2.34,0.99,2,2.34,0.99,2]
["121020017707189","12",155,1998,29.891423369999998,-95.318117779999994,"steel girder",1.65,1.08,1,1.8,1.18,1,1.96,1.28,1,1.63,1.07,1,1.64,1.07,1,1.69,1.1100000000000001,1,1.96,1.28,1,2.15,1.41,1,2.33,1.52,1,1.81,1.18,1,1.86,1.22,1,1.96,1.28,1,1.76,1.1599999999999999,1,1.93,1.27,1,2.1,1.38,1,1.63,1.07,1,1.68,1.1000000000000001,1,1.76,1.1599999999999999,1]
["121020017707209","12",125,1997,29.981727750000001,-95.276860170000006,"prestress concrete special",1.81,0.68,0,2,0.74,0,2.12,0.79,0,1.81,0.68,0,2,0.74,0,2.12,0.79,0,2.16,0.8,0,2.35,0.87,0,2.5,0.93,0,2.16,0.8,0,2.35,0.87,0,2.5,0.93,0,1.95,0.73,0,2.12,0.79,0,2.25,0.83,0,1.95,0.73,0,2.12,0.79,0,2.25,0.83,0]
["121020017707275","12",115,1996,29.9397001,-95.296219199999996,"prestress concrete special",1.93,0.82,0,2.08,0.88,0,2.13,0.89,0,1.93,0.82,0,2.08,0.88,0,2.13,0.89,0,2.27,0.95,0,2.4700000000000002,1.04,0,2.5299999999999998,1.06,0,2.27,0.95,0,2.4700000000000002,1.04,0,2.5299999999999998,1.06,0,2.04,0.86,0,2.23,0.94,0,2.27,0.95,0,2.04,0.86,0,2.23,0.94,0,2.27,0.95,0]
["121020017711173","12",135,1995,29.855152969999999,-95.333755249999996,"prestress concrete special",1.71,0.64,0,1.92,0.71,0,2.06,0.77,0,1.71,0.64,0,1.92,0.71,0,2.06,0.77,0,2.04,0.76,0,2.2599999999999998,0.84,0,2.42,0.9,0,2.04,0.76,0,2.2599999999999998,0.84,0,2.42,0.9,0,1.83,0.68,0,2.0299999999999998,0.75,0,2.1800000000000002,0.81,0,1.83,0.68,0,2.0299999999999998,0.75,0,2.1800000000000002,0.81,0]
["121020017711279","12",130,2002,29.76211906,-95.350321559999998,"prestress concrete special",1.76,0.65,0,1.97,0.74,0,2.1,0.78,0,1.76,0.65,0,1.97,0.74,0,2.1,0.78,0,2.11,0.78,0,2.2999999999999998,0.86,0,2.48,0.92,0,2.11,0.78,0,2.2999999999999998,0.86,0,2.48,0.92,0,1.9,0.71,0,2.0699999999999998,0.77,0,2.23,0.83,0,1.9,0.71,0,2.0699999999999998,0.77,0,2.23,0.83,0]
["121020017711312","12",100,2003,29.769024940000001,-95.341026310000004,"prestress concrete girder",2.0499999999999998,1.01,1,2.15,1.06,1,2.15,1.06,1,2.0499999999999998,1.01,1,2.15,1.06,1,2.15,1.06,1,2.46,1.22,1,2.58,1.28,1,2.58,1.28,1,2.46,1.22,1,2.58,1.28,1,2.58,1.28,1,2.2200000000000002,1.1000000000000001,1,2.3199999999999998,1.1499999999999999,1,2.3199999999999998,1.1499999999999999,1,2.2200000000000002,1.1000000000000001,1,2.3199999999999998,1.1499999999999999,1,2.3199999999999998,1.1499999999999999,1]
["121020027106547","12",125,2005,29.785049149999999,-95.736200359999998,"prestress concrete special",2.29,1.95,0,2.54,2.16,0,2.69,2.29,0,2.2999999999999998,1.95,0,2.54,2.16,0,2.69,2.29,0,2.74,2.33,0,2.98,2.5299999999999998,0,3.17,2.69,0,2.74,2.33,0,2.98,2.5299999999999998,0,3.17,2.69,0,2.4700000000000002,2.1,0,2.68,2.2799999999999998,0,2.85,2.42,0,2.4700000000000002,2.1,0,2.68,2.2799999999999998,0,2.85,2.42,0]
["121020027106550","12",130,2005,29.785413219999999,-95.705715269999999,"prestress concrete special",2.2599999999999998,1.92,0,2.54,2.16,0,2.69,2.29,0,2.2599999999999998,1.92,0,2.54,2.16,0,2.69,2.29,0,2.71,2.2999999999999998,0,2.96,2.52,0,3.19,2.71,0,2.71,2.2999999999999998,0,2.96,2.52,0,3.19,2.71,0,2.44,2.0699999999999998,0,2.66,2.2599999999999998,0,2.87,2.44,0,2.44,2.0699999999999998,0,2.66,2.2599999999999998,0,2.87,2.44,0]
["121020027106554","12",125,2005,29.785259790000001,-95.66614903,"prestress concrete special",2.29,1.95,0,2.54,2.16,0,2.69,2.29,0,2.2999999999999998,1.95,0,2.54,2.16,0,2.69,2.29,0,2.74,2.33,0,2.98,2.5299999999999998,0,3.17,2.69,0,2.74,2.33,0,2.98,2.5299999999999998,0,3.17,2.69,0,2.4700000000000002,2.1,0,2.68,2.2799999999999998,0,2.85,2.42,0,2.4700000000000002,2.1,0,2.68,2.2799999999999998,0,2.85,2.42,0]
["121020027106555","12",125,2005,29.784628229999999,-95.667097600000005,"prestress concrete special",2.29,1.95,0,2.54,2.16,0,2.69,2.29,0,2.2999999999999998,1.95,0,2.54,2.16,0,2.69,2.29,0,2.74,2.33,0,2.98,2.5299999999999998,0,3.17,2.69,0,2.74,2.33,0,2.98,2.5299999999999998,0,3.17,2.69,0,2.4700000000000002,2.1,0,2.68,2.2799999999999998,0,2.85,2.42,0,2.4700000000000002,2.1,0,2.68,2.2799999999999998,0,2.85,2.42,0]
["121020027106690","12",290,2014,29.784997999999998,-95.779969999999992,"Multi Span Long","Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1]
["121020027107306","12",85,1967,29.7773848,-95.41805128,"concrete bridge",1.69,0.5,5,1.66,0.49,5,1.69,0.5,5,1.65,0.49,5,1.66,0.49,5,1.69,0.5,5,1.95,0.57999999999999996,5,1.95,0.57999999999999996,5,2.0099999999999998,0.59,5,1.95,0.57999999999999996,5,1.95,0.57999999999999996,5,2.0099999999999998,0.59,5,1.75,0.52,5,1.75,0.52,5,1.8,0.53,5,1.75,0.52,5,1.75,0.52,5,1.8,0.53,5]
["121020027107310","12",75,2011,29.77650774,-95.398935750000007,"prestress concrete girder",2.4300000000000002,1.82,1,2.4300000000000002,1.82,1,2.4300000000000002,1.82,1,2.4300000000000002,1.82,1,2.4300000000000002,1.82,1,2.4300000000000002,1.82,1,3.01,2.2599999999999998,1,3.01,2.2599999999999998,1,3.01,2.2599999999999998,1,3.01,2.2599999999999998,1,3.01,2.2599999999999998,1,3.01,2.2599999999999998,1,2.7,2.0299999999999998,1,2.7,2.0299999999999998,1,2.7,2.0299999999999998,1,2.7,2.0299999999999998,1,2.7,2.0299999999999998,1,2.7,2.0299999999999998,1]
["121020027107357","12",95,1972,29.76821284,-95.363213819999999,"prestress concrete girder",2.33,0.94,2,2.39,0.95,2,2.39,0.95,2,2.33,0.94,2,2.39,0.95,2,2.39,0.95,2,2.83,1.1299999999999999,1,2.88,1.1499999999999999,1,2.88,1.1499999999999999,1,2.83,1.1299999999999999,1,2.88,1.1499999999999999,1,2.88,1.1499999999999999,1,2.5499999999999998,1.02,1,2.59,1.04,1,2.59,1.04,1,2.5499999999999998,1.02,1,2.59,1.04,1,2.59,1.04,1]
["121020027107392","12",110,1961,29.774198670000001,-95.366361859999998,"steel girder",1.71,0.79,4,1.62,0.75,4,1.57,0.73,4,1.37,0.63,5,1.5,0.7,5,1.56,0.72,4,1.91,0.88,3,1.82,0.84,3,1.78,0.82,3,1.59,0.73,4,1.74,0.8,4,1.78,0.82,3,1.72,0.79,4,1.64,0.76,4,1.6,0.74,4,1.43,0.66,5,1.57,0.73,4,1.6,0.74,4]
["121020027107576","12",235,2006,29.780417379999999,-95.453524979999997,"Multi Span Long","Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1]
["121020027107594","12",260,2007,29.785064999999999,-95.560083999999989,"Multi Span Long","Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1]
["121020027107598","12",75,2007,29.784904999999998,-95.562359000000001,"prestress concrete girder",2.4300000000000002,1.82,1,2.4300000000000002,1.82,1,2.4300000000000002,1.82,1,2.4300000000000002,1.82,1,2.4300000000000002,1.82,1,2.4300000000000002,1.82,1,3.01,2.2599999999999998,1,3.01,2.2599999999999998,1,3.01,2.2599999999999998,1,3.01,2.2599999999999998,1,3.01,2.2599999999999998,1,3.01,2.2599999999999998,1,2.7,2.0299999999999998,1,2.7,2.0299999999999998,1,2.7,2.0299999999999998,1,2.7,2.0299999999999998,1,2.7,2.0299999999999998,1,2.7,2.0299999999999998,1]
["121020027107601","12",185,2007,29.787395,-95.563604999999995,"Multi Span Long","Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1]
["121020027107617","12",130,2007,29.784917,-95.531365999999991,"prestress concrete special",2.2599999999999998,1.92,0,2.54,2.16,0,2.69,2.29,0,2.2599999999999998,1.92,0,2.54,2.16,0,2.69,2.29,0,2.71,2.2999999999999998,0,2.96,2.52,0,3.19,2.71,0,2.71,2.2999999999999998,0,2.96,2.52,0,3.19,2.71,0,2.44,2.0699999999999998,0,2.66,2.2599999999999998,0,2.87,2.44,0,2.44,2.0699999999999998,0,2.66,2.2599999999999998,0,2.87,2.44,0]
["121020027107619","12",125,2007,29.784730999999997,-95.520829999999989,"prestress concrete special",2.29,1.95,0,2.54,2.16,0,2.69,2.29,0,2.2999999999999998,1.95,0,2.54,2.16,0,2.69,2.29,0,2.74,2.33,0,2.98,2.5299999999999998,0,3.17,2.69,0,2.74,2.33,0,2.98,2.5299999999999998,0,3.17,2.69,0,2.4700000000000002,2.1,0,2.68,2.2799999999999998,0,2.85,2.42,0,2.4700000000000002,2.1,0,2.68,2.2799999999999998,0,2.85,2.42,0]
["121020027114387","12",75,1972,29.809102450000001,-95.339996819999996,"prestress concrete girder",2.2599999999999998,0.9,3,2.2599999999999998,0.9,3,2.2599999999999998,0.9,3,2.2599999999999998,0.9,3,2.2599999999999998,0.9,3,2.2599999999999998,0.9,3,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.5099999999999998,1,2,2.5099999999999998,1,2,2.5099999999999998,1,2,2.5099999999999998,1,2,2.5099999999999998,1,2,2.5099999999999998,1,2]
["121020027114404","12",150,1979,29.808597460000001,-95.339480809999998,"steel weathered girder",1.65,0.95,2,1.81,1.04,1,1.97,1.1399999999999999,1,1.6,0.92,2,1.61,0.93,2,1.67,0.97,2,1.97,1.1399999999999999,1,2.16,1.24,1,2.34,1.35,1,1.77,1.02,1,1.83,1.06,1,1.95,1.1299999999999999,1,1.77,1.02,1,1.94,1.1200000000000001,1,2.1,1.22,1,1.59,0.92,2,1.65,0.95,2,1.75,1.01,1]
["121020027114667","12",110,2013,29.813333329999999,-95.429166660000007,"prestress concrete special",2.4,2.04,0,2.58,2.19,0,2.6,2.21,0,2.4,2.04,0,2.58,2.19,0,2.6,2.21,0,2.83,2.41,0,3.09,2.63,0,3.09,2.63,0,2.83,2.41,0,3.09,2.63,0,3.09,2.63,0,2.54,2.16,0,2.78,2.36,0,2.78,2.36,0,2.54,2.16,0,2.78,2.36,0,2.78,2.36,0]
["121020027114669","12",130,2014,29.792200000000001,-95.452200000000005,"prestress concrete special",2.2599999999999998,1.92,0,2.54,2.16,0,2.69,2.29,0,2.2599999999999998,1.92,0,2.54,2.16,0,2.69,2.29,0,2.71,2.2999999999999998,0,2.96,2.52,0,3.19,2.71,0,2.71,2.2999999999999998,0,2.96,2.52,0,3.19,2.71,0,2.44,2.0699999999999998,0,2.66,2.2599999999999998,0,2.87,2.44,0,2.44,2.0699999999999998,0,2.66,2.2599999999999998,0,2.87,2.44,0]
["121020027115437","12",170,1965,29.709495090000001,-95.265906290000004,"steel girder",1.64,0.95,2,1.78,1.03,1,1.93,1.1200000000000001,1,1.59,0.92,2,1.75,1.01,1,1.76,1.02,1,1.93,1.1200000000000001,1,2.1,1.22,1,2.29,1.32,1,1.91,1.1000000000000001,1,1.98,1.1399999999999999,1,2.0099999999999998,1.1599999999999999,1,1.73,1,2,1.89,1.1000000000000001,1,2.0499999999999998,1.19,1,1.72,0.99,2,1.78,1.03,1,1.81,1.04,1]
["121020027115705","12",120,1973,29.727505999999998,-95.266607999999991,"prestress concrete girder",2.2799999999999998,0.8,4,2.4900000000000002,0.88,3,2.6,0.92,2,2.2799999999999998,0.8,4,2.4900000000000002,0.88,3,2.6,0.92,2,2.71,0.95,2,2.94,1.04,1,3.07,1.08,1,2.71,0.95,2,2.94,1.04,1,3.07,1.08,1,2.44,0.86,3,2.65,0.94,2,2.76,0.98,2,2.44,0.86,3,2.65,0.94,2,2.76,0.98,2]
["121020027116238","12",50,1966,29.680809480000001,-95.366890269999999,"prestress concrete girder",2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.99,1.06,1,2.99,1.06,1,2.99,1.06,1,2.99,1.06,1,2.99,1.06,1,2.99,1.06,1,2.67,0.94,2,2.67,0.94,2,2.67,0.94,2,2.67,0.94,2,2.67,0.94,2,2.67,0.94,2]
["121020027116248","12",60,1968,29.688829040000002,-95.331986229999998,"concrete bridge",1.55,0.57999999999999996,5,1.73,0.65,5,2.04,0.76,4,1.55,0.57999999999999996,5,1.73,0.65,5,2.04,0.76,4,1.98,0.74,4,2.2200000000000002,0.83,3,2.5299999999999998,0.94,2,1.98,0.74,4,2.2200000000000002,0.83,3,2.5299999999999998,0.94,2,1.77,0.66,5,1.99,0.74,4,2.27,0.84,3,1.77,0.66,5,1.99,0.74,4,2.27,0.84,3]
["121020027116250","12",60,1968,29.683091310000002,-95.349019740000003,"concrete bridge",1.55,0.57999999999999996,5,1.73,0.65,5,2.04,0.76,4,1.55,0.57999999999999996,5,1.73,0.65,5,2.04,0.76,4,1.98,0.74,4,2.2200000000000002,0.83,3,2.5299999999999998,0.94,2,1.98,0.74,4,2.2200000000000002,0.83,3,2.5299999999999998,0.94,2,1.77,0.66,5,1.99,0.74,4,2.27,0.84,3,1.77,0.66,5,1.99,0.74,4,2.27,0.84,3]
["121020027116251","12",60,1968,29.680553570000001,-95.381337689999995,"concrete bridge",1.55,0.57999999999999996,5,1.73,0.65,5,2.04,0.76,4,1.55,0.57999999999999996,5,1.73,0.65,5,2.04,0.76,4,1.98,0.74,4,2.2200000000000002,0.83,3,2.5299999999999998,0.94,2,1.98,0.74,4,2.2200000000000002,0.83,3,2.5299999999999998,0.94,2,1.77,0.66,5,1.99,0.74,4,2.27,0.84,3,1.77,0.66,5,1.99,0.74,4,2.27,0.84,3]
["121020027116375","12",80,1971,29.680590030000001,-95.458962959999994,"prestress concrete girder",2.29,0.65,5,2.29,0.65,5,2.29,0.65,5,2.29,0.65,5,2.29,0.65,5,2.29,0.65,5,2.81,0.79,4,2.81,0.79,4,2.81,0.79,4,2.81,0.79,4,2.81,0.79,4,2.81,0.79,4,2.52,0.71,4,2.52,0.71,4,2.52,0.71,4,2.52,0.71,4,2.52,0.71,4,2.52,0.71,4]
["121020027116481","12",85,1970,29.695696659999999,-95.298161239999999,"prestress concrete girder",1.69,0.71,4,1.66,0.7,5,1.69,0.71,4,1.65,0.7,5,1.66,0.7,5,1.69,0.71,4,1.95,0.82,3,1.95,0.82,3,2.0099999999999998,0.84,3,1.95,0.82,3,1.95,0.82,3,2.0099999999999998,0.84,3,1.75,0.74,4,1.75,0.74,4,1.8,0.76,4,1.75,0.74,4,1.75,0.74,4,1.8,0.76,4]
["121020027116483","12",65,1966,29.693485849999998,-95.322417939999994,"prestress concrete girder",2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3]
["121020027116493","12",60,1968,29.68896904,-95.332119230000004,"concrete bridge",1.55,0.57999999999999996,5,1.73,0.65,5,2.04,0.76,4,1.55,0.57999999999999996,5,1.73,0.65,5,2.04,0.76,4,1.98,0.74,4,2.2200000000000002,0.83,3,2.5299999999999998,0.94,2,1.98,0.74,4,2.2200000000000002,0.83,3,2.5299999999999998,0.94,2,1.77,0.66,5,1.99,0.74,4,2.27,0.84,3,1.77,0.66,5,1.99,0.74,4,2.27,0.84,3]
["121020027116641","12",125,1980,29.6802472,-95.380443679999999,"steel weathered girder",1.72,0.99,2,1.84,1.07,1,1.75,1.01,1,1.42,0.82,3,1.53,0.89,3,1.63,0.95,2,2.0699999999999998,1.19,1,2.04,1.18,1,1.96,1.1299999999999999,1,1.61,0.93,2,1.77,1.02,1,1.88,1.0900000000000001,1,1.86,1.07,1,1.83,1.06,1,1.76,1.02,1,1.45,0.84,3,1.6,0.92,2,1.69,0.98,2]
["121020027117103","12",130,2004,29.731086439999999,-95.460313760000005,"steel girder",1.83,1.37,1,2.0099999999999998,1.51,1,2.09,1.57,1,1.67,1.25,1,1.77,1.33,1,1.9,1.42,1,2.2000000000000002,1.65,1,2.4,1.8,1,2.33,1.75,1,1.88,1.41,1,2.0299999999999998,1.52,1,2.19,1.64,1,1.98,1.48,1,2.16,1.62,1,2.1,1.58,1,1.69,1.27,1,1.83,1.37,1,1.97,1.48,1]
["121020027117321","12",60,2001,29.698590459999998,-95.459254880000003,"concrete bridge",1.55,0.57999999999999996,5,1.73,0.65,5,2.04,0.76,4,1.55,0.57999999999999996,5,1.73,0.65,5,2.04,0.76,4,1.98,0.74,4,2.2200000000000002,0.83,3,2.5299999999999998,0.94,2,1.98,0.74,4,2.2200000000000002,0.83,3,2.5299999999999998,0.94,2,1.77,0.66,5,1.99,0.74,4,2.27,0.84,3,1.77,0.66,5,1.99,0.74,4,2.27,0.84,3]
["121020027117513","12",130,2002,29.712056260000001,-95.459903370000006,"prestress concrete special",1.76,0.74,0,1.97,0.83,0,2.1,0.88,0,1.76,0.74,0,1.97,0.83,0,2.1,0.88,0,2.11,0.88,0,2.2999999999999998,0.97,0,2.48,1.05,0,2.11,0.88,0,2.2999999999999998,0.97,0,2.48,1.05,0,1.9,0.8,0,2.0699999999999998,0.87,0,2.23,0.94,0,1.9,0.8,0,2.0699999999999998,0.87,0,2.23,0.94,0]
["121020027117515","12",115,2002,29.72828926,-95.461466439999995,"prestress concrete girder",1.93,0.82,3,2.08,0.88,3,2.13,0.89,3,1.93,0.82,3,2.08,0.88,3,2.13,0.89,3,2.27,0.95,2,2.4700000000000002,1.04,1,2.5299999999999998,1.06,1,2.27,0.95,2,2.4700000000000002,1.04,1,2.5299999999999998,1.06,1,2.04,0.86,3,2.23,0.94,2,2.27,0.95,2,2.04,0.86,3,2.23,0.94,2,2.27,0.95,2]
["121020027117519","12",45,2002,29.729126319999999,-95.45927949,"prestress concrete girder",2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.4300000000000002,1.02,1,2.42,1.02,1,2.42,1.02,1,3.23,1.36,1,3.23,1.36,1,3.23,1.36,1,3.23,1.36,1,3.23,1.36,1,3.23,1.36,1,2.92,1.23,1,2.92,1.23,1,2.92,1.23,1,2.92,1.23,1,2.92,1.23,1,2.92,1.23,1]
["121020027117523","12",100,2002,29.73033358,-95.459142009999994,"prestress concrete girder",2.0499999999999998,0.86,3,2.15,0.9,3,2.15,0.9,3,2.0499999999999998,0.86,3,2.15,0.9,3,2.15,0.9,3,2.46,1.04,1,2.58,1.0900000000000001,1,2.58,1.0900000000000001,1,2.46,1.04,1,2.58,1.0900000000000001,1,2.58,1.0900000000000001,1,2.2200000000000002,0.94,2,2.3199999999999998,0.98,2,2.3199999999999998,0.98,2,2.2200000000000002,0.94,2,2.3199999999999998,0.98,2,2.3199999999999998,0.98,2]
["121020027117524","12",130,2002,29.728078289999999,-95.459260979999996,"prestress concrete girder",1.76,0.74,4,1.97,0.83,3,2.1,0.88,3,1.76,0.74,4,1.97,0.83,3,2.1,0.88,3,2.11,0.88,3,2.2999999999999998,0.97,2,2.48,1.05,1,2.11,0.88,3,2.2999999999999998,0.97,2,2.48,1.05,1,1.9,0.8,4,2.0699999999999998,0.87,3,2.23,0.94,2,1.9,0.8,4,2.0699999999999998,0.87,3,2.23,0.94,2]
["121020027117562","12",145,2006,29.75412901,-95.455627789999994,"steel girder",2.1800000000000002,2.1800000000000002,1,2.42,2.42,1,2.67,2.67,1,2.16,2.16,1,2.42,2.42,1,2.67,2.67,1,2.57,2.57,1,2.89,2.89,1,3.11,3.11,1,2.57,2.57,1,2.89,2.89,1,3.11,3.11,1,2.31,2.31,1,2.6,2.6,1,2.8,2.8,1,2.31,2.31,1,2.6,2.6,1,2.8,2.8,1]
["121020050003006","12",85,1985,29.72255805,-95.328069040000003,"steel girder",1.38,0.8,4,1.35,0.78,4,1.38,0.8,4,1.35,0.78,4,1.35,0.78,4,1.38,0.8,4,1.59,0.92,2,1.59,0.92,2,1.64,0.95,2,1.59,0.92,2,1.59,0.92,2,1.64,0.95,2,1.43,0.83,3,1.42,0.82,3,1.47,0.85,3,1.42,0.82,3,1.42,0.82,3,1.47,0.85,3]
["121020050003012","12",60,1981,29.69968751,-95.292288060000004,"steel girder",1.27,0.74,4,1.41,0.82,3,1.66,0.96,2,1.27,0.74,4,1.41,0.82,3,1.66,0.96,2,1.61,0.93,2,1.81,1.04,1,2.06,1.19,1,1.61,0.93,2,1.81,1.04,1,2.06,1.19,1,1.44,0.83,3,1.62,0.94,2,1.85,1.07,1,1.44,0.83,3,1.62,0.94,2,1.85,1.07,1]
["121020050003096","12",90,1959,29.779316510000001,-95.36781585,"steel girder",1.43,0.66,5,1.39,0.64,5,1.4,0.65,5,1.36,0.63,5,1.39,0.64,5,1.4,0.65,5,1.64,0.76,4,1.62,0.75,4,1.64,0.76,4,1.61,0.74,4,1.62,0.75,4,1.64,0.76,4,1.47,0.68,5,1.45,0.67,5,1.47,0.68,5,1.45,0.67,5,1.45,0.67,5,1.47,0.68,5]
["121020050003109","12",75,1963,29.757132240000001,-95.374366219999999,"steel girder",2.1800000000000002,1.1499999999999999,1,2.1800000000000002,1.1499999999999999,1,2.1800000000000002,1.1499999999999999,1,2.1800000000000002,1.1499999999999999,1,2.1800000000000002,1.1499999999999999,1,2.1800000000000002,1.1499999999999999,1,2.7,1.43,1,2.7,1.43,1,2.7,1.43,1,2.7,1.43,1,2.7,1.43,1,2.7,1.43,1,2.42,1.28,1,2.42,1.28,1,2.42,1.28,1,2.42,1.28,1,2.42,1.28,1,2.42,1.28,1]
["121020050003143","12",55,1971,29.569606620000002,-95.169000460000007,"prestress concrete girder",2.19,0.77,4,2.19,0.77,4,2.19,0.77,4,2.19,0.77,4,2.19,0.77,4,2.19,0.77,4,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.59,0.92,2,2.59,0.92,2,2.59,0.92,2,2.59,0.92,2,2.59,0.92,2,2.59,0.92,2]
["121020050003159","12",320,2009,29.522632829999999,-95.12595159,"Multi Span Long","Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1]
["121020050003161","12",110,2008,29.528625080000001,-95.130754710000005,"prestress concrete special",2.4,2.04,0,2.58,2.19,0,2.6,2.21,0,2.4,2.04,0,2.58,2.19,0,2.6,2.21,0,2.83,2.41,0,3.09,2.63,0,3.09,2.63,0,2.83,2.41,0,3.09,2.63,0,3.09,2.63,0,2.54,2.16,0,2.78,2.36,0,2.78,2.36,0,2.54,2.16,0,2.78,2.36,0,2.78,2.36,0]
["121020050003265","12",105,1977,29.697668530000001,-95.28506385,"steel girder",1.64,0.95,2,1.75,1.01,1,1.75,1.01,1,1.64,0.95,2,1.75,1.01,1,1.75,1.01,1,1.95,1.1299999999999999,1,2.09,1.21,1,2.09,1.21,1,1.95,1.1299999999999999,1,2.09,1.21,1,2.09,1.21,1,1.75,1.01,1,1.87,1.08,1,1.87,1.08,1,1.75,1.01,1,1.87,1.08,1,1.87,1.08,1]
["121020050003269","12",75,1985,29.725774980000001,-95.333137179999994,"steel girder",1.29,0.74,4,1.31,0.76,4,1.38,0.8,4,1.29,0.74,4,1.31,0.76,4,1.38,0.8,4,1.53,0.89,3,1.58,0.92,2,1.7,0.98,2,1.53,0.89,3,1.58,0.92,2,1.7,0.98,2,1.37,0.79,4,1.41,0.82,3,1.52,0.88,3,1.37,0.79,4,1.41,0.82,3,1.52,0.88,3]
["121020050003295","12",120,1992,29.680418939999999,-95.272509510000006,"prestress concrete girder",1.87,0.7,5,2.04,0.76,4,2.13,0.79,4,1.87,0.7,5,2.04,0.76,4,2.13,0.79,4,2.2200000000000002,0.83,3,2.41,0.89,3,2.5099999999999998,0.93,2,2.2200000000000002,0.83,3,2.41,0.89,3,2.5099999999999998,0.93,2,1.99,0.74,4,2.17,0.8,4,2.2599999999999998,0.84,3,1.99,0.74,4,2.17,0.8,4,2.2599999999999998,0.84,3]
["121020050003312","12",110,1998,29.610903830000002,-95.210704309999997,"steel weathered girder",1.71,0.99,2,1.62,0.94,2,1.57,0.91,2,1.37,0.79,4,1.5,0.87,3,1.56,0.9,3,1.91,1.1000000000000001,1,1.82,1.05,1,1.78,1.03,1,1.59,0.92,2,1.74,1.01,1,1.78,1.03,1,1.72,0.99,2,1.64,0.95,2,1.6,0.92,2,1.43,0.83,3,1.57,0.91,2,1.6,0.92,2]
["121020050003338","12",50,1971,29.508120980000001,-95.116989779999997,"steel girder",2.06,1.36,1,2.06,1.36,1,2.06,1.36,1,2.06,1.36,1,2.06,1.36,1,2.06,1.36,1,2.79,1.85,1,2.79,1.85,1,2.79,1.85,1,2.79,1.85,1,2.79,1.85,1,2.79,1.85,1,2.5,1.65,1,2.5,1.65,1,2.5,1.65,1,2.5,1.65,1,2.5,1.65,1,2.5,1.65,1]
["121020050003340","12",110,1989,29.616138159999998,-95.215975880000002,"prestress concrete girder",1.97,0.83,3,2.12,0.89,3,2.14,0.9,3,1.97,0.83,3,2.12,0.89,3,2.14,0.9,3,2.3199999999999998,0.98,2,2.54,1.07,1,2.54,1.07,1,2.3199999999999998,0.98,2,2.54,1.07,1,2.54,1.07,1,2.09,0.88,3,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.09,0.88,3,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2]
["121020050003365","12",120,1997,29.60770621,-95.204170899999994,"prestress concrete girder",1.87,0.79,4,2.04,0.86,3,2.13,0.89,3,1.87,0.79,4,2.04,0.86,3,2.13,0.89,3,2.2200000000000002,0.94,2,2.41,1.01,1,2.5099999999999998,1.05,1,2.2200000000000002,0.94,2,2.41,1.01,1,2.5099999999999998,1.05,1,1.99,0.84,3,2.17,0.91,2,2.2599999999999998,0.95,2,1.99,0.84,3,2.17,0.91,2,2.2599999999999998,0.95,2]
["121020050003427","12",120,2010,29.52827778,-95.130527779999994,"prestress concrete special",2.33,1.98,0,2.5499999999999998,2.17,0,2.66,2.2599999999999998,0,2.33,1.98,0,2.5499999999999998,2.17,0,2.66,2.2599999999999998,0,2.77,2.35,0,3.01,2.56,0,3.14,2.67,0,2.77,2.35,0,3.01,2.56,0,3.14,2.67,0,2.4900000000000002,2.12,0,2.71,2.2999999999999998,0,2.82,2.4,0,2.4900000000000002,2.12,0,2.71,2.2999999999999998,0,2.82,2.4,0]
["121020050003429","12",65,1980,29.79836547,-95.371954489999993,"prestress concrete girder",2.25,0.67,5,2.25,0.67,5,2.25,0.67,5,2.25,0.67,5,2.25,0.67,5,2.25,0.67,5,2.86,0.85,3,2.86,0.85,3,2.86,0.85,3,2.86,0.85,3,2.86,0.85,3,2.86,0.85,3,2.56,0.76,4,2.56,0.76,4,2.56,0.76,4,2.56,0.76,4,2.56,0.76,4,2.56,0.76,4]
["121020050801218","12",90,1971,29.769670699999999,-95.34333925,"prestress concrete special",1.76,0.52,0,1.71,0.51,0,1.72,0.51,0,1.67,0.5,0,1.71,0.51,0,1.72,0.51,0,2.0099999999999998,0.59,0,1.98,0.59,0,2.0099999999999998,0.59,0,1.97,0.59,0,1.98,0.59,0,2.0099999999999998,0.59,0,1.81,0.54,0,1.78,0.53,0,1.81,0.54,0,1.78,0.53,0,1.78,0.53,0,1.81,0.54,0]
["121020050801258","12",90,1994,29.774809749999999,-95.138495590000005,"prestress concrete girder",2.16,0.8,4,2.17,0.8,4,2.17,0.8,4,2.16,0.8,4,2.17,0.8,4,2.17,0.8,4,2.63,0.98,2,2.63,0.98,2,2.63,0.98,2,2.63,0.98,2,2.63,0.98,2,2.63,0.98,2,2.36,0.88,3,2.36,0.88,3,2.36,0.88,3,2.36,0.88,3,2.36,0.88,3,2.36,0.88,3]
["121020050801261","12",70,1982,29.791086010000001,-95.083914019999995,"prestress concrete girder",2.23,0.83,3,2.23,0.83,3,2.23,0.83,3,2.23,0.83,3,2.23,0.83,3,2.23,0.83,3,2.79,1.04,1,2.79,1.04,1,2.79,1.04,1,2.79,1.04,1,2.79,1.04,1,2.79,1.04,1,2.5,0.93,2,2.5,0.93,2,2.5,0.93,2,2.5,0.93,2,2.5,0.93,2,2.5,0.93,2]
["121020050801267","12",65,1985,29.770628129999999,-95.213712650000005,"prestress concrete girder",2.25,0.94,2,2.25,0.94,2,2.25,0.94,2,2.25,0.94,2,2.25,0.94,2,2.25,0.94,2,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.56,1.08,1,2.56,1.08,1,2.56,1.08,1,2.56,1.08,1,2.56,1.08,1,2.56,1.08,1]
["121020050801272","12",85,1994,29.771278909999999,-95.153220009999998,"prestress concrete girder",2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.66,0.99,2,2.66,0.99,2,2.66,0.99,2,2.66,0.99,2,2.66,0.99,2,2.66,0.99,2,2.39,0.89,3,2.39,0.89,3,2.39,0.89,3,2.39,0.89,3,2.39,0.89,3,2.39,0.89,3]
["121020050801273","12",85,1994,29.771450909999999,-95.153313010000005,"prestress concrete girder",2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.66,0.99,2,2.66,0.99,2,2.66,0.99,2,2.66,0.99,2,2.66,0.99,2,2.66,0.99,2,2.39,0.89,3,2.39,0.89,3,2.39,0.89,3,2.39,0.89,3,2.39,0.89,3,2.39,0.89,3]
["121020050801315","12",50,1964,29.774346359999999,-95.301218030000001,"concrete bridge",1.75,0.65,5,2.04,0.76,4,2.37,0.88,3,1.75,0.65,5,2.04,0.76,4,2.37,0.88,3,2.2200000000000002,0.83,3,2.5299999999999998,0.94,2,2.77,1.03,1,2.2200000000000002,0.83,3,2.5299999999999998,0.94,2,2.77,1.03,1,1.99,0.74,4,2.2799999999999998,0.85,3,2.5,0.93,2,1.99,0.74,4,2.2799999999999998,0.85,3,2.5,0.93,2]
["121020050801445","12",210,1994,29.770724940000001,-95.156072089999995,"Multi Span Long",0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1]
["121020050801450","12",225,1994,29.76858799,-95.150569959999999,"Multi Span Long",0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1]
["121020050801451","12",200,1994,29.77079282,-95.15013184,"Multi Span Long",0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1]
["121020050801453","12",130,1994,29.77102592,-95.153361020000006,"prestress concrete girder",1.76,0.65,5,1.97,0.74,4,2.1,0.78,4,1.76,0.65,5,1.97,0.74,4,2.1,0.78,4,2.11,0.78,4,2.2999999999999998,0.86,3,2.48,0.92,2,2.11,0.78,4,2.2999999999999998,0.86,3,2.48,0.92,2,1.9,0.71,4,2.0699999999999998,0.77,4,2.23,0.83,3,1.9,0.71,4,2.0699999999999998,0.77,4,2.23,0.83,3]
["121020050801457","12",130,1979,29.771518019999998,-95.196374809999995,"prestress concrete girder",1.76,0.65,5,1.97,0.74,4,2.1,0.78,4,1.76,0.65,5,1.97,0.74,4,2.1,0.78,4,2.11,0.78,4,2.2999999999999998,0.86,3,2.48,0.92,2,2.11,0.78,4,2.2999999999999998,0.86,3,2.48,0.92,2,1.9,0.71,4,2.0699999999999998,0.77,4,2.23,0.83,3,1.9,0.71,4,2.0699999999999998,0.77,4,2.23,0.83,3]
["121020050801462","12",50,1983,29.77141808,-95.206291440000001,"prestress concrete girder",2.36,0.7,5,2.36,0.7,5,2.36,0.7,5,2.36,0.7,5,2.36,0.7,5,2.36,0.7,5,3.2,0.95,2,3.2,0.95,2,3.2,0.95,2,3.2,0.95,2,3.2,0.95,2,3.2,0.95,2,2.86,0.85,3,2.86,0.85,3,2.86,0.85,3,2.86,0.85,3,2.86,0.85,3,2.86,0.85,3]
["121020050801464","12",50,1985,29.773249109999998,-95.232956139999999,"prestress concrete girder",2.36,0.88,3,2.36,0.88,3,2.36,0.88,3,2.36,0.88,3,2.36,0.88,3,2.36,0.88,3,3.2,1.19,1,3.2,1.19,1,3.2,1.19,1,3.2,1.19,1,3.2,1.19,1,3.2,1.19,1,2.86,1.07,1,2.86,1.07,1,2.86,1.07,1,2.86,1.07,1,2.86,1.07,1,2.86,1.07,1]
["121020050801469","12",240,1994,29.768089010000001,-95.150382960000002,"Multi Span Long",0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1]
["121020059801065","12",65,1979,29.73067803,-95.372597290000002,"prestress concrete special",1.53,0.56999999999999995,0,1.64,0.61,0,1.86,0.69,0,1.53,0.56999999999999995,0,1.64,0.61,0,1.86,0.69,0,1.9,0.71,0,2.0699999999999998,0.77,0,2.37,0.88,0,1.9,0.71,0,2.0699999999999998,0.77,0,2.37,0.88,0,1.7,0.63,0,1.85,0.69,0,2.12,0.79,0,1.7,0.63,0,1.85,0.69,0,2.13,0.79,0]
["121700011004133","12",130,1991,30.12678386,-95.443283570000006,"prestress concrete girder",1.76,0.65,5,1.97,0.74,4,2.1,0.78,4,1.76,0.65,5,1.97,0.74,4,2.1,0.78,4,2.11,0.78,4,2.2999999999999998,0.86,3,2.48,0.92,2,2.11,0.78,4,2.2999999999999998,0.86,3,2.48,0.92,2,1.9,0.71,4,2.0699999999999998,0.77,4,2.23,0.83,3,1.9,0.71,4,2.0699999999999998,0.77,4,2.23,0.83,3]
["121700017705314","12",105,2007,30.173577850000001,-95.203446200000002,"prestress concrete girder",2.41,1.81,1,2.57,1.93,1,2.57,1.93,1,2.41,1.81,1,2.57,1.93,1,2.57,1.93,1,2.87,2.15,1,3.07,2.2999999999999998,1,3.07,2.2999999999999998,1,2.87,2.15,1,3.07,2.2999999999999998,1,3.07,2.2999999999999998,1,2.58,1.94,1,2.76,2.0699999999999998,1,2.76,2.0699999999999998,1,2.58,1.94,1,2.76,2.0699999999999998,1,2.76,2.0699999999999998,1]
["121700017705527","12",150,2007,30.069317999999999,-95.246811999999991,"steel girder",2.16,1.84,1,2.39,2.0299999999999998,1,2.65,2.25,1,2.11,1.79,1,2.39,2.0299999999999998,1,2.65,2.25,1,2.54,2.16,1,2.84,2.41,1,3.09,2.63,1,2.54,2.16,1,2.84,2.41,1,3.09,2.63,1,2.2799999999999998,1.94,1,2.5499999999999998,2.17,1,2.78,2.36,1,2.2799999999999998,1.94,1,2.5499999999999998,2.17,1,2.78,2.36,1]
["121700017705528","12",150,2007,30.052097999999997,-95.251795999999999,"steel girder",2.16,1.84,1,2.39,2.0299999999999998,1,2.65,2.25,1,2.11,1.79,1,2.39,2.0299999999999998,1,2.65,2.25,1,2.54,2.16,1,2.84,2.41,1,3.09,2.63,1,2.54,2.16,1,2.84,2.41,1,3.09,2.63,1,2.2799999999999998,1.94,1,2.5499999999999998,2.17,1,2.78,2.36,1,2.2799999999999998,1.94,1,2.5499999999999998,2.17,1,2.78,2.36,1]
["121700067508221","12",215,2010,30.315077840000001,-95.4717105,"Multi Span Long","Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1]
["121700067508225","12",240,2012,30.306114350000001,-95.46807373,"Multi Span Long","Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1]
["122370011411152","12",120,1996,30.084182240000001,-96.004215990000006,"prestress concrete girder",1.87,0.79,4,2.04,0.86,3,2.13,0.89,3,1.87,0.79,4,2.04,0.86,3,2.13,0.89,3,2.2200000000000002,0.94,2,2.41,1.01,1,2.5099999999999998,1.05,1,2.2200000000000002,0.94,2,2.41,1.01,1,2.5099999999999998,1.05,1,1.99,0.84,3,2.17,0.91,2,2.2599999999999998,0.95,2,1.99,0.84,3,2.17,0.91,2,2.2599999999999998,0.95,2]
["122370027104279","12",45,1987,29.778895089999999,-95.935771340000002,"concrete bridge",2.42,0.9,3,2.42,0.9,3,2.42,0.9,3,2.4300000000000002,0.9,3,2.42,0.9,3,2.42,0.9,3,3.23,1.2,1,3.23,1.2,1,3.23,1.2,1,3.23,1.2,1,3.23,1.2,1,3.23,1.2,1,2.92,1.0900000000000001,1,2.92,1.0900000000000001,1,2.92,1.0900000000000001,1,2.92,1.0900000000000001,1,2.92,1.0900000000000001,1,2.92,1.0900000000000001,1]
["122370027104285","12",70,1967,29.777259610000002,-95.881172649999996,"prestress concrete girder",2.23,0.79,4,2.23,0.79,4,2.23,0.79,4,2.23,0.79,4,2.23,0.79,4,2.23,0.79,4,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3]
["130080027102214","13",45,1966,29.761321250000002,-96.205670459999993,"concrete bridge",2.4,0.85,3,2.4,0.85,3,2.4,0.85,3,2.41,0.85,3,2.4,0.85,3,2.4,0.85,3,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1]
["130080027102215","13",50,2008,29.76295811,-96.185254850000007,"prestress concrete girder",2.41,2.0499999999999998,1,2.41,2.0499999999999998,1,2.41,2.0499999999999998,1,2.41,2.0499999999999998,1,2.41,2.0499999999999998,1,2.41,2.0499999999999998,1,3.27,2.78,1,3.27,2.78,1,3.27,2.78,1,3.27,2.78,1,3.27,2.78,1,3.27,2.78,1,2.93,2.4900000000000002,1,2.93,2.4900000000000002,1,2.93,2.4900000000000002,1,2.93,2.4900000000000002,1,2.93,2.4900000000000002,1,2.93,2.4900000000000002,1]
["130080027102216","13",50,1966,29.762790110000001,-96.185324850000001,"prestress concrete girder",2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.99,1.06,1,2.99,1.06,1,2.99,1.06,1,2.99,1.06,1,2.99,1.06,1,2.99,1.06,1,2.67,0.94,2,2.67,0.94,2,2.67,0.94,2,2.67,0.94,2,2.67,0.94,2,2.67,0.94,2]
["130080027103224","13",70,2008,29.765297879999999,-96.150632810000005,"prestress concrete girder",2.42,1.82,1,2.42,1.82,1,2.42,1.82,1,2.42,1.82,1,2.42,1.82,1,2.42,1.82,1,3.03,2.27,1,3.03,2.27,1,3.03,2.27,1,3.03,2.27,1,3.03,2.27,1,3.03,2.27,1,2.71,2.0299999999999998,1,2.71,2.0299999999999998,1,2.71,2.0299999999999998,1,2.71,2.0299999999999998,1,2.71,2.0299999999999998,1,2.71,2.0299999999999998,1]
["130450027101186","13",75,1966,29.741683890000001,-96.330571759999998,"steel girder",1.29,0.74,4,1.31,0.76,4,1.38,0.8,4,1.29,0.74,4,1.31,0.76,4,1.38,0.8,4,1.53,0.89,3,1.58,0.92,2,1.7,0.98,2,1.53,0.89,3,1.58,0.92,2,1.7,0.98,2,1.37,0.79,4,1.41,0.82,3,1.52,0.88,3,1.37,0.79,4,1.41,0.82,3,1.52,0.88,3]
["130760026601048","13",75,1969,29.907102609999999,-96.835337089999996,"prestress concrete girder",2.2599999999999998,0.8,4,2.2599999999999998,0.8,4,2.2599999999999998,0.8,4,2.2599999999999998,0.8,4,2.2599999999999998,0.8,4,2.2599999999999998,0.8,4,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3]
["130760026601070","13",90,1990,29.922698889999999,-96.877509149999995,"prestress concrete girder",2.16,0.91,2,2.17,0.91,2,2.17,0.91,2,2.16,0.91,2,2.17,0.91,2,2.17,0.91,2,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2]
["130760053506101","13",70,1969,29.696962259999999,-97.102477820000004,"prestress concrete girder",2.23,0.89,3,2.23,0.89,3,2.23,0.89,3,2.23,0.89,3,2.23,0.89,3,2.23,0.89,3,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.5099999999999998,1,2,2.5099999999999998,1,2,2.5099999999999998,1,2,2.5099999999999998,1,2,2.5099999999999998,1,2,2.5099999999999998,1,2]
["130760053507051","13",45,1967,29.69615825,-96.87134897,"concrete bridge",2.4,0.85,3,2.4,0.85,3,2.4,0.85,3,2.41,0.85,3,2.4,0.85,3,2.4,0.85,3,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1]
["130760053507070","13",70,1967,29.69173,-97.003198999999995,"prestress concrete girder",2.23,0.89,3,2.23,0.89,3,2.23,0.89,3,2.23,0.89,3,2.23,0.89,3,2.23,0.89,3,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.5099999999999998,1,2,2.5099999999999998,1,2,2.5099999999999998,1,2,2.5099999999999998,1,2,2.5099999999999998,1,2,2.5099999999999998,1,2]
["130760053507188","13",65,1967,29.694310380000001,-96.848812350000003,"prestress concrete girder",2.21,0.88,3,2.21,0.88,3,2.21,0.88,3,2.21,0.88,3,2.21,0.88,3,2.21,0.88,3,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.52,1,2,2.52,1,2,2.52,1,2,2.52,1,2,2.52,1,2,2.52,1,2]
["130900053504091","13",50,1970,29.649826409999999,-97.484189839999999,"prestress concrete girder",2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.99,1.2,1,2.99,1.2,1,2.99,1.2,1,2.99,1.2,1,2.99,1.2,1,2.99,1.2,1,2.67,1.06,1,2.67,1.06,1,2.67,1.06,1,2.67,1.06,1,2.67,1.06,1,2.67,1.06,1]
["130900053504096","13",50,1970,29.65816663,-97.415217459999994,"prestress concrete girder",2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.99,1.06,1,2.99,1.06,1,2.99,1.06,1,2.99,1.06,1,2.99,1.06,1,2.99,1.06,1,2.67,0.94,2,2.67,0.94,2,2.67,0.94,2,2.67,0.94,2,2.67,0.94,2,2.67,0.94,2]
["130900053505145","13",45,1971,29.662819729999999,-97.379390740000005,"concrete bridge",2.4,0.85,3,2.4,0.85,3,2.4,0.85,3,2.41,0.85,3,2.4,0.85,3,2.4,0.85,3,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1]
["130900053505146","13",45,1971,29.662611739999999,-97.379370730000005,"concrete bridge",2.4,0.85,3,2.4,0.85,3,2.4,0.85,3,2.41,0.85,3,2.4,0.85,3,2.4,0.85,3,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1]
["130900053505150","13",95,1971,29.666580939999999,-97.333679799999999,"prestress concrete girder",2.33,0.66,5,2.39,0.67,5,2.39,0.67,5,2.33,0.66,5,2.39,0.67,5,2.39,0.67,5,2.83,0.8,4,2.88,0.81,3,2.88,0.81,3,2.83,0.8,4,2.88,0.81,3,2.88,0.81,3,2.5499999999999998,0.72,4,2.59,0.73,4,2.59,0.73,4,2.5499999999999998,0.72,4,2.59,0.73,4,2.59,0.73,4]
["130900053505162","13",85,1972,29.688624740000002,-97.25311121,"prestress concrete girder",2.3199999999999998,0.82,3,2.3199999999999998,0.82,3,2.3199999999999998,0.82,3,2.3199999999999998,0.82,3,2.3199999999999998,0.82,3,2.3199999999999998,0.82,3,2.83,1,2,2.83,1,2,2.83,1,2,2.83,1,2,2.83,1,2,2.83,1,2,2.54,0.89,3,2.54,0.89,3,2.54,0.89,3,2.54,0.89,3,2.54,0.89,3,2.54,0.89,3]
["130900053505167","13",45,1971,29.692504719999999,-97.23101973,"concrete bridge",2.4,0.85,3,2.4,0.85,3,2.4,0.85,3,2.41,0.85,3,2.4,0.85,3,2.4,0.85,3,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1]
["130900053505169","13",95,1971,29.692301839999999,-97.210513259999999,"prestress concrete girder",2.33,0.83,3,2.39,0.84,3,2.39,0.84,3,2.33,0.83,3,2.39,0.84,3,2.39,0.84,3,2.83,1,2,2.88,1.01,1,2.88,1.01,1,2.83,1,2,2.88,1.01,1,2.88,1.01,1,2.5499999999999998,0.9,3,2.59,0.92,2,2.59,0.92,2,2.5499999999999998,0.9,3,2.59,0.92,2,2.59,0.92,2]
["131210008903010","13",100,1988,28.959832280000001,-96.686925709999997,"prestress concrete girder",2.0499999999999998,0.61,5,2.15,0.64,5,2.15,0.64,5,2.0499999999999998,0.61,5,2.15,0.64,5,2.15,0.64,5,2.46,0.73,4,2.58,0.77,4,2.58,0.77,4,2.46,0.73,4,2.58,0.77,4,2.58,0.77,4,2.2200000000000002,0.66,5,2.3199999999999998,0.69,5,2.3199999999999998,0.69,5,2.2200000000000002,0.66,5,2.3199999999999998,0.69,5,2.3199999999999998,0.69,5]
["131210008904062","13",110,1993,29.025173200000001,-96.553435129999997,"steel girder",1.71,0.79,4,1.62,0.75,4,1.57,0.73,4,1.37,0.63,5,1.5,0.7,5,1.56,0.72,4,1.91,0.88,3,1.82,0.84,3,1.78,0.82,3,1.59,0.73,4,1.74,0.8,4,1.78,0.82,3,1.72,0.79,4,1.64,0.76,4,1.6,0.74,4,1.43,0.66,5,1.57,0.73,4,1.6,0.74,4]
["131210008904122","13",75,1972,29.002857240000001,-96.598280729999999,"prestress concrete girder",2.2599999999999998,0.8,4,2.2599999999999998,0.8,4,2.2599999999999998,0.8,4,2.2599999999999998,0.8,4,2.2599999999999998,0.8,4,2.2599999999999998,0.8,4,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3]
["131210008904164","13",85,1972,29.049697129999998,-96.515597740000004,"prestress concrete girder",2.3199999999999998,0.82,3,2.3199999999999998,0.82,3,2.3199999999999998,0.82,3,2.3199999999999998,0.82,3,2.3199999999999998,0.82,3,2.3199999999999998,0.82,3,2.83,1,2,2.83,1,2,2.83,1,2,2.83,1,2,2.83,1,2,2.83,1,2,2.54,0.89,3,2.54,0.89,3,2.54,0.89,3,2.54,0.89,3,2.54,0.89,3,2.54,0.89,3]
["131210008904192","13",110,1976,29.0249752,-96.553284129999994,"prestress concrete girder",1.97,0.83,3,2.12,0.89,3,2.14,0.9,3,1.97,0.83,3,2.12,0.89,3,2.14,0.9,3,2.3199999999999998,0.98,2,2.54,1.07,1,2.54,1.07,1,2.3199999999999998,0.98,2,2.54,1.07,1,2.54,1.07,1,2.09,0.88,3,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.09,0.88,3,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2]
["132350008805050","13",150,2010,28.7519396,-97.00693527,"steel girder",1.76,1.32,1,1.92,1.44,1,2.09,1.57,1,1.72,1.29,1,1.73,1.3,1,1.8,1.35,1,2.09,1.57,1,2.29,1.72,1,2.48,1.86,1,1.9,1.42,1,1.97,1.48,1,2.09,1.57,1,1.88,1.41,1,2.06,1.55,1,2.23,1.67,1,1.71,1.28,1,1.77,1.33,1,1.88,1.41,1]
["132410008906085","13",80,1970,29.174104450000002,-96.302737260000001,"prestress concrete girder",2.29,0.81,3,2.29,0.81,3,2.29,0.81,3,2.29,0.81,3,2.29,0.81,3,2.29,0.81,3,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3]
["132410008907091","13",80,1970,29.177843129999999,-96.260916190000003,"prestress concrete girder",2.29,0.81,3,2.29,0.81,3,2.29,0.81,3,2.29,0.81,3,2.29,0.81,3,2.29,0.81,3,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3]
["132410008907128","13",180,1972,29.314820229999999,-96.125047379999998,"Multi Span Long",0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1]
["132410008907129","13",180,1972,29.31219389,-96.125086069999995,"Multi Span Long",0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1]
["140110011404130","14",95,1986,30.33631888,-97.366958249999996,"prestress concrete girder",2.1,0.88,3,2.16,0.91,2,2.16,0.91,2,2.1,0.88,3,2.16,0.91,2,2.16,0.91,2,2.5499999999999998,1.07,1,2.6,1.1000000000000001,1,2.6,1.1000000000000001,1,2.5499999999999998,1.07,1,2.6,1.1000000000000001,1,2.6,1.1000000000000001,1,2.2999999999999998,0.97,2,2.34,0.99,2,2.34,0.99,2,2.2999999999999998,0.97,2,2.34,0.99,2,2.34,0.99,2]
["141060001602201","14",100,1993,29.9131277,-97.897936310000006,"prestress concrete girder",2.0499999999999998,0.76,4,2.15,0.8,4,2.15,0.8,4,2.0499999999999998,0.76,4,2.15,0.8,4,2.15,0.8,4,2.46,0.92,2,2.58,0.96,2,2.58,0.96,2,2.46,0.92,2,2.58,0.96,2,2.58,0.96,2,2.2200000000000002,0.83,3,2.3199999999999998,0.86,3,2.3199999999999998,0.86,3,2.2200000000000002,0.83,3,2.3199999999999998,0.86,3,2.3199999999999998,0.86,3]
["141060001602226","14",85,2004,29.904895799999998,-97.902337349999996,"prestress concrete girder",2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.39,1,2,2.39,1,2,2.39,1,2,2.39,1,2,2.39,1,2,2.39,1,2]
["141060001602432","14",100,2014,30.058805339999999,-97.834358420000001,"prestress concrete girder",2.4300000000000002,2.0699999999999998,1,2.5499999999999998,2.17,1,2.5499999999999998,2.17,1,2.4300000000000002,2.0699999999999998,1,2.5499999999999998,2.17,1,2.5499999999999998,2.17,1,2.91,2.4700000000000002,1,3.05,2.59,1,3.05,2.59,1,2.91,2.4700000000000002,1,3.05,2.59,1,3.05,2.59,1,2.62,2.23,1,2.74,2.33,1,2.74,2.33,1,2.62,2.23,1,2.74,2.33,1,2.74,2.33,1]
["141060001603121","14",60,2004,29.892974240000001,-97.912478489999998,"prestress concrete girder",2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1]
["141060001603204","14",90,1996,29.85658286,-97.953293279999997,"prestress concrete girder",2.16,0.91,2,2.17,0.91,2,2.17,0.91,2,2.16,0.91,2,2.17,0.91,2,2.17,0.91,2,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2]
["141060001603212","14",105,2001,29.827766789999998,-97.985513589999996,"prestress concrete girder",2.0099999999999998,0.84,3,2.15,0.9,3,2.15,0.9,3,2.0099999999999998,0.84,3,2.15,0.9,3,2.15,0.9,3,2.39,1,2,2.56,1.08,1,2.56,1.08,1,2.39,1,2,2.56,1.08,1,2.56,1.08,1,2.15,0.9,3,2.2999999999999998,0.97,2,2.2999999999999998,0.97,2,2.15,0.9,3,2.2999999999999998,0.97,2,2.2999999999999998,0.97,2]
["142270001510413","14",95,1990,30.45608876,-97.666420740000007,"prestress concrete girder",2.1,0.88,3,2.16,0.91,2,2.16,0.91,2,2.1,0.88,3,2.16,0.91,2,2.16,0.91,2,2.5499999999999998,1.07,1,2.6,1.1000000000000001,1,2.6,1.1000000000000001,1,2.5499999999999998,1.07,1,2.6,1.1000000000000001,1,2.6,1.1000000000000001,1,2.2999999999999998,0.97,2,2.34,0.99,2,2.34,0.99,2,2.2999999999999998,0.97,2,2.34,0.99,2,2.34,0.99,2]
["142270001513118","14",70,1982,30.257046020000001,-97.736945070000004,"steel girder",1.26,0.73,4,1.31,0.76,4,1.43,0.83,3,1.26,0.73,4,1.31,0.76,4,1.43,0.83,3,1.52,0.88,3,1.61,0.93,2,1.79,1.04,1,1.52,0.88,3,1.61,0.93,2,1.79,1.04,1,1.36,0.79,4,1.44,0.83,3,1.61,0.93,2,1.36,0.79,4,1.44,0.83,3,1.61,0.93,2]
["142270001513210","14",70,1988,30.339201070000001,-97.700143949999998,"prestress concrete girder",2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1]
["142270001513344","14",50,1976,30.274311999999998,-97.731330999999997,"prestress concrete girder",2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,3.2,1.34,1,3.2,1.34,1,3.2,1.34,1,3.2,1.34,1,3.2,1.34,1,3.2,1.34,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1]
["142270001513345","14",135,1976,30.2731444,-97.731616849999995,"steel girder",1.68,0.77,4,1.86,0.86,3,1.89,0.88,3,1.49,0.69,5,1.55,0.71,4,1.65,0.76,4,2.0299999999999998,0.94,2,2.2000000000000002,1.01,1,2.1,0.97,2,1.66,0.77,4,1.77,0.82,3,1.92,0.89,3,1.82,0.84,3,1.98,0.91,2,1.89,0.88,3,1.49,0.69,5,1.59,0.73,4,1.73,0.8,4]
["142270001513450","14",265,2002,30.322459259999999,-97.703536909999997,"Multi Span Long",0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1]
["142270001513454","14",125,2004,30.21576533,-97.751885569999999,"prestress concrete special",1.81,0.68,0,2,0.74,0,2.12,0.79,0,1.81,0.68,0,2,0.74,0,2.12,0.79,0,2.16,0.8,0,2.35,0.87,0,2.5,0.93,0,2.16,0.8,0,2.35,0.87,0,2.5,0.93,0,1.95,0.73,0,2.12,0.79,0,2.25,0.83,0,1.95,0.73,0,2.12,0.79,0,2.25,0.83,0]
["142270001513456","14",120,2003,30.216913300000002,-97.751902950000002,"prestress concrete girder",1.87,0.79,4,2.04,0.86,3,2.13,0.89,3,1.87,0.79,4,2.04,0.86,3,2.13,0.89,3,2.2200000000000002,0.94,2,2.41,1.01,1,2.5099999999999998,1.05,1,2.2200000000000002,0.94,2,2.41,1.01,1,2.5099999999999998,1.05,1,1.99,0.84,3,2.17,0.91,2,2.2599999999999998,0.95,2,1.99,0.84,3,2.17,0.91,2,2.2599999999999998,0.95,2]
["142270001513457","14",75,2017,30.20158765,-97.761581579999998,"prestress concrete girder",2.4300000000000002,2.0699999999999998,1,2.4300000000000002,2.0699999999999998,1,2.4300000000000002,2.0699999999999998,1,2.4300000000000002,2.0699999999999998,1,2.4300000000000002,2.0699999999999998,1,2.4300000000000002,2.0699999999999998,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1]
["142270001513458","14",75,2003,30.20154866,-97.761476579999993,"prestress concrete girder",2.21,0.93,2,2.21,0.93,2,2.21,0.93,2,2.21,0.93,2,2.21,0.93,2,2.21,0.93,2,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.46,1.04,1,2.46,1.04,1,2.46,1.04,1,2.46,1.04,1,2.46,1.04,1,2.46,1.04,1]
["142270001513460","14",200,2004,30.219485930000001,-97.750136130000001,"Multi Span Long","Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1]
["142270001513510","14",115,1972,30.30207278,-97.714921669999995,"prestress concrete girder",2.31,0.93,2,2.4900000000000002,0.99,2,2.56,1.02,1,2.3199999999999998,0.93,2,2.4900000000000002,0.99,2,2.56,1.02,1,2.72,1.0900000000000001,1,2.97,1.19,1,3.03,1.21,1,2.72,1.0900000000000001,1,2.97,1.19,1,3.03,1.21,1,2.4500000000000002,0.98,2,2.67,1.06,1,2.72,1.0900000000000001,1,2.4500000000000002,0.98,2,2.67,1.06,1,2.72,1.0900000000000001,1]
["142270001601453","14",95,2017,30.149919999999998,-97.792952999999997,"prestress concrete girder",2.4500000000000002,2.08,1,2.52,2.14,1,2.52,2.14,1,2.4500000000000002,2.08,1,2.52,2.14,1,2.52,2.14,1,2.98,2.5299999999999998,1,3.04,2.58,1,3.04,2.58,1,2.98,2.5299999999999998,1,3.04,2.58,1,3.04,2.58,1,2.68,2.2799999999999998,1,2.73,2.3199999999999998,1,2.73,2.3199999999999998,1,2.68,2.2799999999999998,1,2.73,2.3199999999999998,1,2.73,2.3199999999999998,1]
["142460001508223","14",65,2000,30.773957100000001,-97.627048700000003,"prestress concrete girder",2.25,0.83,3,2.25,0.83,3,2.25,0.83,3,2.25,0.83,3,2.25,0.83,3,2.25,0.83,3,2.86,1.07,1,2.86,1.07,1,2.86,1.07,1,2.86,1.07,1,2.86,1.07,1,2.86,1.07,1,2.56,0.95,2,2.56,0.95,2,2.56,0.95,2,2.56,0.95,2,2.56,0.95,2,2.56,0.95,2]
["142460001508245","14",65,1986,30.633038030000002,-97.691356150000004,"prestress concrete girder",2.25,0.83,3,2.25,0.83,3,2.25,0.83,3,2.25,0.83,3,2.25,0.83,3,2.25,0.83,3,2.86,1.07,1,2.86,1.07,1,2.86,1.07,1,2.86,1.07,1,2.86,1.07,1,2.86,1.07,1,2.56,0.95,2,2.56,0.95,2,2.56,0.95,2,2.56,0.95,2,2.56,0.95,2,2.56,0.95,2]
["142460001508520","14",130,2008,30.633429039999999,-97.691659900000005,"prestress concrete girder",2.2599999999999998,1.92,1,2.54,2.16,1,2.69,2.29,1,2.2599999999999998,1.92,1,2.54,2.16,1,2.69,2.29,1,2.71,2.2999999999999998,1,2.96,2.52,1,3.19,2.71,1,2.71,2.2999999999999998,1,2.96,2.52,1,3.19,2.71,1,2.44,2.0699999999999998,1,2.66,2.2599999999999998,1,2.87,2.44,1,2.44,2.0699999999999998,1,2.66,2.2599999999999998,1,2.87,2.44,1]
["142460001509416","14",100,1990,30.502016770000001,-97.682731930000003,"prestress concrete girder",2.0499999999999998,0.76,4,2.15,0.8,4,2.15,0.8,4,2.0499999999999998,0.76,4,2.15,0.8,4,2.15,0.8,4,2.46,0.92,2,2.58,0.96,2,2.58,0.96,2,2.46,0.92,2,2.58,0.96,2,2.58,0.96,2,2.2200000000000002,0.83,3,2.3199999999999998,0.86,3,2.3199999999999998,0.86,3,2.2200000000000002,0.83,3,2.3199999999999998,0.86,3,2.3199999999999998,0.86,3]
["142460001509444","14",85,2002,30.553814630000002,-97.692632309999993,"prestress concrete girder",2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.66,0.99,2,2.66,0.99,2,2.66,0.99,2,2.66,0.99,2,2.66,0.99,2,2.66,0.99,2,2.39,0.89,3,2.39,0.89,3,2.39,0.89,3,2.39,0.89,3,2.39,0.89,3,2.39,0.89,3]
["142460001509500","14",95,2007,30.558340479999998,-97.692174510000001,"prestress concrete girder",2.4500000000000002,2.08,1,2.52,2.14,1,2.52,2.14,1,2.4500000000000002,2.08,1,2.52,2.14,1,2.52,2.14,1,2.98,2.5299999999999998,1,3.04,2.58,1,3.04,2.58,1,2.98,2.5299999999999998,1,3.04,2.58,1,3.04,2.58,1,2.68,2.2799999999999998,1,2.73,2.3199999999999998,1,2.73,2.3199999999999998,1,2.68,2.2799999999999998,1,2.73,2.3199999999999998,1,2.73,2.3199999999999998,1]
["142460001509522","14",100,2009,30.50941911,-97.685690910000005,"prestress concrete girder",2.4300000000000002,2.4300000000000002,1,2.5499999999999998,2.5499999999999998,1,2.5499999999999998,2.5499999999999998,1,2.4300000000000002,2.4300000000000002,1,2.5499999999999998,2.5499999999999998,1,2.5499999999999998,2.5499999999999998,1,2.91,2.91,1,3.05,3.05,1,3.05,3.05,1,2.91,2.91,1,3.05,3.05,1,3.05,3.05,1,2.62,2.62,1,2.74,2.74,1,2.74,2.74,1,2.62,2.62,1,2.74,2.74,1,2.74,2.74,1]
["142460044001244","14",125,2014,30.82271691,-97.780808280000002,"prestress concrete girder",2.29,1.95,1,2.54,2.16,1,2.69,2.29,1,2.2999999999999998,1.95,1,2.54,2.16,1,2.69,2.29,1,2.74,2.33,1,2.98,2.5299999999999998,1,3.17,2.69,1,2.74,2.33,1,2.98,2.5299999999999998,1,3.17,2.69,1,2.4700000000000002,2.1,1,2.68,2.2799999999999998,1,2.85,2.42,1,2.4700000000000002,2.1,1,2.68,2.2799999999999998,1,2.85,2.42,1]
["142460044001245","14",120,2014,30.827645860000001,-97.781837210000006,"prestress concrete girder",2.33,2.33,1,2.5499999999999998,2.5499999999999998,1,2.66,2.66,1,2.33,2.33,1,2.5499999999999998,2.5499999999999998,1,2.66,2.66,1,2.77,2.77,1,3.01,3.01,1,3.14,3.14,1,2.77,2.77,1,3.01,3.01,1,3.14,3.14,1,2.4900000000000002,2.4900000000000002,1,2.71,2.71,1,2.82,2.82,1,2.4900000000000002,2.4900000000000002,1,2.71,2.71,1,2.82,2.82,1]
["142460083601094","14",120,2015,30.875439999999998,-97.797889999999995,"prestress concrete girder",2.33,1.98,1,2.5499999999999998,2.17,1,2.66,2.2599999999999998,1,2.33,1.98,1,2.5499999999999998,2.17,1,2.66,2.2599999999999998,1,2.77,2.35,1,3.01,2.56,1,3.14,2.67,1,2.77,2.35,1,3.01,2.56,1,3.14,2.67,1,2.4900000000000002,2.12,1,2.71,2.2999999999999998,1,2.82,2.4,1,2.4900000000000002,2.12,1,2.71,2.2999999999999998,1,2.82,2.4,1]
["142460083601095","14",120,2015,30.875439999999998,-97.797889999999995,"prestress concrete girder",2.33,1.98,1,2.5499999999999998,2.17,1,2.66,2.2599999999999998,1,2.33,1.98,1,2.5499999999999998,2.17,1,2.66,2.2599999999999998,1,2.77,2.35,1,3.01,2.56,1,3.14,2.67,1,2.77,2.35,1,3.01,2.56,1,3.14,2.67,1,2.4900000000000002,2.12,1,2.71,2.2999999999999998,1,2.82,2.4,1,2.4900000000000002,2.12,1,2.71,2.2999999999999998,1,2.82,2.4,1]
["150070007305153","15",55,1975,28.843792929999999,-98.37688713,"prestress concrete girder",2.31,0.97,2,2.31,0.97,2,2.31,0.97,2,2.31,0.97,2,2.31,0.97,2,2.31,0.97,2,3.05,1.28,1,3.05,1.28,1,3.05,1.28,1,3.05,1.28,1,3.05,1.28,1,3.05,1.28,1,2.73,1.1499999999999999,1,2.73,1.1499999999999999,1,2.73,1.1499999999999999,1,2.73,1.1499999999999999,1,2.73,1.1499999999999999,1,2.73,1.1499999999999999,1]
["150070007310234","15",110,1979,29.051657540000001,-98.431802320000003,"prestress concrete girder",1.97,0.74,4,2.12,0.79,4,2.14,0.8,4,1.97,0.74,4,2.12,0.79,4,2.14,0.8,4,2.3199999999999998,0.86,3,2.54,0.95,2,2.54,0.95,2,2.3199999999999998,0.86,3,2.54,0.95,2,2.54,0.95,2,2.09,0.77,4,2.2799999999999998,0.85,3,2.2799999999999998,0.85,3,2.09,0.77,4,2.2799999999999998,0.85,3,2.2799999999999998,0.85,3]
["150070007310254","15",95,1980,28.94524281,-98.436765519999994,"prestress concrete girder",2.1,0.78,4,2.16,0.8,4,2.16,0.8,4,2.1,0.78,4,2.16,0.8,4,2.16,0.8,4,2.5499999999999998,0.95,2,2.6,0.97,2,2.6,0.97,2,2.5499999999999998,0.95,2,2.6,0.97,2,2.6,0.97,2,2.2999999999999998,0.86,3,2.34,0.87,3,2.34,0.87,3,2.2999999999999998,0.86,3,2.34,0.87,3,2.34,0.87,3]
["150150001607161","15",75,1984,29.552140990000002,-98.355329920000003,"prestress concrete girder",2.21,0.93,2,2.21,0.93,2,2.21,0.93,2,2.21,0.93,2,2.21,0.93,2,2.21,0.93,2,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.46,1.04,1,2.46,1.04,1,2.46,1.04,1,2.46,1.04,1,2.46,1.04,1,2.46,1.04,1]
["150150001703275","15",60,1974,29.269891749999999,-98.688704380000004,"prestress concrete girder",2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1]
["150150001703276","15",60,1974,29.269969750000001,-98.688744380000003,"prestress concrete girder",2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1]
["150150001703282","15",85,1974,29.249993979999999,-98.746869250000003,"prestress concrete girder",2.1800000000000002,0.65,5,2.1800000000000002,0.65,5,2.1800000000000002,0.65,5,2.1800000000000002,0.65,5,2.1800000000000002,0.65,5,2.1800000000000002,0.65,5,2.66,0.79,4,2.66,0.79,4,2.66,0.79,4,2.66,0.79,4,2.66,0.79,4,2.66,0.79,4,2.39,0.71,4,2.39,0.71,4,2.39,0.71,4,2.39,0.71,4,2.39,0.71,4,2.39,0.71,4]
["150150001709114","15",75,1985,29.322843339999999,-98.601113150000003,"steel girder",1.29,0.74,4,1.31,0.76,4,1.38,0.8,4,1.29,0.74,4,1.31,0.76,4,1.38,0.8,4,1.53,0.89,3,1.58,0.92,2,1.7,0.98,2,1.53,0.89,3,1.58,0.92,2,1.7,0.98,2,1.37,0.79,4,1.41,0.82,3,1.52,0.88,3,1.37,0.79,4,1.41,0.82,3,1.52,0.88,3]
["150150001710080","15",50,1952,29.41429033,-98.504453089999998,"concrete bridge",1.75,0.65,5,2.04,0.76,4,2.37,0.88,3,1.75,0.65,5,2.04,0.76,4,2.37,0.88,3,2.2200000000000002,0.83,3,2.5299999999999998,0.94,2,2.77,1.03,1,2.2200000000000002,0.83,3,2.5299999999999998,0.94,2,2.77,1.03,1,1.99,0.74,4,2.2799999999999998,0.85,3,2.5,0.93,2,1.99,0.74,4,2.2799999999999998,0.85,3,2.5,0.93,2]
["150150001710184","15",55,2016,29.51028827,-98.397739920000006,"steel girder",1.55,1.1599999999999999,1,1.8,1.35,1,1.94,1.46,1,1.55,1.1599999999999999,1,1.8,1.35,1,1.94,1.46,1,2.0099999999999998,1.51,1,2.2400000000000002,1.68,1,2.5499999999999998,1.91,1,2.0099999999999998,1.51,1,2.2400000000000002,1.68,1,2.5499999999999998,1.91,1,1.8,1.35,1,2.0099999999999998,1.51,1,2.2799999999999998,1.71,1,1.8,1.35,1,2.02,1.52,1,2.2799999999999998,1.71,1]
["150150001710188","15",55,2016,29.48407718,-98.403064950000001,"steel girder",1.55,1.1599999999999999,1,1.8,1.35,1,1.94,1.46,1,1.55,1.1599999999999999,1,1.8,1.35,1,1.94,1.46,1,2.0099999999999998,1.51,1,2.2400000000000002,1.68,1,2.5499999999999998,1.91,1,2.0099999999999998,1.51,1,2.2400000000000002,1.68,1,2.5499999999999998,1.91,1,1.8,1.35,1,2.0099999999999998,1.51,1,2.2799999999999998,1.71,1,1.8,1.35,1,2.02,1.52,1,2.2799999999999998,1.71,1]
["150150001710298","15",105,1972,29.43867595,-98.475528440000005,"steel girder",1.63,1.07,1,1.55,1.01,1,1.52,0.99,2,1.37,0.89,3,1.49,0.98,2,1.52,0.99,2,1.83,1.2,1,1.76,1.1599999999999999,1,1.73,1.1299999999999999,1,1.6,1.05,1,1.73,1.1299999999999999,1,1.73,1.1299999999999999,1,1.65,1.08,1,1.58,1.04,1,1.56,1.02,1,1.44,0.94,2,1.56,1.02,1,1.56,1.02,1]
["150150001710299","15",95,1972,29.440984749999998,-98.478698449999996,"steel girder",1.49,0.98,2,1.44,0.94,2,1.43,0.94,2,1.38,0.9,3,1.44,0.94,2,1.43,0.94,2,1.7,1.1100000000000001,1,1.66,1.0900000000000001,1,1.66,1.0900000000000001,1,1.61,1.05,1,1.66,1.0900000000000001,1,1.66,1.0900000000000001,1,1.53,1,2,1.49,0.98,2,1.49,0.98,2,1.45,0.95,2,1.49,0.98,2,1.49,0.98,2]
["150150001710359","15",115,1993,29.435902590000001,-98.494251980000001,"prestress concrete segmental",2.16,0,0,2.06,0,0,1.99,0,0,1.7,0,0,1.86,0,0,1.96,0,0,2.44,0,0,2.3199999999999998,0,0,2.25,0,0,1.94,0,0,2.16,0,0,2.2400000000000002,0,0,2.19,0,0,2.08,0,0,2.02,0,0,1.75,0,0,1.94,0,0,2.0099999999999998,0,0]
["150150001710361","15",100,1994,29.44012047,-98.485685790000005,"prestress concrete segmental",1.91,0,0,1.83,0,0,1.8,0,0,1.69,0,0,1.8,0,0,1.8,0,0,2.16,0,0,2.09,0,0,2.08,0,0,2,0,0,2.08,0,0,2.08,0,0,1.94,0,0,1.88,0,0,1.87,0,0,1.8,0,0,1.87,0,0,1.87,0,0]
["150150002407174","15",110,1990,29.37481344,-98.765134840000002,"prestress concrete girder",1.97,0.83,3,2.12,0.89,3,2.14,0.9,3,1.97,0.83,3,2.12,0.89,3,2.14,0.9,3,2.3199999999999998,0.98,2,2.54,1.07,1,2.54,1.07,1,2.3199999999999998,0.98,2,2.54,1.07,1,2.54,1.07,1,2.09,0.88,3,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.09,0.88,3,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2]
["150150002408137","15",70,1968,29.40488865,-98.558768450000002,"steel girder",1.26,0.73,4,1.31,0.76,4,1.43,0.83,3,1.26,0.73,4,1.31,0.76,4,1.43,0.83,3,1.52,0.88,3,1.61,0.93,2,1.79,1.04,1,1.52,0.88,3,1.61,0.93,2,1.79,1.04,1,1.36,0.79,4,1.44,0.83,3,1.61,0.93,2,1.36,0.79,4,1.44,0.83,3,1.61,0.93,2]
["150150002408143","15",65,1991,29.40464266,-98.557043399999998,"steel girder",1.25,0.82,3,1.33,0.87,3,1.51,0.99,2,1.25,0.82,3,1.33,0.87,3,1.51,0.99,2,1.54,1.01,1,1.68,1.1000000000000001,1,1.93,1.27,1,1.54,1.01,1,1.68,1.1000000000000001,1,1.93,1.27,1,1.38,0.9,3,1.51,0.99,2,1.73,1.1299999999999999,1,1.38,0.9,3,1.51,0.99,2,1.73,1.1299999999999999,1]
["150150002502106","15",65,1962,29.465633459999999,-98.291919960000001,"prestress concrete girder",2.21,0.62,5,2.21,0.62,5,2.21,0.62,5,2.21,0.62,5,2.21,0.62,5,2.21,0.62,5,2.81,0.79,4,2.81,0.79,4,2.81,0.79,4,2.81,0.79,4,2.81,0.79,4,2.81,0.79,4,2.52,0.71,4,2.52,0.71,4,2.52,0.71,4,2.52,0.71,4,2.52,0.71,4,2.52,0.71,4]
["150150002502109","15",45,1962,29.472646399999999,-98.269657559999999,"concrete bridge",2.4,0.85,3,2.4,0.85,3,2.4,0.85,3,2.41,0.85,3,2.4,0.85,3,2.4,0.85,3,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1]
["150150002502113","15",50,1962,29.47777769,-98.253992100000005,"prestress concrete girder",2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.99,1.06,1,2.99,1.06,1,2.99,1.06,1,2.99,1.06,1,2.99,1.06,1,2.99,1.06,1,2.67,0.94,2,2.67,0.94,2,2.67,0.94,2,2.67,0.94,2,2.67,0.94,2,2.67,0.94,2]
["150150002502163","15",100,1967,29.394376099999999,-98.485998499999994,"steel girder",1.56,1.02,1,1.49,0.98,2,1.47,0.96,2,1.38,0.9,3,1.47,0.96,2,1.47,0.96,2,1.76,1.1599999999999999,1,1.7,1.1100000000000001,1,1.69,1.1100000000000001,1,1.63,1.07,1,1.7,1.1100000000000001,1,1.69,1.1100000000000001,1,1.58,1.04,1,1.53,1,2,1.52,0.99,2,1.46,0.95,2,1.53,1,2,1.52,0.99,2]
["150150002502180","15",90,1968,29.408661779999999,-98.436817399999995,"steel girder",1.43,0.94,2,1.39,0.91,2,1.4,0.92,2,1.36,0.89,3,1.39,0.91,2,1.4,0.92,2,1.64,1.07,1,1.62,1.06,1,1.64,1.07,1,1.61,1.05,1,1.62,1.06,1,1.64,1.07,1,1.47,0.96,2,1.45,0.95,2,1.47,0.96,2,1.45,0.95,2,1.45,0.95,2,1.47,0.96,2]
["150150007207224","15",50,1988,29.670493329999999,-98.630286679999998,"concrete bridge",1.75,0.74,4,2.04,0.86,3,2.37,0.99,2,1.75,0.74,4,2.04,0.86,3,2.37,0.99,2,2.2200000000000002,0.94,2,2.5299999999999998,1.06,1,2.77,1.1599999999999999,1,2.2200000000000002,0.94,2,2.5299999999999998,1.06,1,2.77,1.1599999999999999,1,1.99,0.84,3,2.2799999999999998,0.96,2,2.5,1.05,1,1.99,0.84,3,2.2799999999999998,0.96,2,2.5,1.05,1]
["150150007208244","15",130,1987,29.59088878,-98.601142609999997,"prestress concrete girder",1.76,0.74,4,1.97,0.83,3,2.1,0.88,3,1.76,0.74,4,1.97,0.83,3,2.1,0.88,3,2.11,0.88,3,2.2999999999999998,0.97,2,2.48,1.05,1,2.11,0.88,3,2.2999999999999998,0.97,2,2.48,1.05,1,1.9,0.8,4,2.0699999999999998,0.87,3,2.23,0.94,2,1.9,0.8,4,2.0699999999999998,0.87,3,2.23,0.94,2]
["150150007208251","15",130,1992,29.605957679999999,-98.601964580000001,"prestress concrete girder",1.76,0.65,5,1.97,0.74,4,2.1,0.78,4,1.76,0.65,5,1.97,0.74,4,2.1,0.78,4,2.11,0.78,4,2.2999999999999998,0.86,3,2.48,0.92,2,2.11,0.78,4,2.2999999999999998,0.86,3,2.48,0.92,2,1.9,0.71,4,2.0699999999999998,0.77,4,2.23,0.83,3,1.9,0.71,4,2.0699999999999998,0.77,4,2.23,0.83,3]
["150150007208257","15",105,1992,29.599774999999998,-98.599603000000002,"prestress concrete girder",2.0099999999999998,0.74,4,2.15,0.8,4,2.15,0.8,4,2.0099999999999998,0.74,4,2.15,0.8,4,2.15,0.8,4,2.39,0.89,3,2.56,0.95,2,2.56,0.95,2,2.39,0.89,3,2.56,0.95,2,2.56,0.95,2,2.15,0.8,4,2.2999999999999998,0.86,3,2.2999999999999998,0.86,3,2.15,0.8,4,2.2999999999999998,0.86,3,2.2999999999999998,0.86,3]
["150150007208389","15",115,2015,29.563489999999998,-98.591419999999999,"prestress concrete girder",2.38,2.38,1,2.56,2.56,1,2.63,2.63,1,2.38,2.38,1,2.56,2.56,1,2.63,2.63,1,2.8,2.8,1,3.05,3.05,1,3.12,3.12,1,2.8,2.8,1,3.05,3.05,1,3.12,3.12,1,2.52,2.52,1,2.75,2.75,1,2.8,2.8,1,2.52,2.52,1,2.75,2.75,1,2.8,2.8,1]
["150150007208397","15",100,2018,29.62487264,-98.609508640000001,"prestress concrete girder",2.4300000000000002,2.0699999999999998,1,2.5499999999999998,2.17,1,2.5499999999999998,2.17,1,2.4300000000000002,2.0699999999999998,1,2.5499999999999998,2.17,1,2.5499999999999998,2.17,1,2.91,2.4700000000000002,1,3.05,2.59,1,3.05,2.59,1,2.91,2.4700000000000002,1,3.05,2.59,1,3.05,2.59,1,2.62,2.23,1,2.74,2.33,1,2.74,2.33,1,2.62,2.23,1,2.74,2.33,1,2.74,2.33,1]
["150150007212039","15",85,1949,29.44038041,-98.509304389999997,"concrete bridge",1.69,0.63,5,1.66,0.62,5,1.69,0.63,5,1.65,0.62,5,1.66,0.62,5,1.69,0.63,5,1.95,0.73,4,1.95,0.73,4,2.0099999999999998,0.74,4,1.95,0.73,4,1.95,0.73,4,2.0099999999999998,0.74,4,1.75,0.65,5,1.75,0.65,5,1.8,0.67,5,1.75,0.65,5,1.75,0.65,5,1.8,0.67,5]
["150150007212042","15",50,1992,29.438719469999999,-98.505089269999999,"steel girder",1.92,1.1100000000000001,1,1.92,1.1100000000000001,1,1.92,1.1100000000000001,1,1.93,1.1200000000000001,1,1.92,1.1100000000000001,1,1.92,1.1100000000000001,1,2.61,1.51,1,2.61,1.51,1,2.61,1.51,1,2.61,1.51,1,2.61,1.51,1,2.61,1.51,1,2.33,1.34,1,2.33,1.34,1,2.33,1.34,1,2.33,1.34,1,2.33,1.34,1,2.33,1.34,1]
["150150007212209","15",110,1993,29.443587300000001,-98.515314559999993,"prestress concrete segmental",2.1,0,0,1.98,0,0,1.93,0,0,1.68,0,0,1.84,0,0,1.92,0,0,2.34,0,0,2.2400000000000002,0,0,2.1800000000000002,0,0,1.95,0,0,2.14,0,0,2.1800000000000002,0,0,2.11,0,0,2.0099999999999998,0,0,1.96,0,0,1.75,0,0,1.92,0,0,1.96,0,0]
["150150007212236","15",180,1990,29.431759710000001,-98.49998909,"Multi Span Long",0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1]
["150150007212265","15",125,1994,29.550213230000001,-98.585401649999994,"prestress concrete girder",1.81,0.77,4,2,0.84,3,2.12,0.89,3,1.81,0.77,4,2,0.84,3,2.12,0.89,3,2.16,0.91,2,2.35,0.99,2,2.5,1.05,1,2.16,0.91,2,2.35,0.99,2,2.5,1.05,1,1.95,0.82,3,2.12,0.89,3,2.25,0.94,2,1.95,0.82,3,2.12,0.89,3,2.25,0.94,2]
["150150007212276","15",60,1999,29.531106059999999,-98.561791659999997,"prestress concrete girder",2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1]
["150150007212298","15",100,2008,29.466713590000001,-98.516120430000001,"prestress concrete girder",2.4300000000000002,2.0699999999999998,1,2.5499999999999998,2.17,1,2.5499999999999998,2.17,1,2.4300000000000002,2.0699999999999998,1,2.5499999999999998,2.17,1,2.5499999999999998,2.17,1,2.91,2.4700000000000002,1,3.05,2.59,1,3.05,2.59,1,2.91,2.4700000000000002,1,3.05,2.59,1,3.05,2.59,1,2.62,2.23,1,2.74,2.33,1,2.74,2.33,1,2.62,2.23,1,2.74,2.33,1,2.74,2.33,1]
["150150007212302","15",135,2008,29.481380300000001,-98.526426099999995,"prestress concrete girder",2.23,1.9,1,2.4900000000000002,2.12,1,2.68,2.2799999999999998,1,2.23,1.9,1,2.4900000000000002,2.12,1,2.68,2.2799999999999998,1,2.65,2.25,1,2.94,2.5,1,3.15,2.68,1,2.65,2.25,1,2.94,2.5,1,3.15,2.68,1,2.39,2.0299999999999998,1,2.65,2.25,1,2.84,2.41,1,2.39,2.0299999999999998,1,2.65,2.25,1,2.84,2.41,1]
["150150007308082","15",50,1967,29.28981924,-98.395112800000007,"prestress concrete girder",2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.99,1.06,1,2.99,1.06,1,2.99,1.06,1,2.99,1.06,1,2.99,1.06,1,2.99,1.06,1,2.67,0.94,2,2.67,0.94,2,2.67,0.94,2,2.67,0.94,2,2.67,0.94,2,2.67,0.94,2]
["150830001706251","15",100,1973,28.899388129999998,-99.114452290000003,"prestress concrete girder",2.3199999999999998,0.93,2,2.4300000000000002,0.97,2,2.4300000000000002,0.97,2,2.3199999999999998,0.93,2,2.4300000000000002,0.97,2,2.4300000000000002,0.97,2,2.78,1.1100000000000001,1,2.91,1.1599999999999999,1,2.91,1.1599999999999999,1,2.78,1.1100000000000001,1,2.91,1.1599999999999999,1,2.91,1.1599999999999999,1,2.5099999999999998,1,2,2.62,1.05,1,2.62,1.05,1,2.5099999999999998,1,2,2.62,1.05,1,2.62,1.05,1]
["150950053502114","15",85,1969,29.61487739,-97.832055789999998,"prestress concrete girder",2.3199999999999998,0.93,2,2.3199999999999998,0.93,2,2.3199999999999998,0.93,2,2.3199999999999998,0.93,2,2.3199999999999998,0.93,2,2.3199999999999998,0.93,2,2.83,1.1299999999999999,1,2.83,1.1299999999999999,1,2.83,1.1299999999999999,1,2.83,1.1299999999999999,1,2.83,1.1299999999999999,1,2.83,1.1299999999999999,1,2.54,1.01,1,2.54,1.01,1,2.54,1.01,1,2.54,1.01,1,2.54,1.01,1,2.54,1.01,1]
["151330014214116","15",75,1972,30.116030930000001,-99.199888270000002,"prestress concrete girder",2.2599999999999998,0.9,3,2.2599999999999998,0.9,3,2.2599999999999998,0.9,3,2.2599999999999998,0.9,3,2.2599999999999998,0.9,3,2.2599999999999998,0.9,3,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.5099999999999998,1,2,2.5099999999999998,1,2,2.5099999999999998,1,2,2.5099999999999998,1,2,2.5099999999999998,1,2,2.5099999999999998,1,2]
["161490044701151","16",120,2008,28.333057289999999,-98.090053339999997,"prestress concrete girder",2.33,1.98,1,2.5499999999999998,2.17,1,2.66,2.2599999999999998,1,2.33,1.98,1,2.5499999999999998,2.17,1,2.66,2.2599999999999998,1,2.77,2.35,1,3.01,2.56,1,3.14,2.67,1,2.77,2.35,1,3.01,2.56,1,3.14,2.67,1,2.4900000000000002,2.12,1,2.71,2.2999999999999998,1,2.82,2.4,1,2.4900000000000002,2.12,1,2.71,2.2999999999999998,1,2.82,2.4,1]
["162050007405048","16",130,1986,27.89569358,-97.629254169999996,"steel girder",1.7,0.79,4,1.88,0.87,3,1.81,0.83,3,1.45,0.67,5,1.54,0.71,4,1.65,0.76,4,2.0499999999999998,0.95,2,2.12,0.98,2,2.02,0.94,2,1.63,0.76,4,1.77,0.82,3,1.9,0.88,3,1.84,0.85,3,1.9,0.88,3,1.82,0.84,3,1.47,0.68,5,1.59,0.73,4,1.71,0.79,4]
["172360067507251","17",130,2018,30.547426999999999,-95.497602999999998,"prestress concrete girder",2.2599999999999998,2.2599999999999998,1,2.54,2.54,1,2.69,2.69,1,2.2599999999999998,2.2599999999999998,1,2.54,2.54,1,2.69,2.69,1,2.71,2.71,1,2.96,2.96,1,3.19,3.19,1,2.71,2.71,1,2.96,2.96,1,3.19,3.19,1,2.44,2.44,1,2.66,2.66,1,2.87,2.87,1,2.44,2.44,1,2.66,2.66,1,2.87,2.87,1]
["180570000911272","18",95,1965,32.774791520000001,-96.787696170000004,"concrete bridge",1.83,0.68,5,1.77,0.66,5,1.76,0.65,5,1.69,0.63,5,1.77,0.66,5,1.76,0.65,5,2.09,0.77,4,2.0299999999999998,0.75,4,2.04,0.76,4,1.98,0.74,4,2.0299999999999998,0.75,4,2.04,0.76,4,1.87,0.7,5,1.82,0.68,5,1.83,0.68,5,1.78,0.66,5,1.82,0.68,5,1.83,0.68,5]
["180570004707260","18",60,1993,32.898809630000002,-96.768857839999995,"prestress concrete girder",2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1]
["180570019603070","18",70,2014,32.938284629999998,-96.902322470000001,"steel girder",1.71,1.28,1,1.77,1.33,1,1.94,1.46,1,1.71,1.28,1,1.78,1.34,1,1.94,1.46,1,2.06,1.55,1,2.1800000000000002,1.64,1,2.4300000000000002,1.82,1,2.06,1.55,1,2.1800000000000002,1.64,1,2.4300000000000002,1.82,1,1.85,1.39,1,1.96,1.47,1,2.1800000000000002,1.64,1,1.85,1.39,1,1.96,1.47,1,2.1800000000000002,1.64,1]
["180570019603275","18",80,1961,32.862609259999999,-96.89406314,"steel girder",1.33,0.77,4,1.33,0.77,4,1.37,0.79,4,1.33,0.77,4,1.33,0.77,4,1.37,0.79,4,1.55,0.89,3,1.57,0.91,2,1.65,0.95,2,1.55,0.89,3,1.57,0.91,2,1.65,0.95,2,1.39,0.8,4,1.41,0.82,3,1.48,0.86,3,1.39,0.8,4,1.41,0.82,3,1.48,0.86,3]
["180570237401459","18",120,2005,32.924360999999998,-96.764900000000011,"prestress concrete special",2.33,1.98,0,2.5499999999999998,2.17,0,2.66,2.2599999999999998,0,2.33,1.98,0,2.5499999999999998,2.17,0,2.66,2.2599999999999998,0,2.77,2.35,0,3.01,2.56,0,3.14,2.67,0,2.77,2.35,0,3.01,2.56,0,3.14,2.67,0,2.4900000000000002,2.12,0,2.71,2.2999999999999998,0,2.82,2.4,0,2.4900000000000002,2.12,0,2.71,2.2999999999999998,0,2.82,2.4,0]
["180570237402066","18",70,1967,32.870745999999997,-96.673884999999999,"steel girder",1.26,0.73,4,1.31,0.76,4,1.43,0.83,3,1.26,0.73,4,1.31,0.76,4,1.43,0.83,3,1.52,0.88,3,1.61,0.93,2,1.79,1.04,1,1.52,0.88,3,1.61,0.93,2,1.79,1.04,1,1.36,0.79,4,1.44,0.83,3,1.61,0.93,2,1.36,0.79,4,1.44,0.83,3,1.61,0.93,2]
["180570237403182","18",75,1974,32.642027210000002,-96.82407551,"prestress concrete girder",2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2]
["180570237404299","18",200,1975,32.672231830000001,-96.947877689999999,"Multi Span Long",0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1]
["180610008113115","18",80,1969,33.064726,-97.242497,"prestress concrete girder",2.29,0.54,5,2.29,0.54,5,2.29,0.54,5,2.29,0.54,5,2.29,0.54,5,2.29,0.54,5,2.81,0.66,5,2.81,0.66,5,2.81,0.66,5,2.81,0.66,5,2.81,0.66,5,2.81,0.66,5,2.52,0.59,5,2.52,0.59,5,2.52,0.59,5,2.52,0.59,5,2.52,0.59,5,2.52,0.59,5]
["180610019602379","18",85,2006,32.996265999999999,-96.952432999999999,"prestress concrete girder",2.4700000000000002,2.1,1,2.4700000000000002,2.1,1,2.4700000000000002,2.1,1,2.4700000000000002,2.1,1,2.4700000000000002,2.1,1,2.4700000000000002,2.1,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,2.71,2.2999999999999998,1,2.71,2.2999999999999998,1,2.71,2.2999999999999998,1,2.71,2.2999999999999998,1,2.71,2.2999999999999998,1,2.71,2.2999999999999998,1]
["190190021802049","19",90,1981,33.411868890000001,-94.097197649999998,"prestress concrete girder",2.16,0.91,2,2.17,0.91,2,2.17,0.91,2,2.16,0.91,2,2.17,0.91,2,2.17,0.91,2,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2]
["191030049509209","19",75,1965,32.489055209999997,-94.409444260000001,"prestress concrete girder",2.2599999999999998,0.9,3,2.2599999999999998,0.9,3,2.2599999999999998,0.9,3,2.2599999999999998,0.9,3,2.2599999999999998,0.9,3,2.2599999999999998,0.9,3,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.5099999999999998,1,2,2.5099999999999998,1,2,2.5099999999999998,1,2,2.5099999999999998,1,2,2.5099999999999998,1,2,2.5099999999999998,1,2]
["201240002813082","20",90,1989,30.09596848,-94.116840060000001,"steel girder",1.43,0.66,5,1.39,0.64,5,1.4,0.65,5,1.36,0.63,5,1.39,0.64,5,1.4,0.65,5,1.64,0.76,4,1.62,0.75,4,1.64,0.76,4,1.61,0.74,4,1.62,0.75,4,1.64,0.76,4,1.47,0.68,5,1.45,0.67,5,1.47,0.68,5,1.45,0.67,5,1.45,0.67,5,1.47,0.68,5]
["210310003907365","21",95,2005,26.135668729999999,-97.649439509999993,"prestress concrete girder",2.4500000000000002,2.08,1,2.52,2.14,1,2.52,2.14,1,2.4500000000000002,2.08,1,2.52,2.14,1,2.52,2.14,1,2.98,2.5299999999999998,1,3.04,2.58,1,3.04,2.58,1,2.98,2.5299999999999998,1,3.04,2.58,1,3.04,2.58,1,2.68,2.2799999999999998,1,2.73,2.3199999999999998,1,2.73,2.3199999999999998,1,2.68,2.2799999999999998,1,2.73,2.3199999999999998,1,2.73,2.3199999999999998,1]
["210310003919184","21",85,1969,26.163653159999999,-97.848584220000006,"prestress concrete girder",2.3199999999999998,0.82,3,2.3199999999999998,0.82,3,2.3199999999999998,0.82,3,2.3199999999999998,0.82,3,2.3199999999999998,0.82,3,2.3199999999999998,0.82,3,2.83,1,2,2.83,1,2,2.83,1,2,2.83,1,2,2.83,1,2,2.83,1,2,2.54,0.89,3,2.54,0.89,3,2.54,0.89,3,2.54,0.89,3,2.54,0.89,3,2.54,0.89,3]
["211090003918343","21",115,2005,26.179948580000001,-98.041377870000005,"prestress concrete girder",2.38,2.02,1,2.56,2.1800000000000002,1,2.63,2.2400000000000002,1,2.38,2.02,1,2.56,2.1800000000000002,1,2.63,2.2400000000000002,1,2.8,2.38,1,3.05,2.59,1,3.12,2.65,1,2.8,2.38,1,3.05,2.59,1,3.12,2.65,1,2.52,2.14,1,2.75,2.34,1,2.8,2.38,1,2.52,2.14,1,2.75,2.34,1,2.8,2.38,1]
["212450032710057","21",120,2003,26.467280559999999,-97.770811109999997,"prestress concrete girder",1.87,0.79,4,2.04,0.86,3,2.13,0.89,3,1.87,0.79,4,2.04,0.86,3,2.13,0.89,3,2.2200000000000002,0.94,2,2.41,1.01,1,2.5099999999999998,1.05,1,2.2200000000000002,0.94,2,2.41,1.01,1,2.5099999999999998,1.05,1,1.99,0.84,3,2.17,0.91,2,2.2599999999999998,0.95,2,1.99,0.84,3,2.17,0.91,2,2.2599999999999998,0.95,2]
["222400001806147","22",75,1981,27.508711850000001,-99.503097729999993,"prestress concrete special",1.58,0.59,0,1.61,0.6,0,1.7,0.63,0,1.58,0.59,0,1.61,0.6,0,1.7,0.63,0,1.88,0.7,0,1.93,0.72,0,2.08,0.77,0,1.88,0.7,0,1.93,0.72,0,2.08,0.77,0,1.68,0.62,0,1.73,0.65,0,1.87,0.7,0,1.68,0.62,0,1.73,0.65,0,1.87,0.7,0]
["241160212106179","24",70,1965,31.304020099999999,-105.83993275,"prestress concrete girder",2.23,0.79,4,2.23,0.79,4,2.23,0.79,4,2.23,0.79,4,2.23,0.79,4,2.23,0.79,4,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3]
["010920004703157","01",50,1963,33.576071300000002,-96.602693220000006,"prestress concrete girder",2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.99,1.2,1,2.99,1.2,1,2.99,1.2,1,2.99,1.2,1,2.99,1.2,1,2.99,1.2,1,2.67,1.06,1,2.67,1.06,1,2.67,1.06,1,2.67,1.06,1,2.67,1.06,1,2.67,1.06,1]
["021270001403231","02",50,1965,32.543706649999997,-97.314871409999995,"prestress concrete girder",2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.99,1.06,1,2.99,1.06,1,2.99,1.06,1,2.99,1.06,1,2.99,1.06,1,2.99,1.06,1,2.67,0.94,2,2.67,0.94,2,2.67,0.94,2,2.67,0.94,2,2.67,0.94,2,2.67,0.94,2]
["021840031401074","02",80,1970,32.701160649999998,-97.960257499999997,"prestress concrete girder",2.29,0.65,5,2.29,0.65,5,2.29,0.65,5,2.29,0.65,5,2.29,0.65,5,2.29,0.65,5,2.81,0.79,4,2.81,0.79,4,2.81,0.79,4,2.81,0.79,4,2.81,0.79,4,2.81,0.79,4,2.52,0.71,4,2.52,0.71,4,2.52,0.71,4,2.52,0.71,4,2.52,0.71,4,2.52,0.71,4]
["022200000813120","02",60,1963,32.689002909999999,-97.240829489999996,"prestress concrete girder",2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.84,1,2,2.84,1,2,2.84,1,2,2.84,1,2,2.84,1,2,2.84,1,2,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3]
["022200000814203","02",140,1973,32.837772049999998,-97.358682490000007,"steel girder",1.67,1.1000000000000001,1,1.84,1.21,1,1.96,1.28,1,1.52,0.99,2,1.57,1.03,1,1.66,1.0900000000000001,1,2,1.31,1,2.2000000000000002,1.44,1,2.1800000000000002,1.43,1,1.69,1.1100000000000001,1,1.79,1.17,1,1.94,1.27,1,1.8,1.18,1,1.98,1.29,1,1.96,1.28,1,1.52,0.99,2,1.61,1.05,1,1.75,1.1499999999999999,1]
["022200000815219","02",120,1975,32.73326599,-97.481345849999997,"prestress concrete girder",1.87,0.7,5,2.04,0.76,4,2.13,0.79,4,1.87,0.7,5,2.04,0.76,4,2.13,0.79,4,2.2200000000000002,0.83,3,2.41,0.89,3,2.5099999999999998,0.93,2,2.2200000000000002,0.83,3,2.41,0.89,3,2.5099999999999998,0.93,2,1.99,0.74,4,2.17,0.8,4,2.2599999999999998,0.84,3,1.99,0.74,4,2.17,0.8,4,2.2599999999999998,0.84,3]
["022200001416548","02",220,2014,32.886029999999998,-97.317139999999995,"Multi Span Long","Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1]
["022200106801564","02",100,2017,32.72963,-97.503700000000009,"prestress concrete girder",2.4300000000000002,2.4300000000000002,1,2.5499999999999998,2.5499999999999998,1,2.5499999999999998,2.5499999999999998,1,2.4300000000000002,2.4300000000000002,1,2.5499999999999998,2.5499999999999998,1,2.5499999999999998,2.5499999999999998,1,2.91,2.91,1,3.05,3.05,1,3.05,3.05,1,2.91,2.91,1,3.05,3.05,1,3.05,3.05,1,2.62,2.62,1,2.74,2.74,1,2.74,2.74,1,2.62,2.62,1,2.74,2.74,1,2.74,2.74,1]
["022200106802488","02",120,2010,32.759773459999998,-97.097155009999994,"prestress concrete girder",2.33,2.33,1,2.5499999999999998,2.5499999999999998,1,2.66,2.66,1,2.33,2.33,1,2.5499999999999998,2.5499999999999998,1,2.66,2.66,1,2.77,2.77,1,3.01,3.01,1,3.14,3.14,1,2.77,2.77,1,3.01,3.01,1,3.14,3.14,1,2.4900000000000002,2.4900000000000002,1,2.71,2.71,1,2.82,2.82,1,2.4900000000000002,2.4900000000000002,1,2.71,2.71,1,2.82,2.82,1]
["022200237405496","02",110,2005,32.67753845,-97.092598429999995,"prestress concrete girder",2.4,2.4,1,2.58,2.58,1,2.6,2.6,1,2.4,2.4,1,2.58,2.58,1,2.6,2.6,1,2.83,2.83,1,3.09,3.09,1,3.09,3.09,1,2.83,2.83,1,3.09,3.09,1,3.09,3.09,1,2.54,2.54,1,2.78,2.78,1,2.78,2.78,1,2.54,2.54,1,2.78,2.78,1,2.78,2.78,1]
["030490019501120","03",90,1985,33.624398130000003,-97.152237339999999,"steel girder",1.43,0.94,2,1.39,0.91,2,1.4,0.92,2,1.36,0.89,3,1.39,0.91,2,1.4,0.92,2,1.64,1.07,1,1.62,1.06,1,1.64,1.07,1,1.61,1.05,1,1.62,1.06,1,1.64,1.07,1,1.47,0.96,2,1.45,0.95,2,1.47,0.96,2,1.45,0.95,2,1.45,0.95,2,1.47,0.96,2]
["032430015604089","03",100,1990,33.893611819999997,-98.503730970000007,"prestress concrete special",1.91,0.81,0,1.83,0.77,0,1.8,0.76,0,1.69,0.71,0,1.8,0.76,0,1.8,0.76,0,2.16,0.91,0,2.09,0.88,0,2.08,0.88,0,2,0.84,0,2.08,0.88,0,2.08,0.88,0,1.94,0.82,0,1.88,0.79,0,1.87,0.79,0,1.8,0.76,0,1.87,0.79,0,1.87,0.79,0]
["041800009003038","04",65,1969,35.269510490000002,-102.67362846,"steel girder",1.25,0.57999999999999996,5,1.33,0.61,5,1.51,0.7,5,1.25,0.57999999999999996,5,1.33,0.61,5,1.51,0.7,5,1.54,0.71,4,1.68,0.77,4,1.93,0.89,3,1.54,0.71,4,1.68,0.77,4,1.93,0.89,3,1.38,0.64,5,1.51,0.7,5,1.73,0.8,4,1.38,0.64,5,1.51,0.7,5,1.73,0.8,4]
["041910016809069","04",75,1990,35.175508290000003,-101.85520803,"steel girder",1.29,0.74,4,1.31,0.76,4,1.38,0.8,4,1.29,0.74,4,1.31,0.76,4,1.38,0.8,4,1.53,0.89,3,1.58,0.92,2,1.7,0.98,2,1.53,0.89,3,1.58,0.92,2,1.7,0.98,2,1.37,0.79,4,1.41,0.82,3,1.52,0.88,3,1.37,0.79,4,1.41,0.82,3,1.52,0.88,3]
["051520006707084","05",120,1978,33.69387364,-101.83692243,"prestress concrete girder",2.13,0.79,4,2.16,0.8,4,2.06,0.77,4,1.72,0.64,5,1.88,0.7,5,1.99,0.74,4,2.5499999999999998,0.95,2,2.41,0.89,3,2.33,0.86,3,1.95,0.73,4,2.1800000000000002,0.81,3,2.2799999999999998,0.85,3,2.29,0.85,3,2.16,0.8,4,2.09,0.77,4,1.76,0.65,5,1.96,0.73,4,2.0499999999999998,0.76,4]
["061860014001321","06",75,1983,30.897277039999999,-102.8546856,"prestress concrete girder",2.21,0.93,2,2.21,0.93,2,2.21,0.93,2,2.21,0.93,2,2.21,0.93,2,2.21,0.93,2,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.46,1.04,1,2.46,1.04,1,2.46,1.04,1,2.46,1.04,1,2.46,1.04,1,2.46,1.04,1]
["061950000306077","06",60,1968,31.361303490000001,-103.6862884,"prestress concrete girder",2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.84,1,2,2.84,1,2,2.84,1,2,2.84,1,2,2.84,1,2,2.84,1,2,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3]
["070530014013294","07",70,1980,30.741204379999999,-101.67401762,"prestress concrete girder",2.23,0.83,3,2.23,0.83,3,2.23,0.83,3,2.23,0.83,3,2.23,0.83,3,2.23,0.83,3,2.79,1.04,1,2.79,1.04,1,2.79,1.04,1,2.79,1.04,1,2.79,1.04,1,2.79,1.04,1,2.5,0.93,2,2.5,0.93,2,2.5,0.93,2,2.5,0.93,2,2.5,0.93,2,2.5,0.93,2]
["072180014107148","07",50,1978,30.460669849999999,-100.14288455000001,"prestress concrete girder",2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,3.2,1.34,1,3.2,1.34,1,3.2,1.34,1,3.2,1.34,1,3.2,1.34,1,3.2,1.34,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1]
["080300000702109","08",45,1966,32.371430080000003,-99.195692989999998,"concrete bridge",1.87,0.79,4,2.35,0.99,2,2.42,1.02,1,1.87,0.79,4,2.35,0.99,2,2.42,1.02,1,2.35,0.99,2,2.56,1.08,1,2.56,1.08,1,2.35,0.99,2,2.56,1.08,1,2.56,1.08,1,2.12,0.89,3,2.2999999999999998,0.97,2,2.2999999999999998,0.97,2,2.12,0.89,3,2.2999999999999998,0.97,2,2.2999999999999998,0.97,2]
["081680000508093","08",100,1962,32.393027160000003,-100.90703333,"steel girder",1.56,0.72,4,1.49,0.69,5,1.47,0.68,5,1.38,0.64,5,1.47,0.68,5,1.47,0.68,5,1.76,0.82,3,1.7,0.79,4,1.69,0.78,4,1.63,0.76,4,1.7,0.79,4,1.69,0.78,4,1.58,0.73,4,1.53,0.71,4,1.52,0.7,5,1.46,0.67,5,1.53,0.71,4,1.52,0.7,5]
["081770000603315","08",60,2000,32.494564390000001,-100.29259351,"prestress concrete girder",2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1]
["090140001504398","09",80,1985,31.138996779999999,-97.330362280000003,"prestress concrete girder",1.63,0.69,5,1.63,0.69,5,1.68,0.71,4,1.63,0.69,5,1.63,0.69,5,1.68,0.71,4,1.91,0.81,3,1.93,0.82,3,2.0299999999999998,0.85,3,1.91,0.81,3,1.93,0.82,3,2.0299999999999998,0.85,3,1.71,0.72,4,1.73,0.73,4,1.82,0.77,4,1.71,0.72,4,1.73,0.73,4,1.82,0.77,4]
["091100001423286","09",50,1965,32.230299950000003,-97.153814620000006,"concrete bridge",1.75,0.74,4,2.04,0.86,3,2.37,0.99,2,1.75,0.74,4,2.04,0.86,3,2.37,0.99,2,2.2200000000000002,0.94,2,2.5299999999999998,1.06,1,2.77,1.1599999999999999,1,2.2200000000000002,0.94,2,2.5299999999999998,1.06,1,2.77,1.1599999999999999,1,1.99,0.84,3,2.2799999999999998,0.96,2,2.5,1.05,1,1.99,0.84,3,2.2799999999999998,0.96,2,2.5,1.05,1]
["091610001501376","09",85,1971,31.577225120000001,-97.112682169999999,"steel girder",1.38,0.8,4,1.35,0.78,4,1.38,0.8,4,1.35,0.78,4,1.35,0.78,4,1.38,0.8,4,1.59,0.92,2,1.59,0.92,2,1.64,0.95,2,1.59,0.92,2,1.59,0.92,2,1.64,0.95,2,1.43,0.83,3,1.42,0.82,3,1.47,0.85,3,1.42,0.82,3,1.42,0.82,3,1.47,0.85,3]
["102120049504060","10",50,1962,32.468606960000002,-95.400844699999993,"steel girder",1.43,0.83,3,1.66,0.96,2,1.93,1.1200000000000001,1,1.43,0.83,3,1.66,0.96,2,1.93,1.1200000000000001,1,1.81,1.04,1,2.06,1.19,1,2.2599999999999998,1.31,1,1.81,1.04,1,2.06,1.19,1,2.2599999999999998,1.31,1,1.62,0.94,2,1.86,1.07,1,2.04,1.18,1,1.62,0.94,2,1.86,1.07,1,2.04,1.18,1]
["110030017603090","11",150,1991,31.310510999999998,-94.725837999999996,"steel girder",1.65,0.95,2,1.81,1.04,1,1.97,1.1399999999999999,1,1.6,0.92,2,1.61,0.93,2,1.67,0.97,2,1.97,1.1399999999999999,1,2.16,1.24,1,2.34,1.35,1,1.77,1.02,1,1.83,1.06,1,1.95,1.1299999999999999,1,1.77,1.02,1,1.94,1.1200000000000001,1,2.1,1.22,1,1.59,0.92,2,1.65,0.95,2,1.75,1.01,1]
["121020002713049","12",100,2003,29.72357208,-95.490785310000007,"prestress concrete girder",2.0499999999999998,0.86,3,2.15,0.9,3,2.15,0.9,3,2.0499999999999998,0.86,3,2.15,0.9,3,2.15,0.9,3,2.46,1.04,1,2.58,1.0900000000000001,1,2.58,1.0900000000000001,1,2.46,1.04,1,2.58,1.0900000000000001,1,2.58,1.0900000000000001,1,2.2200000000000002,0.94,2,2.3199999999999998,0.98,2,2.3199999999999998,0.98,2,2.2200000000000002,0.94,2,2.3199999999999998,0.98,2,2.3199999999999998,0.98,2]
["121020002802283","12",130,2010,29.776781,-95.260741999999993,"prestress concrete girder",2.2599999999999998,1.92,1,2.54,2.16,1,2.69,2.29,1,2.2599999999999998,1.92,1,2.54,2.16,1,2.69,2.29,1,2.71,2.2999999999999998,1,2.96,2.52,1,3.19,2.71,1,2.71,2.2999999999999998,1,2.96,2.52,1,3.19,2.71,1,2.44,2.0699999999999998,1,2.66,2.2599999999999998,1,2.87,2.44,1,2.44,2.0699999999999998,1,2.66,2.2599999999999998,1,2.87,2.44,1]
["121020011005389","12",130,2016,30.092502769999999,-95.435277769999999,"prestress concrete girder",2.2599999999999998,2.2599999999999998,1,2.54,2.54,1,2.69,2.69,1,2.2599999999999998,2.2599999999999998,1,2.54,2.54,1,2.69,2.69,1,2.71,2.71,1,2.96,2.96,1,3.19,3.19,1,2.71,2.71,1,2.96,2.96,1,3.19,3.19,1,2.44,2.44,1,2.66,2.66,1,2.87,2.87,1,2.44,2.44,1,2.66,2.66,1,2.87,2.87,1]
["121020017707202","12",135,1997,29.952789809999999,-95.290431699999999,"prestress concrete special",1.71,0.72,0,1.92,0.81,0,2.06,0.87,0,1.71,0.72,0,1.92,0.81,0,2.06,0.87,0,2.04,0.86,0,2.2599999999999998,0.95,0,2.42,1.02,0,2.04,0.86,0,2.2599999999999998,0.95,0,2.42,1.02,0,1.83,0.77,0,2.0299999999999998,0.85,0,2.1800000000000002,0.92,0,1.83,0.77,0,2.0299999999999998,0.85,0,2.1800000000000002,0.92,0]
["121020027107343","12",130,2008,29.783737179999999,-95.486855340000005,"prestress concrete special",2.2599999999999998,1.92,0,2.54,2.16,0,2.69,2.29,0,2.2599999999999998,1.92,0,2.54,2.16,0,2.69,2.29,0,2.71,2.2999999999999998,0,2.96,2.52,0,3.19,2.71,0,2.71,2.2999999999999998,0,2.96,2.52,0,3.19,2.71,0,2.44,2.0699999999999998,0,2.66,2.2599999999999998,0,2.87,2.44,0,2.44,2.0699999999999998,0,2.66,2.2599999999999998,0,2.87,2.44,0]
["121020027114391","12",55,1972,29.809277999999999,-95.309027999999998,"prestress concrete girder",2.19,0.88,3,2.19,0.88,3,2.19,0.88,3,2.19,0.88,3,2.19,0.88,3,2.19,0.88,3,2.89,1.1599999999999999,1,2.89,1.1599999999999999,1,2.89,1.1599999999999999,1,2.89,1.1599999999999999,1,2.89,1.1599999999999999,1,2.89,1.1599999999999999,1,2.59,1.04,1,2.59,1.04,1,2.59,1.04,1,2.59,1.04,1,2.59,1.04,1,2.59,1.04,1]
["121020027117526","12",175,2002,29.726830970000002,-95.461400839999996,"steel girder",1.65,1.08,1,1.78,1.1599999999999999,1,1.92,1.26,1,1.57,1.03,1,1.77,1.1599999999999999,1,1.79,1.17,1,1.93,1.27,1,2.1,1.38,1,2.27,1.49,1,1.9,1.24,1,2.0099999999999998,1.32,1,2.04,1.33,1,1.73,1.1299999999999999,1,1.88,1.23,1,2.04,1.33,1,1.71,1.1200000000000001,1,1.81,1.18,1,1.83,1.2,1]
["121020050003212","12",55,1962,29.762033079999998,-95.37336415,"steel girder",2.0699999999999998,1.37,1,2.0699999999999998,1.37,1,2.0699999999999998,1.37,1,2.0699999999999998,1.37,1,2.0699999999999998,1.37,1,2.0699999999999998,1.37,1,2.73,1.81,1,2.73,1.81,1,2.73,1.81,1,2.73,1.81,1,2.73,1.81,1,2.73,1.81,1,2.44,1.61,1,2.44,1.61,1,2.44,1.61,1,2.44,1.61,1,2.44,1.61,1,2.44,1.61,1]
["121020050003420","12",60,1961,29.81419446,-95.375232740000001,"concrete bridge",1.55,0.46,5,1.73,0.52,5,2.04,0.61,5,1.55,0.46,5,1.73,0.52,5,2.04,0.61,5,1.98,0.59,5,2.2200000000000002,0.66,5,2.5299999999999998,0.75,4,1.98,0.59,5,2.2200000000000002,0.66,5,2.5299999999999998,0.75,4,1.77,0.53,5,1.99,0.59,5,2.27,0.67,5,1.77,0.53,5,1.99,0.59,5,2.27,0.67,5]
["121020050801205","12",80,1971,29.770209350000002,-95.352507700000004,"prestress concrete girder",2.29,0.92,2,2.29,0.92,2,2.29,0.92,2,2.29,0.92,2,2.29,0.92,2,2.29,0.92,2,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.52,1,2,2.52,1,2,2.52,1,2,2.52,1,2,2.52,1,2,2.52,1,2]
["122370027104282","12",75,1967,29.77721481,-95.901335270000004,"prestress concrete girder",2.2599999999999998,0.9,3,2.2599999999999998,0.9,3,2.2599999999999998,0.9,3,2.2599999999999998,0.9,3,2.2599999999999998,0.9,3,2.2599999999999998,0.9,3,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.5099999999999998,1,2,2.5099999999999998,1,2,2.5099999999999998,1,2,2.5099999999999998,1,2,2.5099999999999998,1,2,2.5099999999999998,1,2]
["130450027101433","13",65,1966,29.71385729,-96.482344420000004,"steel girder",1.25,0.57999999999999996,5,1.33,0.61,5,1.51,0.7,5,1.25,0.57999999999999996,5,1.33,0.61,5,1.51,0.7,5,1.54,0.71,4,1.68,0.77,4,1.93,0.89,3,1.54,0.71,4,1.68,0.77,4,1.93,0.89,3,1.38,0.64,5,1.51,0.7,5,1.73,0.8,4,1.38,0.64,5,1.51,0.7,5,1.73,0.8,4]
["141060001603229","14",55,2004,29.872995719999999,-97.934648019999997,"prestress concrete girder",2.31,0.97,2,2.31,0.97,2,2.31,0.97,2,2.31,0.97,2,2.31,0.97,2,2.31,0.97,2,3.05,1.28,1,3.05,1.28,1,3.05,1.28,1,3.05,1.28,1,3.05,1.28,1,3.05,1.28,1,2.73,1.1499999999999999,1,2.73,1.1499999999999999,1,2.73,1.1499999999999999,1,2.73,1.1499999999999999,1,2.73,1.1499999999999999,1,2.73,1.1499999999999999,1]
["142270001601452","14",95,2017,30.149597999999997,-97.792310000000001,"prestress concrete girder",2.4500000000000002,2.4500000000000002,1,2.52,2.52,1,2.52,2.52,1,2.4500000000000002,2.4500000000000002,1,2.52,2.52,1,2.52,2.52,1,2.98,2.98,1,3.04,3.04,1,3.04,3.04,1,2.98,2.98,1,3.04,3.04,1,3.04,3.04,1,2.68,2.68,1,2.73,2.73,1,2.73,2.73,1,2.68,2.68,1,2.73,2.73,1,2.73,2.73,1]
["142460001509501","14",120,2007,30.577113400000002,-97.693374719999994,"prestress concrete girder",2.33,2.33,1,2.5499999999999998,2.5499999999999998,1,2.66,2.66,1,2.33,2.33,1,2.5499999999999998,2.5499999999999998,1,2.66,2.66,1,2.77,2.77,1,3.01,3.01,1,3.14,3.14,1,2.77,2.77,1,3.01,3.01,1,3.14,3.14,1,2.4900000000000002,2.4900000000000002,1,2.71,2.71,1,2.82,2.82,1,2.4900000000000002,2.4900000000000002,1,2.71,2.71,1,2.82,2.82,1]
["150150001607155","15",95,1983,29.53327552,-98.389570770000006,"prestress concrete girder",2.1,0.88,3,2.16,0.91,2,2.16,0.91,2,2.1,0.88,3,2.16,0.91,2,2.16,0.91,2,2.5499999999999998,1.07,1,2.6,1.1000000000000001,1,2.6,1.1000000000000001,1,2.5499999999999998,1.07,1,2.6,1.1000000000000001,1,2.6,1.1000000000000001,1,2.2999999999999998,0.97,2,2.34,0.99,2,2.34,0.99,2,2.2999999999999998,0.97,2,2.34,0.99,2,2.34,0.99,2]
["150150001710380","15",115,2010,29.438879289999999,-98.45035661,"prestress concrete girder",2.38,2.02,1,2.56,2.1800000000000002,1,2.63,2.2400000000000002,1,2.38,2.02,1,2.56,2.1800000000000002,1,2.63,2.2400000000000002,1,2.8,2.38,1,3.05,2.59,1,3.12,2.65,1,2.8,2.38,1,3.05,2.59,1,3.12,2.65,1,2.52,2.14,1,2.75,2.34,1,2.8,2.38,1,2.52,2.14,1,2.75,2.34,1,2.8,2.38,1]
["150150007212207","15",110,1993,29.452972970000001,-98.515860630000006,"prestress concrete segmental",2.1,0,0,1.98,0,0,1.93,0,0,1.68,0,0,1.84,0,0,1.92,0,0,2.34,0,0,2.2400000000000002,0,0,2.1800000000000002,0,0,1.95,0,0,2.14,0,0,2.1800000000000002,0,0,2.11,0,0,2.0099999999999998,0,0,1.96,0,0,1.75,0,0,1.92,0,0,1.96,0,0]
["150150007308262","15",85,1988,29.427664929999999,-98.481807619999998,"prestress concrete girder",2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.39,1,2,2.39,1,2,2.39,1,2,2.39,1,2,2.39,1,2,2.39,1,2]
["150150052104376","15",125,2008,29.517914529999999,-98.470317989999998,"prestress concrete girder",2.29,1.95,1,2.54,2.16,1,2.69,2.29,1,2.2999999999999998,1.95,1,2.54,2.16,1,2.69,2.29,1,2.74,2.33,1,2.98,2.5299999999999998,1,3.17,2.69,1,2.74,2.33,1,2.98,2.5299999999999998,1,3.17,2.69,1,2.4700000000000002,2.1,1,2.68,2.2799999999999998,1,2.85,2.42,1,2.4700000000000002,2.1,1,2.68,2.2799999999999998,1,2.85,2.42,1]
["151310007205174","15",150,1971,29.969602819999999,-98.892619190000005,"steel girder",1.65,0.95,2,1.81,1.04,1,1.97,1.1399999999999999,1,1.6,0.92,2,1.61,0.93,2,1.67,0.97,2,1.97,1.1399999999999999,1,2.16,1.24,1,2.34,1.35,1,1.77,1.02,1,1.83,1.06,1,1.95,1.1299999999999999,1,1.77,1.02,1,1.94,1.1200000000000001,1,2.1,1.22,1,1.59,0.92,2,1.65,0.95,2,1.75,1.01,1]
["161490007401167","16",45,1976,28.370070689999999,-98.048773699999998,"prestress concrete girder",2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.4300000000000002,1.02,1,2.42,1.02,1,2.42,1.02,1,3.23,1.36,1,3.23,1.36,1,3.23,1.36,1,3.23,1.36,1,3.23,1.36,1,3.23,1.36,1,2.92,1.23,1,2.92,1.23,1,2.92,1.23,1,2.92,1.23,1,2.92,1.23,1,2.92,1.23,1]
["161780007406191","16",85,1991,27.86156064,-97.617240050000007,"prestress concrete girder",2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.39,1,2,2.39,1,2,2.39,1,2,2.39,1,2,2.39,1,2,2.39,1,2]
["162050037201019","16",55,1997,27.95805017,-97.575337169999997,"prestress concrete girder",2.31,0.86,3,2.31,0.86,3,2.31,0.86,3,2.31,0.86,3,2.31,0.86,3,2.31,0.86,3,3.05,1.1299999999999999,1,3.05,1.1299999999999999,1,3.05,1.1299999999999999,1,3.05,1.1299999999999999,1,3.05,1.1299999999999999,1,3.05,1.1299999999999999,1,2.73,1.01,1,2.73,1.01,1,2.73,1.01,1,2.73,1.01,1,2.73,1.01,1,2.73,1.01,1]
["170820067501188","17",90,1971,31.771802999999998,-96.221750999999998,"prestress concrete girder",2.35,0.94,2,2.36,0.94,2,2.36,0.94,2,2.35,0.94,2,2.36,0.94,2,2.36,0.94,2,2.85,1.1399999999999999,1,2.85,1.1399999999999999,1,2.85,1.1399999999999999,1,2.85,1.1399999999999999,1,2.85,1.1399999999999999,1,2.85,1.1399999999999999,1,2.56,1.02,1,2.56,1.02,1,2.56,1.02,1,2.56,1.02,1,2.56,1.02,1,2.56,1.02,1]
["180570000911205","18",75,1961,32.794507520000003,-96.722562429999996,"steel girder",1.29,0.74,4,1.31,0.76,4,1.38,0.8,4,1.29,0.74,4,1.31,0.76,4,1.38,0.8,4,1.53,0.89,3,1.58,0.92,2,1.7,0.98,2,1.53,0.89,3,1.58,0.92,2,1.7,0.98,2,1.37,0.79,4,1.41,0.82,3,1.52,0.88,3,1.37,0.79,4,1.41,0.82,3,1.52,0.88,3]
["180570000911460","18",195,2012,32.859660999999996,-96.549796999999998,"Multi Span Long","Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1]
["180570009202312","18",85,1995,32.559473169999997,-96.664382320000001,"prestress concrete girder",2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.39,1,2,2.39,1,2,2.39,1,2,2.39,1,2,2.39,1,2,2.39,1,2]
["180570044202013","18",60,1959,32.754237519999997,-96.809197479999995,"concrete bridge",1.55,0.57999999999999996,5,1.73,0.65,5,2.04,0.76,4,1.55,0.57999999999999996,5,1.73,0.65,5,2.04,0.76,4,1.98,0.74,4,2.2200000000000002,0.83,3,2.5299999999999998,0.94,2,1.98,0.74,4,2.2200000000000002,0.83,3,2.5299999999999998,0.94,2,1.77,0.66,5,1.99,0.74,4,2.27,0.84,3,1.77,0.66,5,1.99,0.74,4,2.27,0.84,3]
["180570106804322","18",105,2006,32.766699039999999,-96.902077030000001,"prestress concrete girder",2.41,2.0499999999999998,1,2.57,2.1800000000000002,1,2.57,2.1800000000000002,1,2.41,2.0499999999999998,1,2.57,2.1800000000000002,1,2.57,2.1800000000000002,1,2.87,2.44,1,3.07,2.61,1,3.07,2.61,1,2.87,2.44,1,3.07,2.61,1,3.07,2.61,1,2.58,2.19,1,2.76,2.35,1,2.76,2.35,1,2.58,2.19,1,2.76,2.35,1,2.76,2.35,1]
["180570237402417","18",100,1987,32.699883610000001,-96.624788809999998,"prestress concrete girder",2.0499999999999998,0.86,3,2.15,0.9,3,2.15,0.9,3,2.0499999999999998,0.86,3,2.15,0.9,3,2.15,0.9,3,2.46,1.04,1,2.58,1.0900000000000001,1,2.58,1.0900000000000001,1,2.46,1.04,1,2.58,1.0900000000000001,1,2.58,1.0900000000000001,1,2.2200000000000002,0.94,2,2.3199999999999998,0.98,2,2.3199999999999998,0.98,2,2.2200000000000002,0.94,2,2.3199999999999998,0.98,2,2.3199999999999998,0.98,2]
["180570237403150","18",65,1971,32.694416240000002,-96.637234120000002,"prestress concrete girder",2.21,0.88,3,2.21,0.88,3,2.21,0.88,3,2.21,0.88,3,2.21,0.88,3,2.21,0.88,3,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.52,1,2,2.52,1,2,2.52,1,2,2.52,1,2,2.52,1,2,2.52,1,2]
["180610019503133","18",100,1992,33.255742089999998,-97.17759839,"prestress concrete girder",2.0499999999999998,0.76,4,2.15,0.8,4,2.15,0.8,4,2.0499999999999998,0.76,4,2.15,0.8,4,2.15,0.8,4,2.46,0.92,2,2.58,0.96,2,2.58,0.96,2,2.46,0.92,2,2.58,0.96,2,2.58,0.96,2,2.2200000000000002,0.83,3,2.3199999999999998,0.86,3,2.3199999999999998,0.86,3,2.2200000000000002,0.83,3,2.3199999999999998,0.86,3,2.3199999999999998,0.86,3]
["180710004804492","18",95,2008,32.49746245,-96.822642439999996,"prestress concrete girder",2.4500000000000002,2.08,1,2.52,2.14,1,2.52,2.14,1,2.4500000000000002,2.08,1,2.52,2.14,1,2.52,2.14,1,2.98,2.5299999999999998,1,3.04,2.58,1,3.04,2.58,1,2.98,2.5299999999999998,1,3.04,2.58,1,3.04,2.58,1,2.68,2.2799999999999998,1,2.73,2.3199999999999998,1,2.73,2.3199999999999998,1,2.68,2.2799999999999998,1,2.73,2.3199999999999998,1,2.73,2.3199999999999998,1]
["181300049501164","18",95,1964,32.701412609999998,-96.275312850000006,"steel girder",1.49,0.69,5,1.44,0.67,5,1.43,0.66,5,1.38,0.64,5,1.44,0.67,5,1.43,0.66,5,1.7,0.79,4,1.66,0.77,4,1.66,0.77,4,1.61,0.74,4,1.66,0.77,4,1.66,0.77,4,1.53,0.71,4,1.49,0.69,5,1.49,0.69,5,1.45,0.67,5,1.49,0.69,5,1.49,0.69,5]
["191030020705023","19",80,1996,32.376605750000003,-94.4536236,"prestress concrete girder",2.19,0.92,2,2.19,0.92,2,2.19,0.92,2,2.2000000000000002,0.93,2,2.2000000000000002,0.93,2,2.2000000000000002,0.93,2,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1]
["210310003907216","21",70,1972,26.248472809999999,-97.727396249999998,"prestress concrete girder",2.23,0.89,3,2.23,0.89,3,2.23,0.89,3,2.23,0.89,3,2.23,0.89,3,2.23,0.89,3,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.5099999999999998,1,2,2.5099999999999998,1,2,2.5099999999999998,1,2,2.5099999999999998,1,2,2.5099999999999998,1,2,2.5099999999999998,1,2]
["210310003916386","21",135,2005,25.94904889,-97.504709259999998,"prestress concrete girder",2.23,1.9,1,2.4900000000000002,2.12,1,2.68,2.2799999999999998,1,2.23,1.9,1,2.4900000000000002,2.12,1,2.68,2.2799999999999998,1,2.65,2.25,1,2.94,2.5,1,3.15,2.68,1,2.65,2.25,1,2.94,2.5,1,3.15,2.68,1,2.39,2.0299999999999998,1,2.65,2.25,1,2.84,2.41,1,2.39,2.0299999999999998,1,2.65,2.25,1,2.84,2.41,1]
["211090003917107","21",65,1993,26.206083469999999,-98.194263809999995,"prestress concrete girder",2.25,0.94,2,2.25,0.94,2,2.25,0.94,2,2.25,0.94,2,2.25,0.94,2,2.25,0.94,2,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.56,1.08,1,2.56,1.08,1,2.56,1.08,1,2.56,1.08,1,2.56,1.08,1,2.56,1.08,1]
["211090003918351","21",135,2005,26.16121785,-97.958122540000005,"prestress concrete girder",2.23,1.9,1,2.4900000000000002,2.12,1,2.68,2.2799999999999998,1,2.23,1.9,1,2.4900000000000002,2.12,1,2.68,2.2799999999999998,1,2.65,2.25,1,2.94,2.5,1,3.15,2.68,1,2.65,2.25,1,2.94,2.5,1,3.15,2.68,1,2.39,2.0299999999999998,1,2.65,2.25,1,2.84,2.41,1,2.39,2.0299999999999998,1,2.65,2.25,1,2.84,2.41,1]
["221420001708243","22",100,1971,28.450746559999999,-99.237640099999993,"prestress concrete girder",2.3199999999999998,0.93,2,2.4300000000000002,0.97,2,2.4300000000000002,0.97,2,2.3199999999999998,0.93,2,2.4300000000000002,0.97,2,2.4300000000000002,0.97,2,2.78,1.1100000000000001,1,2.91,1.1599999999999999,1,2.91,1.1599999999999999,1,2.78,1.1100000000000001,1,2.91,1.1599999999999999,1,2.91,1.1599999999999999,1,2.5099999999999998,1,2,2.62,1.05,1,2.62,1.05,1,2.5099999999999998,1,2,2.62,1.05,1,2.62,1.05,1]
["222400001803159","22",50,1983,27.951937170000001,-99.381423560000002,"prestress concrete girder",2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,3.2,1.34,1,3.2,1.34,1,3.2,1.34,1,3.2,1.34,1,3.2,1.34,1,3.2,1.34,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1]
["240720016701059","24",90,1970,31.769308800000001,-106.45067638,"steel girder",1.43,0.83,3,1.39,0.8,4,1.4,0.81,3,1.36,0.79,4,1.39,0.8,4,1.4,0.81,3,1.64,0.95,2,1.62,0.94,2,1.64,0.95,2,1.61,0.93,2,1.62,0.94,2,1.64,0.95,2,1.47,0.85,3,1.45,0.84,3,1.47,0.85,3,1.45,0.84,3,1.45,0.84,3,1.47,0.85,3]
["240720212103242","24",85,1990,31.781392570000001,-106.40731289999999,"prestress concrete girder",2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.66,0.99,2,2.66,0.99,2,2.66,0.99,2,2.66,0.99,2,2.66,0.99,2,2.66,0.99,2,2.39,0.89,3,2.39,0.89,3,2.39,0.89,3,2.39,0.89,3,2.39,0.89,3,2.39,0.89,3]
["010920004718230","01",60,1981,33.650151989999998,-96.611533780000002,"prestress concrete girder",2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1]
["021840000803316","02",140,1986,32.720660160000001,-97.570113689999999,"steel girder",1.67,0.77,4,1.84,0.85,3,1.96,0.91,2,1.52,0.7,5,1.57,0.73,4,1.66,0.77,4,2,0.92,2,2.2000000000000002,1.01,1,2.1800000000000002,1.01,1,1.69,0.78,4,1.79,0.83,3,1.94,0.89,3,1.8,0.83,3,1.98,0.91,2,1.96,0.91,2,1.52,0.7,5,1.61,0.74,4,1.75,0.81,3]
["022200000813313","02",80,1963,32.808993999999998,-97.210763,"steel girder",1.33,0.77,4,1.33,0.77,4,1.37,0.79,4,1.33,0.77,4,1.33,0.77,4,1.37,0.79,4,1.55,0.89,3,1.57,0.91,2,1.65,0.95,2,1.55,0.89,3,1.57,0.91,2,1.65,0.95,2,1.39,0.8,4,1.41,0.82,3,1.48,0.86,3,1.39,0.8,4,1.41,0.82,3,1.48,0.86,3]
["022200000816478","02",125,2014,32.68309,-97.411670000000001,"prestress concrete girder",2.29,1.72,1,2.54,1.91,1,2.69,2.02,1,2.2999999999999998,1.72,1,2.54,1.91,1,2.69,2.02,1,2.74,2.06,1,2.98,2.2400000000000002,1,3.17,2.38,1,2.74,2.06,1,2.98,2.2400000000000002,1,3.17,2.38,1,2.4700000000000002,1.85,1,2.68,2.0099999999999998,1,2.85,2.14,1,2.4700000000000002,1.85,1,2.68,2.0099999999999998,1,2.85,2.14,1]
["022200001416438","02",80,1990,32.665001369999999,-97.320731859999995,"prestress concrete girder",2.19,0.92,2,2.19,0.92,2,2.19,0.92,2,2.2000000000000002,0.93,2,2.2000000000000002,0.93,2,2.2000000000000002,0.93,2,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1]
["022200008112078","02",65,1967,32.972294750000003,-97.309024730000004,"prestress concrete girder",2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3]
["022200106801454","02",115,2001,32.744624020000003,-97.331888509999999,"prestress concrete girder",1.93,0.72,4,2.08,0.77,4,2.13,0.79,4,1.93,0.72,4,2.08,0.77,4,2.13,0.79,4,2.27,0.84,3,2.4700000000000002,0.92,2,2.5299999999999998,0.94,2,2.27,0.84,3,2.4700000000000002,0.92,2,2.5299999999999998,0.94,2,2.04,0.76,4,2.23,0.83,3,2.27,0.84,3,2.04,0.76,4,2.23,0.83,3,2.27,0.84,3]
["022200106802370","02",85,1997,32.74660944,-97.306589239999994,"prestress concrete girder",2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.39,1,2,2.39,1,2,2.39,1,2,2.39,1,2,2.39,1,2,2.39,1,2]
["022490001307065","02",60,1981,33.349137329999998,-97.692332280000002,"prestress concrete girder",2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1]
["032430004309188","03",80,2001,33.909327920000003,-98.5014982,"steel girder",1.33,0.87,3,1.33,0.87,3,1.37,0.89,3,1.33,0.87,3,1.33,0.87,3,1.37,0.89,3,1.55,1.01,1,1.57,1.03,1,1.65,1.08,1,1.55,1.01,1,1.57,1.03,1,1.65,1.08,1,1.39,0.91,2,1.41,0.93,2,1.48,0.97,2,1.39,0.91,2,1.41,0.93,2,1.48,0.97,2]
["032430015607055","03",45,1964,34.055729229999997,-98.556951659999996,"prestress concrete girder",2.2200000000000002,0.78,4,2.2200000000000002,0.78,4,2.2200000000000002,0.78,4,2.23,0.79,4,2.2200000000000002,0.78,4,2.2200000000000002,0.78,4,2.96,1.04,1,2.96,1.04,1,2.96,1.04,1,2.96,1.04,1,2.96,1.04,1,2.96,1.04,1,2.68,0.95,2,2.68,0.95,2,2.68,0.95,2,2.68,0.95,2,2.68,0.95,2,2.68,0.95,2]
["040910027505126","04",85,1978,35.198414049999997,-101.08505629,"prestress concrete girder",2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.66,0.99,2,2.66,0.99,2,2.66,0.99,2,2.66,0.99,2,2.66,0.99,2,2.66,0.99,2,2.39,0.89,3,2.39,0.89,3,2.39,0.89,3,2.39,0.89,3,2.39,0.89,3,2.39,0.89,3]
["041880009005065","04",80,1972,35.19131745,-102.06387049999999,"prestress concrete girder",2.29,0.65,5,2.29,0.65,5,2.29,0.65,5,2.29,0.65,5,2.29,0.65,5,2.29,0.65,5,2.81,0.79,4,2.81,0.79,4,2.81,0.79,4,2.81,0.79,4,2.81,0.79,4,2.81,0.79,4,2.52,0.71,4,2.52,0.71,4,2.52,0.71,4,2.52,0.71,4,2.52,0.71,4,2.52,0.71,4]
["051520005318077","05",110,1986,33.529731150000003,-101.81892248,"steel girder",1.71,0.99,2,1.62,0.94,2,1.57,0.91,2,1.37,0.79,4,1.5,0.87,3,1.56,0.9,3,1.91,1.1000000000000001,1,1.82,1.05,1,1.78,1.03,1,1.59,0.92,2,1.74,1.01,1,1.78,1.03,1,1.72,0.99,2,1.64,0.95,2,1.6,0.92,2,1.43,0.83,3,1.57,0.91,2,1.6,0.92,2]
["051850016802073","05",60,1993,34.529749789999997,-102.87807662,"prestress concrete girder",2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1]
["060690000513172","06",80,1966,31.829524769999999,-102.34973836,"steel girder",1.33,0.77,4,1.33,0.77,4,1.37,0.79,4,1.33,0.77,4,1.33,0.77,4,1.37,0.79,4,1.55,0.89,3,1.57,0.91,2,1.65,0.95,2,1.55,0.89,3,1.57,0.91,2,1.65,0.95,2,1.39,0.8,4,1.41,0.82,3,1.48,0.86,3,1.39,0.8,4,1.41,0.82,3,1.48,0.86,3]
["062380000404029","06",50,1964,31.560752099999998,-102.99702116,"prestress concrete girder",2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.99,1.06,1,2.99,1.06,1,2.99,1.06,1,2.99,1.06,1,2.99,1.06,1,2.99,1.06,1,2.67,0.94,2,2.67,0.94,2,2.67,0.94,2,2.67,0.94,2,2.67,0.94,2,2.67,0.94,2]
["072180014102070","07",60,1969,30.62608552,-100.84998399,"prestress concrete girder",2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.84,1.1299999999999999,1,2.84,1.1299999999999999,1,2.84,1.1299999999999999,1,2.84,1.1299999999999999,1,2.84,1.1299999999999999,1,2.84,1.1299999999999999,1,2.5499999999999998,1.02,1,2.5499999999999998,1.02,1,2.5499999999999998,1.02,1,2.5499999999999998,1.02,1,2.5499999999999998,1.02,1,2.5499999999999998,1.02,1]
["080300000701091","08",70,1965,32.403349669999997,-99.407006170000002,"concrete bridge",1.54,0.56999999999999995,5,1.6,0.59,5,1.75,0.65,5,1.54,0.56999999999999995,5,1.61,0.6,5,1.75,0.65,5,1.87,0.7,5,1.97,0.74,4,2.2000000000000002,0.82,3,1.87,0.7,5,1.97,0.74,4,2.2000000000000002,0.82,3,1.67,0.62,5,1.77,0.66,5,1.97,0.74,4,1.67,0.62,5,1.77,0.66,5,1.97,0.74,4]
["081680000508055","08",45,1957,32.385594580000003,-100.96094499,"concrete bridge",1.87,0.7,5,2.35,0.87,3,2.42,0.9,3,1.87,0.7,5,2.35,0.87,3,2.42,0.9,3,2.35,0.87,3,2.56,0.95,2,2.56,0.95,2,2.35,0.87,3,2.56,0.95,2,2.56,0.95,2,2.12,0.79,4,2.2999999999999998,0.86,3,2.2999999999999998,0.86,3,2.12,0.79,4,2.2999999999999998,0.86,3,2.2999999999999998,0.86,3]
["082210000604105","08",45,1958,32.49326928,-100.12000971000001,"concrete bridge",1.87,0.7,5,2.35,0.87,3,2.42,0.9,3,1.87,0.7,5,2.35,0.87,3,2.42,0.9,3,2.35,0.87,3,2.56,0.95,2,2.56,0.95,2,2.35,0.87,3,2.56,0.95,2,2.56,0.95,2,2.12,0.79,4,2.2999999999999998,0.86,3,2.2999999999999998,0.86,3,2.12,0.79,4,2.2999999999999998,0.86,3,2.2999999999999998,0.86,3]
["090140001507394","09",115,2009,30.888058440000002,-97.57327085,"prestress concrete special",2.38,2.02,0,2.56,2.1800000000000002,0,2.63,2.2400000000000002,0,2.38,2.02,0,2.56,2.1800000000000002,0,2.63,2.2400000000000002,0,2.8,2.38,0,3.05,2.59,0,3.12,2.65,0,2.8,2.38,0,3.05,2.59,0,3.12,2.65,0,2.52,2.14,0,2.75,2.34,0,2.8,2.38,0,2.52,2.14,0,2.75,2.34,0,2.8,2.38,0]
["091610001408523","09",135,2015,31.818870999999998,-97.097661000000002,"prestress concrete girder",2.23,1.9,1,2.4900000000000002,2.12,1,2.68,2.2799999999999998,1,2.23,1.9,1,2.4900000000000002,2.12,1,2.68,2.2799999999999998,1,2.65,2.25,1,2.94,2.5,1,3.15,2.68,1,2.65,2.25,1,2.94,2.5,1,3.15,2.68,1,2.39,2.0299999999999998,1,2.65,2.25,1,2.84,2.41,1,2.39,2.0299999999999998,1,2.65,2.25,1,2.84,2.41,1]
["091610001409512","09",125,2013,31.687700000000003,-97.099629999999991,"prestress concrete special",2.29,2.29,0,2.54,2.54,0,2.69,2.69,0,2.2999999999999998,2.2999999999999998,0,2.54,2.54,0,2.69,2.69,0,2.74,2.74,0,2.98,2.98,0,3.17,3.17,0,2.74,2.74,0,2.98,2.98,0,3.17,3.17,0,2.4700000000000002,2.4700000000000002,0,2.68,2.68,0,2.85,2.85,0,2.4700000000000002,2.4700000000000002,0,2.68,2.68,0,2.85,2.85,0]
["100930049507276","10",90,1967,32.434353860000002,-94.828747660000005,"steel girder",1.43,0.94,2,1.39,0.91,2,1.4,0.92,2,1.36,0.89,3,1.39,0.91,2,1.4,0.92,2,1.64,1.07,1,1.62,1.06,1,1.64,1.07,1,1.61,1.05,1,1.62,1.06,1,1.64,1.07,1,1.47,0.96,2,1.45,0.95,2,1.47,0.96,2,1.45,0.95,2,1.45,0.95,2,1.47,0.96,2]
["111870017701237","11",125,2001,30.572085099999999,-94.949408680000005,"prestress concrete girder",1.81,0.77,4,2,0.84,3,2.12,0.89,3,1.81,0.77,4,2,0.84,3,2.12,0.89,3,2.16,0.91,2,2.35,0.99,2,2.5,1.05,1,2.16,0.91,2,2.35,0.99,2,2.5,1.05,1,1.95,0.82,3,2.12,0.89,3,2.25,0.94,2,1.95,0.82,3,2.12,0.89,3,2.25,0.94,2]
["120850050001194","12",65,1976,29.288317129999999,-94.837814039999998,"prestress concrete girder",2.25,0.94,2,2.25,0.94,2,2.25,0.94,2,2.25,0.94,2,2.25,0.94,2,2.25,0.94,2,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.56,1.08,1,2.56,1.08,1,2.56,1.08,1,2.56,1.08,1,2.56,1.08,1,2.56,1.08,1]
["121020005006159","12",130,2004,30.010145219999998,-95.798812690000005,"prestress concrete girder",1.76,0.74,4,1.97,0.83,3,2.1,0.88,3,1.76,0.74,4,1.97,0.83,3,2.1,0.88,3,2.11,0.88,3,2.2999999999999998,0.97,2,2.48,1.05,1,2.11,0.88,3,2.2999999999999998,0.97,2,2.48,1.05,1,1.9,0.8,4,2.0699999999999998,0.87,3,2.23,0.94,2,1.9,0.8,4,2.0699999999999998,0.87,3,2.23,0.94,2]
["121020005009494","12",135,2016,29.86691982,-95.540422629999995,"prestress concrete special",2.23,1.9,0,2.4900000000000002,2.12,0,2.68,2.2799999999999998,0,2.23,1.9,0,2.4900000000000002,2.12,0,2.68,2.2799999999999998,0,2.65,2.25,0,2.94,2.5,0,3.15,2.68,0,2.65,2.25,0,2.94,2.5,0,3.15,2.68,0,2.39,2.0299999999999998,0,2.65,2.25,0,2.84,2.41,0,2.39,2.0299999999999998,0,2.65,2.25,0,2.84,2.41,0]
["121020017707205","12",125,1997,29.966113249999999,-95.284523849999999,"prestress concrete special",1.81,0.77,0,2,0.84,0,2.12,0.89,0,1.81,0.77,0,2,0.84,0,2.12,0.89,0,2.16,0.91,0,2.35,0.99,0,2.5,1.05,0,2.16,0.91,0,2.35,0.99,0,2.5,1.05,0,1.95,0.82,0,2.12,0.89,0,2.25,0.94,0,1.95,0.82,0,2.12,0.89,0,2.25,0.94,0]
["121020017711171","12",110,1995,29.851218410000001,-95.333649109999996,"prestress concrete special",1.97,0.74,0,2.12,0.79,0,2.14,0.8,0,1.97,0.74,0,2.12,0.79,0,2.14,0.8,0,2.3199999999999998,0.86,0,2.54,0.95,0,2.54,0.95,0,2.3199999999999998,0.86,0,2.54,0.95,0,2.54,0.95,0,2.09,0.77,0,2.2799999999999998,0.85,0,2.2799999999999998,0.85,0,2.09,0.77,0,2.2799999999999998,0.85,0,2.2799999999999998,0.85,0]
["121020027107069","12",130,2008,29.784662310000002,-95.498293680000003,"prestress concrete special",2.2599999999999998,1.92,0,2.54,2.16,0,2.69,2.29,0,2.2599999999999998,1.92,0,2.54,2.16,0,2.69,2.29,0,2.71,2.2999999999999998,0,2.96,2.52,0,3.19,2.71,0,2.71,2.2999999999999998,0,2.96,2.52,0,3.19,2.71,0,2.44,2.0699999999999998,0,2.66,2.2599999999999998,0,2.87,2.44,0,2.44,2.0699999999999998,0,2.66,2.2599999999999998,0,2.87,2.44,0]
["121020027114671","12",280,2014,29.804216669999999,-95.447816669999995,"Multi Span Long","Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1]
["121020050003271","12",100,1985,29.699655509999999,-95.291918050000007,"prestress concrete girder",2.0499999999999998,0.76,4,2.15,0.8,4,2.15,0.8,4,2.0499999999999998,0.76,4,2.15,0.8,4,2.15,0.8,4,2.46,0.92,2,2.58,0.96,2,2.58,0.96,2,2.46,0.92,2,2.58,0.96,2,2.58,0.96,2,2.2200000000000002,0.83,3,2.3199999999999998,0.86,3,2.3199999999999998,0.86,3,2.2200000000000002,0.83,3,2.3199999999999998,0.86,3,2.3199999999999998,0.86,3]
["121020050003311","12",125,1998,29.611211740000002,-95.210316120000002,"steel weathered girder",1.72,1.1200000000000001,1,1.84,1.21,1,1.75,1.1499999999999999,1,1.42,0.93,2,1.53,1,2,1.63,1.07,1,2.0699999999999998,1.35,1,2.04,1.33,1,1.96,1.28,1,1.61,1.05,1,1.77,1.1599999999999999,1,1.88,1.23,1,1.86,1.22,1,1.83,1.2,1,1.76,1.1599999999999999,1,1.45,0.95,2,1.6,1.05,1,1.69,1.1100000000000001,1]
["121020050801334","12",100,2001,29.804886549999999,-94.981225030000004,"prestress concrete girder",2.0499999999999998,0.76,4,2.15,0.8,4,2.15,0.8,4,2.0499999999999998,0.76,4,2.15,0.8,4,2.15,0.8,4,2.46,0.92,2,2.58,0.96,2,2.58,0.96,2,2.46,0.92,2,2.58,0.96,2,2.58,0.96,2,2.2200000000000002,0.83,3,2.3199999999999998,0.86,3,2.3199999999999998,0.86,3,2.2200000000000002,0.83,3,2.3199999999999998,0.86,3,2.3199999999999998,0.86,3]
["121020351005048","12",120,2012,29.779807340000001,-95.776974010000004,"prestress concrete special",2.33,1.98,0,2.5499999999999998,2.17,0,2.66,2.2599999999999998,0,2.33,1.98,0,2.5499999999999998,2.17,0,2.66,2.2599999999999998,0,2.77,2.35,0,3.01,2.56,0,3.14,2.67,0,2.77,2.35,0,3.01,2.56,0,3.14,2.67,0,2.4900000000000002,2.12,0,2.71,2.2999999999999998,0,2.82,2.4,0,2.4900000000000002,2.12,0,2.71,2.2999999999999998,0,2.82,2.4,0]
["130080027103242","13",45,1967,29.773163480000001,-96.133964300000002,"concrete bridge",2.4,0.85,3,2.4,0.85,3,2.4,0.85,3,2.41,0.85,3,2.4,0.85,3,2.4,0.85,3,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1]
["131210008903107","13",90,1972,28.969267850000001,-96.670583160000007,"prestress concrete girder",2.35,0.66,5,2.36,0.67,5,2.36,0.67,5,2.35,0.66,5,2.36,0.67,5,2.36,0.67,5,2.85,0.8,4,2.85,0.8,4,2.85,0.8,4,2.85,0.8,4,2.85,0.8,4,2.85,0.8,4,2.56,0.72,4,2.56,0.72,4,2.56,0.72,4,2.56,0.72,4,2.56,0.72,4,2.56,0.72,4]
["132410008907125","13",85,1972,29.281635640000001,-96.134392009999999,"prestress concrete girder",2.3199999999999998,0.93,2,2.3199999999999998,0.93,2,2.3199999999999998,0.93,2,2.3199999999999998,0.93,2,2.3199999999999998,0.93,2,2.3199999999999998,0.93,2,2.83,1.1299999999999999,1,2.83,1.1299999999999999,1,2.83,1.1299999999999999,1,2.83,1.1299999999999999,1,2.83,1.1299999999999999,1,2.83,1.1299999999999999,1,2.54,1.01,1,2.54,1.01,1,2.54,1.01,1,2.54,1.01,1,2.54,1.01,1,2.54,1.01,1]
["142270001513462","14",115,2005,30.215858399999998,-97.749125469999996,"prestress concrete special",2.38,2.02,0,2.56,2.1800000000000002,0,2.63,2.2400000000000002,0,2.38,2.02,0,2.56,2.1800000000000002,0,2.63,2.2400000000000002,0,2.8,2.38,0,3.05,2.59,0,3.12,2.65,0,2.8,2.38,0,3.05,2.59,0,3.12,2.65,0,2.52,2.14,0,2.75,2.34,0,2.8,2.38,0,2.52,2.14,0,2.75,2.34,0,2.8,2.38,0]
["150150001710098","15",75,1989,29.439826490000002,-98.4820007,"steel girder",1.29,0.74,4,1.31,0.76,4,1.38,0.8,4,1.29,0.74,4,1.31,0.76,4,1.38,0.8,4,1.53,0.89,3,1.58,0.92,2,1.7,0.98,2,1.53,0.89,3,1.58,0.92,2,1.7,0.98,2,1.37,0.79,4,1.41,0.82,3,1.52,0.88,3,1.37,0.79,4,1.41,0.82,3,1.52,0.88,3]
["150150001710156","15",75,1962,29.44011063,-98.44157869,"steel girder",1.29,0.74,4,1.31,0.76,4,1.38,0.8,4,1.29,0.74,4,1.31,0.76,4,1.38,0.8,4,1.53,0.89,3,1.58,0.92,2,1.7,0.98,2,1.53,0.89,3,1.58,0.92,2,1.7,0.98,2,1.37,0.79,4,1.41,0.82,3,1.52,0.88,3,1.37,0.79,4,1.41,0.82,3,1.52,0.88,3]
["150150002502105","15",50,1962,29.458522819999999,-98.317585219999998,"prestress concrete girder",2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.99,1.06,1,2.99,1.06,1,2.99,1.06,1,2.99,1.06,1,2.99,1.06,1,2.99,1.06,1,2.67,0.94,2,2.67,0.94,2,2.67,0.94,2,2.67,0.94,2,2.67,0.94,2,2.67,0.94,2]
["150150007212343","15",100,1991,29.42874389,-98.500608490000005,"prestress concrete segmental",1.91,0,0,1.83,0,0,1.8,0,0,1.69,0,0,1.8,0,0,1.8,0,0,2.16,0,0,2.09,0,0,2.08,0,0,2,0,0,2.08,0,0,2.08,0,0,1.94,0,0,1.88,0,0,1.87,0,0,1.8,0,0,1.87,0,0,1.87,0,0]
["150150007308177","15",100,2009,29.315782250000002,-98.406311180000003,"steel girder",1.96,1.47,1,1.93,1.45,1,1.9,1.42,1,1.78,1.34,1,1.89,1.42,1,1.9,1.42,1,2.2799999999999998,1.71,1,2.2000000000000002,1.65,1,2.19,1.64,1,2.11,1.58,1,2.2000000000000002,1.65,1,2.19,1.64,1,2.0499999999999998,1.54,1,1.98,1.48,1,1.96,1.47,1,1.89,1.42,1,1.97,1.48,1,1.96,1.47,1]
["150150052104290","15",100,2008,29.48246786,-98.600265930000006,"prestress concrete special",2.4300000000000002,2.0699999999999998,0,2.5499999999999998,2.17,0,2.5499999999999998,2.17,0,2.4300000000000002,2.0699999999999998,0,2.5499999999999998,2.17,0,2.5499999999999998,2.17,0,2.91,2.4700000000000002,0,3.05,2.59,0,3.05,2.59,0,2.91,2.4700000000000002,0,3.05,2.59,0,3.05,2.59,0,2.62,2.23,0,2.74,2.33,0,2.74,2.33,0,2.62,2.23,0,2.74,2.33,0,2.74,2.33,0]
["150150052106107","15",60,1981,29.452168,-98.406112999999991,"steel girder",1.27,0.74,4,1.41,0.82,3,1.66,0.96,2,1.27,0.74,4,1.41,0.82,3,1.66,0.96,2,1.61,0.93,2,1.81,1.04,1,2.06,1.19,1,1.61,0.93,2,1.81,1.04,1,2.06,1.19,1,1.44,0.83,3,1.62,0.94,2,1.85,1.07,1,1.44,0.83,3,1.62,0.94,2,1.85,1.07,1]
["150830001706221","15",50,1968,29.054475350000001,-99.012376979999999,"steel girder",1.43,0.94,2,1.66,1.0900000000000001,1,1.93,1.27,1,1.43,0.94,2,1.66,1.0900000000000001,1,1.93,1.27,1,1.81,1.18,1,2.06,1.35,1,2.2599999999999998,1.48,1,1.81,1.18,1,2.06,1.35,1,2.2599999999999998,1.48,1,1.62,1.06,1,1.86,1.22,1,2.04,1.33,1,1.62,1.06,1,1.86,1.22,1,2.04,1.33,1]
["160130010101055","16",45,1976,28.314085160000001,-97.702605739999996,"prestress concrete girder",2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.4300000000000002,1.02,1,2.42,1.02,1,2.42,1.02,1,3.23,1.36,1,3.23,1.36,1,3.23,1.36,1,3.23,1.36,1,3.23,1.36,1,3.23,1.36,1,2.92,1.23,1,2.92,1.23,1,2.92,1.23,1,2.92,1.23,1,2.92,1.23,1,2.92,1.23,1]
["161490007402145","16",50,1975,28.34393493,-98.031446259999996,"prestress concrete girder",2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,3.2,1.34,1,3.2,1.34,1,3.2,1.34,1,3.2,1.34,1,3.2,1.34,1,3.2,1.34,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1]
["171540067505104","17",65,1965,31.092481240000001,-95.961089189999996,"concrete bridge",1.53,0.56999999999999995,5,1.64,0.61,5,1.86,0.69,5,1.53,0.56999999999999995,5,1.64,0.61,5,1.86,0.69,5,1.9,0.71,4,2.0699999999999998,0.77,4,2.37,0.88,3,1.9,0.71,4,2.0699999999999998,0.77,4,2.37,0.88,3,1.7,0.63,5,1.85,0.69,5,2.12,0.79,4,1.7,0.63,5,1.85,0.69,5,2.13,0.79,4]
["180430004714607","18",120,2010,33.217095190000002,-96.636380250000002,"prestress concrete girder",2.33,1.98,1,2.5499999999999998,2.17,1,2.66,2.2599999999999998,1,2.33,1.98,1,2.5499999999999998,2.17,1,2.66,2.2599999999999998,1,2.77,2.35,1,3.01,2.56,1,3.14,2.67,1,2.77,2.35,1,3.01,2.56,1,3.14,2.67,1,2.4900000000000002,2.12,1,2.71,2.2999999999999998,1,2.82,2.4,1,2.4900000000000002,2.12,1,2.71,2.2999999999999998,1,2.82,2.4,1]
["180570000911388","18",75,1961,32.794898490000001,-96.722347290000002,"steel girder",1.29,0.74,4,1.31,0.76,4,1.38,0.8,4,1.29,0.74,4,1.31,0.76,4,1.38,0.8,4,1.53,0.89,3,1.58,0.92,2,1.7,0.98,2,1.53,0.89,3,1.58,0.92,2,1.7,0.98,2,1.37,0.79,4,1.41,0.82,3,1.52,0.88,3,1.37,0.79,4,1.41,0.82,3,1.52,0.88,3]
["180570004707365","18",145,1998,32.864082459999999,-96.771036839999994,"prestress concrete girder",2.04,0.76,4,2.2400000000000002,0.83,3,2.44,0.91,2,1.92,0.71,4,1.95,0.73,4,2.04,0.76,4,2.44,0.91,2,2.68,1,2,2.77,1.03,1,2.12,0.79,4,2.2200000000000002,0.83,3,2.39,0.89,3,2.19,0.81,3,2.4,0.89,3,2.4900000000000002,0.92,2,1.91,0.71,4,2,0.74,4,2.15,0.8,4]
["180570009513392","18",75,1987,32.70192763,-96.623089919999998,"prestress concrete girder",2.21,0.93,2,2.21,0.93,2,2.21,0.93,2,2.21,0.93,2,2.21,0.93,2,2.21,0.93,2,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.46,1.04,1,2.46,1.04,1,2.46,1.04,1,2.46,1.04,1,2.46,1.04,1,2.46,1.04,1]
["180570019603473","18",315,2014,32.868938,-96.898895999999993,"Multi Span Long","Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1]
["180570237401522","18",135,2013,32.925511,-96.803641999999996,"prestress concrete girder",2.23,1.9,1,2.4900000000000002,2.12,1,2.68,2.2799999999999998,1,2.23,1.9,1,2.4900000000000002,2.12,1,2.68,2.2799999999999998,1,2.65,2.25,1,2.94,2.5,1,3.15,2.68,1,2.65,2.25,1,2.94,2.5,1,3.15,2.68,1,2.39,2.0299999999999998,1,2.65,2.25,1,2.84,2.41,1,2.39,2.0299999999999998,1,2.65,2.25,1,2.84,2.41,1]
["180570237401555","18",65,2013,32.923930999999996,-96.782167000000001,"prestress concrete girder",2.4,2.04,1,2.4,2.04,1,2.4,2.04,1,2.4,2.04,1,2.4,2.04,1,2.4,2.04,1,3.05,2.59,1,3.05,2.59,1,3.05,2.59,1,3.05,2.59,1,3.05,2.59,1,3.05,2.59,1,2.74,2.33,1,2.74,2.33,1,2.74,2.33,1,2.74,2.33,1,2.74,2.33,1,2.74,2.33,1]
["180570237407346","18",125,1992,32.945774,-97.021968999999999,"prestress concrete girder",1.81,0.68,5,2,0.74,4,2.12,0.79,4,1.81,0.68,5,2,0.74,4,2.12,0.79,4,2.16,0.8,4,2.35,0.87,3,2.5,0.93,2,2.16,0.8,4,2.35,0.87,3,2.5,0.93,2,1.95,0.73,4,2.12,0.79,4,2.25,0.83,3,1.95,0.73,4,2.12,0.79,4,2.25,0.83,3]
["180610019502074","18",70,1989,33.314657400000002,-97.179652160000003,"steel girder",1.26,0.73,4,1.31,0.76,4,1.43,0.83,3,1.26,0.73,4,1.31,0.76,4,1.43,0.83,3,1.52,0.88,3,1.61,0.93,2,1.79,1.04,1,1.52,0.88,3,1.61,0.93,2,1.79,1.04,1,1.36,0.79,4,1.44,0.83,3,1.61,0.93,2,1.36,0.79,4,1.44,0.83,3,1.61,0.93,2]
["180610036403129","18",130,2009,33.071514380000004,-96.876640980000005,"prestress concrete girder",2.2599999999999998,1.92,1,2.54,2.16,1,2.69,2.29,1,2.2599999999999998,1.92,1,2.54,2.16,1,2.69,2.29,1,2.71,2.2999999999999998,1,2.96,2.52,1,3.19,2.71,1,2.71,2.2999999999999998,1,2.96,2.52,1,3.19,2.71,1,2.44,2.0699999999999998,1,2.66,2.2599999999999998,1,2.87,2.44,1,2.44,2.0699999999999998,1,2.66,2.2599999999999998,1,2.87,2.44,1]
["180710009204276","18",100,1992,32.446443330000001,-96.664708079999997,"prestress concrete girder",2.0499999999999998,0.61,5,2.15,0.64,5,2.15,0.64,5,2.0499999999999998,0.61,5,2.15,0.64,5,2.15,0.64,5,2.46,0.73,4,2.58,0.77,4,2.58,0.77,4,2.46,0.73,4,2.58,0.77,4,2.58,0.77,4,2.2200000000000002,0.66,5,2.3199999999999998,0.69,5,2.3199999999999998,0.69,5,2.2200000000000002,0.66,5,2.3199999999999998,0.69,5,2.3199999999999998,0.69,5]
["190190021802055","19",120,1981,33.44341627,-94.096844239999996,"prestress concrete girder",1.87,0.79,4,2.04,0.86,3,2.13,0.89,3,1.87,0.79,4,2.04,0.86,3,2.13,0.89,3,2.2200000000000002,0.94,2,2.41,1.01,1,2.5099999999999998,1.05,1,2.2200000000000002,0.94,2,2.41,1.01,1,2.5099999999999998,1.05,1,1.99,0.84,3,2.17,0.91,2,2.2599999999999998,0.95,2,1.99,0.84,3,2.17,0.91,2,2.2599999999999998,0.95,2]
["192250061003048","19",70,1986,33.158808809999996,-95.034489249999993,"steel girder",1.26,0.82,3,1.31,0.86,3,1.43,0.94,2,1.26,0.82,3,1.31,0.86,3,1.43,0.94,2,1.52,0.99,2,1.61,1.05,1,1.79,1.17,1,1.52,0.99,2,1.61,1.05,1,1.79,1.17,1,1.36,0.89,3,1.44,0.94,2,1.61,1.05,1,1.36,0.89,3,1.44,0.94,2,1.61,1.05,1]
["201810002809252","20",85,2006,30.098040999999998,-94.06729399999999,"prestress concrete girder",2.4700000000000002,2.1,1,2.4700000000000002,2.1,1,2.4700000000000002,2.1,1,2.4700000000000002,2.1,1,2.4700000000000002,2.1,1,2.4700000000000002,2.1,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,2.71,2.2999999999999998,1,2.71,2.2999999999999998,1,2.71,2.2999999999999998,1,2.71,2.2999999999999998,1,2.71,2.2999999999999998,1,2.71,2.2999999999999998,1]
["201810002811260","20",120,2009,30.130517050000002,-93.916282649999999,"prestress concrete girder",2.33,1.98,1,2.5499999999999998,2.17,1,2.66,2.2599999999999998,1,2.33,1.98,1,2.5499999999999998,2.17,1,2.66,2.2599999999999998,1,2.77,2.35,1,3.01,2.56,1,3.14,2.67,1,2.77,2.35,1,3.01,2.56,1,3.14,2.67,1,2.4900000000000002,2.12,1,2.71,2.2999999999999998,1,2.82,2.4,1,2.4900000000000002,2.12,1,2.71,2.2999999999999998,1,2.82,2.4,1]
["211090003918345","21",115,2006,26.172538119999999,-98.00730978,"prestress concrete girder",2.38,2.02,1,2.56,2.1800000000000002,1,2.63,2.2400000000000002,1,2.38,2.02,1,2.56,2.1800000000000002,1,2.63,2.2400000000000002,1,2.8,2.38,1,3.05,2.59,1,3.12,2.65,1,2.8,2.38,1,3.05,2.59,1,3.12,2.65,1,2.52,2.14,1,2.75,2.34,1,2.8,2.38,1,2.52,2.14,1,2.75,2.34,1,2.8,2.38,1]
["222400001806089","22",90,1997,27.530840189999999,-99.502938549999996,"steel girder",1.43,0.83,3,1.39,0.8,4,1.4,0.81,3,1.36,0.79,4,1.39,0.8,4,1.4,0.81,3,1.64,0.95,2,1.62,0.94,2,1.64,0.95,2,1.61,0.93,2,1.62,0.94,2,1.64,0.95,2,1.47,0.85,3,1.45,0.84,3,1.47,0.85,3,1.45,0.84,3,1.45,0.84,3,1.47,0.85,3]
["230680000706147","23",85,1970,32.452726560000002,-98.662452869999996,"prestress concrete girder",2.3199999999999998,0.82,3,2.3199999999999998,0.82,3,2.3199999999999998,0.82,3,2.3199999999999998,0.82,3,2.3199999999999998,0.82,3,2.3199999999999998,0.82,3,2.83,1,2,2.83,1,2,2.83,1,2,2.83,1,2,2.83,1,2,2.83,1,2,2.54,0.89,3,2.54,0.89,3,2.54,0.89,3,2.54,0.89,3,2.54,0.89,3,2.54,0.89,3]
["240720016701251","24",230,2010,31.830911109999999,-106.44003888,"Multi Span Long","Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1]
["240720212104284","24",85,2009,31.65972137,-106.23936870999999,"prestress concrete girder",2.4700000000000002,2.1,1,2.4700000000000002,2.1,1,2.4700000000000002,2.1,1,2.4700000000000002,2.1,1,2.4700000000000002,2.1,1,2.4700000000000002,2.1,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,2.71,2.2999999999999998,1,2.71,2.2999999999999998,1,2.71,2.2999999999999998,1,2.71,2.2999999999999998,1,2.71,2.2999999999999998,1,2.71,2.2999999999999998,1]
["252420027512066","25",80,1968,35.22688282,-100.34314252999999,"prestress concrete girder",2.29,0.54,5,2.29,0.54,5,2.29,0.54,5,2.29,0.54,5,2.29,0.54,5,2.29,0.54,5,2.81,0.66,5,2.81,0.66,5,2.81,0.66,5,2.81,0.66,5,2.81,0.66,5,2.81,0.66,5,2.52,0.59,5,2.52,0.59,5,2.52,0.59,5,2.52,0.59,5,2.52,0.59,5,2.52,0.59,5]
["021840031407051","02",65,2011,32.72964365,-97.789520580000001,"prestress concrete girder",2.4,1.44,1,2.4,1.44,1,2.4,1.44,1,2.4,1.44,1,2.4,1.44,1,2.4,1.44,1,3.05,1.83,1,3.05,1.83,1,3.05,1.83,1,3.05,1.83,1,3.05,1.83,1,3.05,1.83,1,2.74,1.64,1,2.74,1.64,1,2.74,1.64,1,2.74,1.64,1,2.74,1.64,1,2.74,1.64,1]
["021840031407059","02",65,1969,32.727344870000003,-97.80750544,"prestress concrete girder",2.21,0.88,3,2.21,0.88,3,2.21,0.88,3,2.21,0.88,3,2.21,0.88,3,2.21,0.88,3,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.52,1,2,2.52,1,2,2.52,1,2,2.52,1,2,2.52,1,2,2.52,1,2]
["022200000814442","02",115,2005,32.840528980000002,-97.238917400000005,"steel girder",1.9,1.62,1,2.04,1.73,1,1.98,1.68,1,1.69,1.44,1,1.85,1.57,1,1.94,1.65,1,2.2999999999999998,1.95,1,2.2999999999999998,1.95,1,2.2400000000000002,1.9,1,1.93,1.64,1,2.15,1.83,1,2.23,1.9,1,2.0699999999999998,1.76,1,2.0699999999999998,1.76,1,2.0099999999999998,1.71,1,1.74,1.48,1,1.93,1.64,1,2,1.7,1]
["022200001402439","02",115,2007,32.552693320000003,-97.318949549999999,"prestress concrete girder",2.38,2.02,1,2.56,2.1800000000000002,1,2.63,2.2400000000000002,1,2.38,2.02,1,2.56,2.1800000000000002,1,2.63,2.2400000000000002,1,2.8,2.38,1,3.05,2.59,1,3.12,2.65,1,2.8,2.38,1,3.05,2.59,1,3.12,2.65,1,2.52,2.14,1,2.75,2.34,1,2.8,2.38,1,2.52,2.14,1,2.75,2.34,1,2.8,2.38,1]
["022200001416594","02",230,2016,32.808900000000001,-97.314639999999997,"steel girder",2.14,2.14,1,2.27,2.27,1,2.41,2.41,1,1.75,1.75,1,1.94,1.94,1,2.17,2.17,1,2.46,2.46,1,2.6,2.6,1,2.77,2.77,1,2.0699999999999998,2.0699999999999998,1,2.31,2.31,1,2.61,2.61,1,2.21,2.21,1,2.34,2.34,1,2.4900000000000002,2.4900000000000002,1,1.86,1.86,1,2.08,2.08,1,2.35,2.35,1]
["022200036401668","02",90,2014,32.839140999999998,-97.188532269999996,"prestress concrete girder",2.4900000000000002,2.12,1,2.5,2.13,1,2.5,2.13,1,2.4900000000000002,2.12,1,2.5,2.13,1,2.5,2.13,1,3.02,2.57,1,3.02,2.57,1,3.02,2.57,1,3.02,2.57,1,3.02,2.57,1,3.02,2.57,1,2.72,2.31,1,2.72,2.31,1,2.72,2.31,1,2.72,2.31,1,2.72,2.31,1,2.72,2.31,1]
["022200106801215","02",125,1975,32.739950999999998,-97.482241999999999,"prestress concrete girder",1.81,0.77,4,2,0.84,3,2.12,0.89,3,1.81,0.77,4,2,0.84,3,2.12,0.89,3,2.16,0.91,2,2.35,0.99,2,2.5,1.05,1,2.16,0.91,2,2.35,0.99,2,2.5,1.05,1,1.95,0.82,3,2.12,0.89,3,2.25,0.94,2,1.95,0.82,3,2.12,0.89,3,2.25,0.94,2]
["022200106802197","02",60,1997,32.759813459999997,-97.17344464,"prestress concrete girder",2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1]
["031690022403048","03",125,1977,33.575125900000003,-97.895313580000007,"prestress concrete girder",1.81,0.77,4,2,0.84,3,2.12,0.89,3,1.81,0.77,4,2,0.84,3,2.12,0.89,3,2.16,0.91,2,2.35,0.99,2,2.5,1.05,1,2.16,0.91,2,2.35,0.99,2,2.5,1.05,1,1.95,0.82,3,2.12,0.89,3,2.25,0.94,2,1.95,0.82,3,2.12,0.89,3,2.25,0.94,2]
["032430004308116","03",70,1968,34.045966440000001,-98.95273967,"prestress concrete girder",2.23,0.79,4,2.23,0.79,4,2.23,0.79,4,2.23,0.79,4,2.23,0.79,4,2.23,0.79,4,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3]
["032440004306186","03",60,1995,34.152664000000001,-99.245554999999996,"prestress concrete girder",2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1]
["041880027501082","04",70,1968,35.205114180000002,-101.67172352999999,"prestress concrete girder",2.23,0.63,5,2.23,0.63,5,2.23,0.63,5,2.23,0.63,5,2.23,0.63,5,2.23,0.63,5,2.8,0.79,4,2.8,0.79,4,2.8,0.79,4,2.8,0.79,4,2.8,0.79,4,2.8,0.79,4,2.5099999999999998,0.71,4,2.5099999999999998,0.71,4,2.5099999999999998,0.71,4,2.5099999999999998,0.71,4,2.5099999999999998,0.71,4,2.5099999999999998,0.71,4]
["041910016809078","04",70,2005,35.072072140000003,-101.91911378,"prestress concrete girder",2.42,2.42,1,2.42,2.42,1,2.42,2.42,1,2.42,2.42,1,2.42,2.42,1,2.42,2.42,1,3.03,3.03,1,3.03,3.03,1,3.03,3.03,1,3.03,3.03,1,3.03,3.03,1,3.03,3.03,1,2.71,2.71,1,2.71,2.71,1,2.71,2.71,1,2.71,2.71,1,2.71,2.71,1,2.71,2.71,1]
["051520006711202","05",125,1992,33.56335953,-101.8451068,"prestress concrete girder",1.81,0.77,4,2,0.84,3,2.12,0.89,3,1.81,0.77,4,2,0.84,3,2.12,0.89,3,2.16,0.91,2,2.35,0.99,2,2.5,1.05,1,2.16,0.91,2,2.35,0.99,2,2.5,1.05,1,1.95,0.82,3,2.12,0.89,3,2.25,0.94,2,1.95,0.82,3,2.12,0.89,3,2.25,0.94,2]
["061650000515192","06",65,1965,31.97620526,-102.05740702,"prestress concrete girder",2.21,0.62,5,2.21,0.62,5,2.21,0.62,5,2.21,0.62,5,2.21,0.62,5,2.21,0.62,5,2.81,0.79,4,2.81,0.79,4,2.81,0.79,4,2.81,0.79,4,2.81,0.79,4,2.81,0.79,4,2.52,0.71,4,2.52,0.71,4,2.52,0.71,4,2.52,0.71,4,2.52,0.71,4,2.52,0.71,4]
["061860044107175","06",105,1982,30.94756022,-103.37117682,"prestress concrete girder",2.0099999999999998,0.84,3,2.15,0.9,3,2.15,0.9,3,2.0099999999999998,0.84,3,2.15,0.9,3,2.15,0.9,3,2.39,1,2,2.56,1.08,1,2.56,1.08,1,2.39,1,2,2.56,1.08,1,2.56,1.08,1,2.15,0.9,3,2.2999999999999998,0.97,2,2.2999999999999998,0.97,2,2.15,0.9,3,2.2999999999999998,0.97,2,2.2999999999999998,0.97,2]
["070530014011109","07",90,1974,30.69921995,-101.23196108,"prestress concrete girder",2.16,0.91,2,2.17,0.91,2,2.17,0.91,2,2.16,0.91,2,2.17,0.91,2,2.17,0.91,2,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2]
["071340014201101","07",60,1969,30.4137199,-99.667279840000006,"prestress concrete girder",2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.84,1.1299999999999999,1,2.84,1.1299999999999999,1,2.84,1.1299999999999999,1,2.84,1.1299999999999999,1,2.84,1.1299999999999999,1,2.84,1.1299999999999999,1,2.5499999999999998,1.02,1,2.5499999999999998,1.02,1,2.5499999999999998,1.02,1,2.5499999999999998,1.02,1,2.5499999999999998,1.02,1,2.5499999999999998,1.02,1]
["081280003305031","08",55,1981,32.598425329999998,-99.814603300000002,"steel girder",1.32,0.77,4,1.53,0.89,3,1.82,1.05,1,1.32,0.77,4,1.54,0.89,3,1.82,1.05,1,1.72,0.99,2,1.91,1.1000000000000001,1,2.2400000000000002,1.29,1,1.72,0.99,2,1.91,1.1000000000000001,1,2.2400000000000002,1.29,1,1.53,0.89,3,1.72,0.99,2,2.02,1.17,1,1.53,0.89,3,1.72,0.99,2,2.02,1.17,1]
["082210000604132","08",45,1958,32.462976830000002,-99.953351710000007,"concrete bridge",1.87,0.7,5,2.35,0.87,3,2.42,0.9,3,1.87,0.7,5,2.35,0.87,3,2.42,0.9,3,2.35,0.87,3,2.56,0.95,2,2.56,0.95,2,2.35,0.87,3,2.56,0.95,2,2.56,0.95,2,2.12,0.79,4,2.2999999999999998,0.86,3,2.2999999999999998,0.86,3,2.12,0.79,4,2.2999999999999998,0.86,3,2.2999999999999998,0.86,3]
["082210003306077","08",85,1970,32.501565730000003,-99.755868210000003,"prestress concrete girder",2.3199999999999998,0.82,3,2.3199999999999998,0.82,3,2.3199999999999998,0.82,3,2.3199999999999998,0.82,3,2.3199999999999998,0.82,3,2.3199999999999998,0.82,3,2.83,1,2,2.83,1,2,2.83,1,2,2.83,1,2,2.83,1,2,2.83,1,2,2.54,0.89,3,2.54,0.89,3,2.54,0.89,3,2.54,0.89,3,2.54,0.89,3,2.54,0.89,3]
["090140023103078","09",125,2015,31.070531249999998,-97.669560419999996,"prestress concrete girder",2.29,1.72,1,2.54,1.91,1,2.69,2.02,1,2.2999999999999998,1.72,1,2.54,1.91,1,2.69,2.02,1,2.74,2.06,1,2.98,2.2400000000000002,1,3.17,2.38,1,2.74,2.06,1,2.98,2.2400000000000002,1,3.17,2.38,1,2.4700000000000002,1.85,1,2.68,2.0099999999999998,1,2.85,2.14,1,2.4700000000000002,1.85,1,2.68,2.0099999999999998,1,2.85,2.14,1]
["091100001424063","09",135,2007,31.968074949999998,-97.118832569999995,"steel girder",1.8,1.53,1,1.99,1.69,1,2.12,1.8,1,1.68,1.43,1,1.75,1.49,1,1.87,1.59,1,2.17,1.84,1,2.39,2.0299999999999998,1,2.37,2.0099999999999998,1,1.87,1.59,1,2,1.7,1,2.17,1.84,1,1.95,1.66,1,2.14,1.82,1,2.13,1.81,1,1.69,1.44,1,1.8,1.53,1,1.95,1.66,1]
["091610001501541","09",125,2013,31.651111,-97.100551999999993,"prestress concrete special",2.29,2.29,0,2.54,2.54,0,2.69,2.69,0,2.2999999999999998,2.2999999999999998,0,2.54,2.54,0,2.69,2.69,0,2.74,2.74,0,2.98,2.98,0,3.17,3.17,0,2.74,2.74,0,2.98,2.98,0,3.17,3.17,0,2.4700000000000002,2.4700000000000002,0,2.68,2.68,0,2.85,2.85,0,2.4700000000000002,2.4700000000000002,0,2.68,2.68,0,2.85,2.85,0]
["111740017507079","11",75,1970,31.681576249999999,-94.665824270000002,"prestress concrete girder",2.2599999999999998,0.8,4,2.2599999999999998,0.8,4,2.2599999999999998,0.8,4,2.2599999999999998,0.8,4,2.2599999999999998,0.8,4,2.2599999999999998,0.8,4,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3]
["120850050004358","12",95,2001,29.448893989999998,-95.076588220000005,"prestress concrete girder",2.1,0.88,3,2.16,0.91,2,2.16,0.91,2,2.1,0.88,3,2.16,0.91,2,2.16,0.91,2,2.5499999999999998,1.07,1,2.6,1.1000000000000001,1,2.6,1.1000000000000001,1,2.5499999999999998,1.07,1,2.6,1.1000000000000001,1,2.6,1.1000000000000001,1,2.2999999999999998,0.97,2,2.34,0.99,2,2.34,0.99,2,2.2999999999999998,0.97,2,2.34,0.99,2,2.34,0.99,2]
["121020011006105","12",225,1989,29.91964059,-95.412330319999995,"Multi Span Long",0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1]
["121020017707221","12",105,1998,29.987317310000002,-95.275488539999998,"prestress concrete special",2.0099999999999998,0.74,0,2.15,0.8,0,2.15,0.8,0,2.0099999999999998,0.74,0,2.15,0.8,0,2.15,0.8,0,2.39,0.89,0,2.56,0.95,0,2.56,0.95,0,2.39,0.89,0,2.56,0.95,0,2.56,0.95,0,2.15,0.8,0,2.2999999999999998,0.86,0,2.2999999999999998,0.86,0,2.15,0.8,0,2.2999999999999998,0.86,0,2.2999999999999998,0.86,0]
["121020027107608","12",125,2007,29.784492360000002,-95.606530309999997,"prestress concrete special",2.29,1.95,0,2.54,2.16,0,2.69,2.29,0,2.2999999999999998,1.95,0,2.54,2.16,0,2.69,2.29,0,2.74,2.33,0,2.98,2.5299999999999998,0,3.17,2.69,0,2.74,2.33,0,2.98,2.5299999999999998,0,3.17,2.69,0,2.4700000000000002,2.1,0,2.68,2.2799999999999998,0,2.85,2.42,0,2.4700000000000002,2.1,0,2.68,2.2799999999999998,0,2.85,2.42,0]
["121020027116151","12",65,1992,29.679284989999999,-95.446585600000006,"prestress concrete girder",2.25,0.83,3,2.25,0.83,3,2.25,0.83,3,2.25,0.83,3,2.25,0.83,3,2.25,0.83,3,2.86,1.07,1,2.86,1.07,1,2.86,1.07,1,2.86,1.07,1,2.86,1.07,1,2.86,1.07,1,2.56,0.95,2,2.56,0.95,2,2.56,0.95,2,2.56,0.95,2,2.56,0.95,2,2.56,0.95,2]
["121020027116496","12",60,1968,29.683257300000001,-95.349083739999998,"concrete bridge",1.55,0.57999999999999996,5,1.73,0.65,5,2.04,0.76,4,1.55,0.57999999999999996,5,1.73,0.65,5,2.04,0.76,4,1.98,0.74,4,2.2200000000000002,0.83,3,2.5299999999999998,0.94,2,1.98,0.74,4,2.2200000000000002,0.83,3,2.5299999999999998,0.94,2,1.77,0.66,5,1.99,0.74,4,2.27,0.84,3,1.77,0.66,5,1.99,0.74,4,2.27,0.84,3]
["121020050003216","12",95,1996,29.755422159999998,-95.374557699999997,"steel girder",1.49,0.86,3,1.44,0.83,3,1.43,0.83,3,1.38,0.8,4,1.44,0.83,3,1.43,0.83,3,1.7,0.98,2,1.66,0.96,2,1.66,0.96,2,1.61,0.93,2,1.66,0.96,2,1.66,0.96,2,1.53,0.89,3,1.49,0.86,3,1.49,0.86,3,1.45,0.84,3,1.49,0.86,3,1.49,0.86,3]
["121020050003444","12",120,2016,29.553355999999997,-95.153804999999991,"prestress concrete girder",2.33,2.33,1,2.5499999999999998,2.5499999999999998,1,2.66,2.66,1,2.33,2.33,1,2.5499999999999998,2.5499999999999998,1,2.66,2.66,1,2.77,2.77,1,3.01,3.01,1,3.14,3.14,1,2.77,2.77,1,3.01,3.01,1,3.14,3.14,1,2.4900000000000002,2.4900000000000002,1,2.71,2.71,1,2.82,2.82,1,2.4900000000000002,2.4900000000000002,1,2.71,2.71,1,2.82,2.82,1]
["121020050801317","12",270,1995,29.79179602,-95.059956700000001,"Multi Span Long",0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1]
["130080027103223","13",50,1966,29.764467920000001,-96.152751870000003,"prestress concrete girder",2.2000000000000002,0.62,5,2.2000000000000002,0.62,5,2.2000000000000002,0.62,5,2.2000000000000002,0.62,5,2.2000000000000002,0.62,5,2.2000000000000002,0.62,5,2.99,0.85,3,2.99,0.85,3,2.99,0.85,3,2.99,0.85,3,2.99,0.85,3,2.99,0.85,3,2.67,0.75,4,2.67,0.75,4,2.67,0.75,4,2.67,0.75,4,2.67,0.75,4,2.67,0.75,4]
["130900053504143","13",45,1971,29.662619719999999,-97.38176378,"concrete bridge",2.4,0.85,3,2.4,0.85,3,2.4,0.85,3,2.41,0.85,3,2.4,0.85,3,2.4,0.85,3,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1]
["132350037101067","13",110,1986,28.531606409999998,-97.04294634,"prestress concrete girder",1.97,0.74,4,2.12,0.79,4,2.14,0.8,4,1.97,0.74,4,2.12,0.79,4,2.14,0.8,4,2.3199999999999998,0.86,3,2.54,0.95,2,2.54,0.95,2,2.3199999999999998,0.86,3,2.54,0.95,2,2.54,0.95,2,2.09,0.77,4,2.2799999999999998,0.85,3,2.2799999999999998,0.85,3,2.09,0.77,4,2.2799999999999998,0.85,3,2.2799999999999998,0.85,3]
["142270001513363","14",100,2017,30.309918150000001,-97.710004780000006,"steel weathered girder",1.96,1.67,1,1.93,1.64,1,1.9,1.62,1,1.78,1.51,1,1.89,1.61,1,1.9,1.62,1,2.2799999999999998,1.94,1,2.2000000000000002,1.87,1,2.19,1.86,1,2.11,1.79,1,2.2000000000000002,1.87,1,2.19,1.86,1,2.0499999999999998,1.74,1,1.98,1.68,1,1.96,1.67,1,1.89,1.61,1,1.97,1.67,1,1.96,1.67,1]
["142460001508242","14",75,1981,30.649972439999999,-97.679540029999998,"prestress concrete girder",2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2]
["150070007305163","15",80,1976,28.771442820000001,-98.305080770000004,"prestress concrete girder",2.19,0.92,2,2.19,0.92,2,2.19,0.92,2,2.2000000000000002,0.93,2,2.2000000000000002,0.93,2,2.2000000000000002,0.93,2,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1]
["150150001710154","15",60,1962,29.441730580000002,-98.438034610000003,"steel girder",1.27,0.74,4,1.41,0.82,3,1.66,0.96,2,1.27,0.74,4,1.41,0.82,3,1.66,0.96,2,1.61,0.93,2,1.81,1.04,1,2.06,1.19,1,1.61,0.93,2,1.81,1.04,1,2.06,1.19,1,1.44,0.83,3,1.62,0.94,2,1.85,1.07,1,1.44,0.83,3,1.62,0.94,2,1.85,1.07,1]
["150150002502132","15",60,1964,29.432904999999998,-98.400793999999991,"steel girder",1.27,0.74,4,1.41,0.82,3,1.66,0.96,2,1.27,0.74,4,1.41,0.82,3,1.66,0.96,2,1.61,0.93,2,1.81,1.04,1,2.06,1.19,1,1.61,0.93,2,1.81,1.04,1,2.06,1.19,1,1.44,0.83,3,1.62,0.94,2,1.85,1.07,1,1.44,0.83,3,1.62,0.94,2,1.85,1.07,1]
["150150007208197","15",75,1981,29.591430209999999,-98.597181390000003,"steel girder",1.29,0.84,3,1.31,0.86,3,1.38,0.9,3,1.29,0.84,3,1.31,0.86,3,1.38,0.9,3,1.53,1,2,1.58,1.04,1,1.7,1.1100000000000001,1,1.53,1,2,1.58,1.04,1,1.7,1.1100000000000001,1,1.37,0.89,3,1.41,0.93,2,1.52,0.99,2,1.37,0.89,3,1.41,0.93,2,1.52,0.99,2]
["150150052104261","15",60,1988,29.432639999999999,-98.646827000000002,"prestress concrete girder",2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1]
["150150052106109","15",60,1964,29.450830379999999,-98.403991809999994,"steel girder",1.27,0.74,4,1.41,0.82,3,1.66,0.96,2,1.27,0.74,4,1.41,0.82,3,1.66,0.96,2,1.61,0.93,2,1.81,1.04,1,2.06,1.19,1,1.61,0.93,2,1.81,1.04,1,2.06,1.19,1,1.44,0.83,3,1.62,0.94,2,1.85,1.07,1,1.44,0.83,3,1.62,0.94,2,1.85,1.07,1]
["150950001606207","15",115,1999,29.609433289999998,-98.267151069999997,"prestress concrete girder",1.93,0.72,4,2.08,0.77,4,2.13,0.79,4,1.93,0.72,4,2.08,0.77,4,2.13,0.79,4,2.27,0.84,3,2.4700000000000002,0.92,2,2.5299999999999998,0.94,2,2.27,0.84,3,2.4700000000000002,0.92,2,2.5299999999999998,0.94,2,2.04,0.76,4,2.23,0.83,3,2.27,0.84,3,2.04,0.76,4,2.23,0.83,3,2.27,0.84,3]
["151330014202153","15",60,1976,30.24134398,-99.435699299999996,"prestress concrete girder",2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1]
["151630002404177","15",55,1996,29.33454626,-99.260474740000006,"prestress concrete girder",2.31,0.97,2,2.31,0.97,2,2.31,0.97,2,2.31,0.97,2,2.31,0.97,2,2.31,0.97,2,3.05,1.28,1,3.05,1.28,1,3.05,1.28,1,3.05,1.28,1,3.05,1.28,1,3.05,1.28,1,2.73,1.1499999999999999,1,2.73,1.1499999999999999,1,2.73,1.1499999999999999,1,2.73,1.1499999999999999,1,2.73,1.1499999999999999,1,2.73,1.1499999999999999,1]
["161780037310046","16",110,1999,27.816788880000001,-97.637537589999994,"prestress concrete girder",1.97,0.74,4,2.12,0.79,4,2.14,0.8,4,1.97,0.74,4,2.12,0.79,4,2.14,0.8,4,2.3199999999999998,0.86,3,2.54,0.95,2,2.54,0.95,2,2.3199999999999998,0.86,3,2.54,0.95,2,2.54,0.95,2,2.09,0.77,4,2.2799999999999998,0.85,3,2.2799999999999998,0.85,3,2.09,0.77,4,2.2799999999999998,0.85,3,2.2799999999999998,0.85,3]
["162050007405111","16",80,1969,27.947934999999998,-97.656150710000006,"prestress concrete girder",2.29,0.65,5,2.29,0.65,5,2.29,0.65,5,2.29,0.65,5,2.29,0.65,5,2.29,0.65,5,2.81,0.79,4,2.81,0.79,4,2.81,0.79,4,2.81,0.79,4,2.81,0.79,4,2.81,0.79,4,2.52,0.71,4,2.52,0.71,4,2.52,0.71,4,2.52,0.71,4,2.52,0.71,4,2.52,0.71,4]
["172360067507007","17",60,1959,30.705184840000001,-95.561213690000002,"concrete bridge",1.55,0.57999999999999996,5,1.73,0.65,5,2.04,0.76,4,1.55,0.57999999999999996,5,1.73,0.65,5,2.04,0.76,4,1.98,0.74,4,2.2200000000000002,0.83,3,2.5299999999999998,0.94,2,1.98,0.74,4,2.2200000000000002,0.83,3,2.5299999999999998,0.94,2,1.77,0.66,5,1.99,0.74,4,2.27,0.84,3,1.77,0.66,5,1.99,0.74,4,2.27,0.84,3]
["180570004707361","18",105,1998,32.861056159999997,-96.769953470000004,"prestress concrete girder",2.0099999999999998,0.84,3,2.15,0.9,3,2.15,0.9,3,2.0099999999999998,0.84,3,2.15,0.9,3,2.15,0.9,3,2.39,1,2,2.56,1.08,1,2.56,1.08,1,2.39,1,2,2.56,1.08,1,2.56,1.08,1,2.15,0.9,3,2.2999999999999998,0.97,2,2.2999999999999998,0.97,2,2.15,0.9,3,2.2999999999999998,0.97,2,2.2999999999999998,0.97,2]
["180570009513372","18",105,1988,32.702274150000001,-96.60553779,"prestress concrete girder",2.0099999999999998,0.74,4,2.15,0.8,4,2.15,0.8,4,2.0099999999999998,0.74,4,2.15,0.8,4,2.15,0.8,4,2.39,0.89,3,2.56,0.95,2,2.56,0.95,2,2.39,0.89,3,2.56,0.95,2,2.56,0.95,2,2.15,0.8,4,2.2999999999999998,0.86,3,2.2999999999999998,0.86,3,2.15,0.8,4,2.2999999999999998,0.86,3,2.2999999999999998,0.86,3]
["180570019603273","18",60,1958,32.835739240000002,-96.875229820000001,"prestress concrete girder",2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.84,1,2,2.84,1,2,2.84,1,2,2.84,1,2,2.84,1,2,2.84,1,2,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3]
["180570044202088","18",125,2005,32.619160860000001,-96.8233046,"prestress concrete girder",2.29,1.95,1,2.54,2.16,1,2.69,2.29,1,2.2999999999999998,1.95,1,2.54,2.16,1,2.69,2.29,1,2.74,2.33,1,2.98,2.5299999999999998,1,3.17,2.69,1,2.74,2.33,1,2.98,2.5299999999999998,1,3.17,2.69,1,2.4700000000000002,2.1,1,2.68,2.2799999999999998,1,2.85,2.42,1,2.4700000000000002,2.1,1,2.68,2.2799999999999998,1,2.85,2.42,1]
["180570237401558","18",130,2013,32.909053,-96.891888999999992,"prestress concrete girder",2.2599999999999998,2.2599999999999998,1,2.54,2.54,1,2.69,2.69,1,2.2599999999999998,2.2599999999999998,1,2.54,2.54,1,2.69,2.69,1,2.71,2.71,1,2.96,2.96,1,3.19,3.19,1,2.71,2.71,1,2.96,2.96,1,3.19,3.19,1,2.44,2.44,1,2.66,2.66,1,2.87,2.87,1,2.44,2.44,1,2.66,2.66,1,2.87,2.87,1]
["180570237403308","18",105,1973,32.659709700000001,-96.730088240000001,"steel girder",1.63,0.95,2,1.55,0.89,3,1.52,0.88,3,1.37,0.79,4,1.49,0.86,3,1.52,0.88,3,1.83,1.06,1,1.76,1.02,1,1.73,1,2,1.6,0.92,2,1.73,1,2,1.73,1,2,1.65,0.95,2,1.58,0.92,2,1.56,0.9,3,1.44,0.83,3,1.56,0.9,3,1.56,0.9,3]
["180570237404265","18",110,1974,32.663361469999998,-96.900782019999994,"steel girder",1.71,1.1200000000000001,1,1.62,1.06,1,1.57,1.03,1,1.37,0.89,3,1.5,0.99,2,1.56,1.02,1,1.91,1.25,1,1.82,1.19,1,1.78,1.1599999999999999,1,1.59,1.04,1,1.74,1.1399999999999999,1,1.78,1.1599999999999999,1,1.72,1.1200000000000001,1,1.64,1.07,1,1.6,1.05,1,1.43,0.94,2,1.57,1.03,1,1.6,1.05,1]
["180610036403173","18",130,2009,33.065326059999997,-96.889299370000003,"prestress concrete girder",2.2599999999999998,1.92,1,2.54,2.16,1,2.69,2.29,1,2.2599999999999998,1.92,1,2.54,2.16,1,2.69,2.29,1,2.71,2.2999999999999998,1,2.96,2.52,1,3.19,2.71,1,2.71,2.2999999999999998,1,2.96,2.52,1,3.19,2.71,1,2.44,2.0699999999999998,1,2.66,2.2599999999999998,1,2.87,2.44,1,2.44,2.0699999999999998,1,2.66,2.2599999999999998,1,2.87,2.44,1]
["190190061005164","19",65,1970,33.311506420000001,-94.696963220000001,"prestress concrete girder",2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3]
["190190061007201","19",105,2010,33.465355879999997,-94.066720590000003,"prestress concrete girder",2.41,2.0499999999999998,1,2.57,2.1800000000000002,1,2.57,2.1800000000000002,1,2.41,2.0499999999999998,1,2.57,2.1800000000000002,1,2.57,2.1800000000000002,1,2.87,2.44,1,3.07,2.61,1,3.07,2.61,1,2.87,2.44,1,3.07,2.61,1,3.07,2.61,1,2.58,2.19,1,2.76,2.35,1,2.76,2.35,1,2.58,2.19,1,2.76,2.35,1,2.76,2.35,1]
["201240002813223","20",90,1993,30.087587769999999,-94.136045760000002,"prestress concrete girder",2.16,0.91,2,2.17,0.91,2,2.17,0.91,2,2.16,0.91,2,2.17,0.91,2,2.17,0.91,2,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2]
["201240073902038","20",80,1989,30.044438,-94.150346999999996,"steel girder",1.33,0.77,4,1.33,0.77,4,1.37,0.79,4,1.33,0.77,4,1.33,0.77,4,1.37,0.79,4,1.55,0.89,3,1.57,0.91,2,1.65,0.95,2,1.55,0.89,3,1.57,0.91,2,1.65,0.95,2,1.39,0.8,4,1.41,0.82,3,1.48,0.86,3,1.39,0.8,4,1.41,0.82,3,1.48,0.86,3]
["210310003907367","21",120,2005,26.13103692,-97.64308733,"prestress concrete girder",2.33,1.98,1,2.5499999999999998,2.17,1,2.66,2.2599999999999998,1,2.33,1.98,1,2.5499999999999998,2.17,1,2.66,2.2599999999999998,1,2.77,2.35,1,3.01,2.56,1,3.14,2.67,1,2.77,2.35,1,3.01,2.56,1,3.14,2.67,1,2.4900000000000002,2.12,1,2.71,2.2999999999999998,1,2.82,2.4,1,2.4900000000000002,2.12,1,2.71,2.2999999999999998,1,2.82,2.4,1]
["211090003917108","21",55,1993,26.206810449999999,-98.181934330000004,"prestress concrete girder",2.31,0.86,3,2.31,0.86,3,2.31,0.86,3,2.31,0.86,3,2.31,0.86,3,2.31,0.86,3,3.05,1.1299999999999999,1,3.05,1.1299999999999999,1,3.05,1.1299999999999999,1,3.05,1.1299999999999999,1,3.05,1.1299999999999999,1,3.05,1.1299999999999999,1,2.73,1.01,1,2.73,1.01,1,2.73,1.01,1,2.73,1.01,1,2.73,1.01,1,2.73,1.01,1]
["211090003918284","21",110,2002,26.191077969999998,-98.122297810000006,"prestress concrete girder",1.97,0.83,3,2.12,0.89,3,2.14,0.9,3,1.97,0.83,3,2.12,0.89,3,2.14,0.9,3,2.3199999999999998,0.98,2,2.54,1.07,1,2.54,1.07,1,2.3199999999999998,0.98,2,2.54,1.07,1,2.54,1.07,1,2.09,0.88,3,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.09,0.88,3,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2]
["221590029904066","22",160,2009,28.73824303,-100.49131503,"steel girder",2.13,1.81,1,2.34,1.99,1,2.58,2.19,1,2.02,1.72,1,2.34,1.99,1,2.58,2.19,1,2.4900000000000002,2.12,1,2.76,2.35,1,3.06,2.6,1,2.4500000000000002,2.08,1,2.76,2.35,1,3.06,2.6,1,2.2400000000000002,1.9,1,2.48,2.11,1,2.75,2.34,1,2.2000000000000002,1.87,1,2.48,2.11,1,2.75,2.34,1]
["240720212102176","24",105,1968,31.764058540000001,-106.48649257,"steel girder",1.63,0.76,4,1.55,0.71,4,1.52,0.7,5,1.37,0.63,5,1.49,0.69,5,1.52,0.7,5,1.83,0.85,3,1.76,0.82,3,1.73,0.8,4,1.6,0.74,4,1.73,0.8,4,1.73,0.8,4,1.65,0.76,4,1.58,0.73,4,1.56,0.72,4,1.44,0.67,5,1.56,0.72,4,1.56,0.72,4]
["241160000205172","24",80,1981,31.176996549999998,-105.7048865,"prestress concrete girder",2.19,0.65,5,2.19,0.65,5,2.19,0.65,5,2.2000000000000002,0.65,5,2.2000000000000002,0.65,5,2.2000000000000002,0.65,5,2.7,0.8,4,2.7,0.8,4,2.7,0.8,4,2.7,0.8,4,2.7,0.8,4,2.7,0.8,4,2.42,0.72,4,2.42,0.72,4,2.42,0.72,4,2.42,0.72,4,2.42,0.72,4,2.42,0.72,4]
["251000004302143","25",120,1970,34.316108,-99.824246000000002,"prestress concrete girder",2.2799999999999998,0.8,4,2.4900000000000002,0.88,3,2.6,0.92,2,2.2799999999999998,0.8,4,2.4900000000000002,0.88,3,2.6,0.92,2,2.71,0.95,2,2.94,1.04,1,3.07,1.08,1,2.71,0.95,2,2.94,1.04,1,3.07,1.08,1,2.44,0.86,3,2.65,0.94,2,2.76,0.98,2,2.44,0.86,3,2.65,0.94,2,2.76,0.98,2]
["021270001403193","02",60,2007,32.429958589999998,-97.238142479999993,"steel girder",1.6,0.96,2,1.78,1.07,1,1.94,1.1599999999999999,1,1.6,0.96,2,1.78,1.07,1,1.94,1.1599999999999999,1,2.0299999999999998,1.22,1,2.29,1.37,1,2.5,1.5,1,2.0299999999999998,1.22,1,2.29,1.37,1,2.5,1.5,1,1.82,1.0900000000000001,1,2.0499999999999998,1.23,1,2.2400000000000002,1.34,1,1.82,1.0900000000000001,1,2.0499999999999998,1.23,1,2.2400000000000002,1.34,1]
["022200000812387","02",110,1995,32.675146699999999,-97.381218730000001,"prestress concrete girder",1.97,0.83,3,2.12,0.89,3,2.14,0.9,3,1.97,0.83,3,2.12,0.89,3,2.14,0.9,3,2.3199999999999998,0.98,2,2.54,1.07,1,2.54,1.07,1,2.3199999999999998,0.98,2,2.54,1.07,1,2.54,1.07,1,2.09,0.88,3,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.09,0.88,3,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2]
["022200000813531","02",125,2018,32.808997999999995,-97.210017999999991,"prestress concrete girder",2.29,2.29,1,2.54,2.54,1,2.69,2.69,1,2.2999999999999998,2.2999999999999998,1,2.54,2.54,1,2.69,2.69,1,2.74,2.74,1,2.98,2.98,1,3.17,3.17,1,2.74,2.74,1,2.98,2.98,1,3.17,3.17,1,2.4700000000000002,2.4700000000000002,1,2.68,2.68,1,2.85,2.85,1,2.4700000000000002,2.4700000000000002,1,2.68,2.68,1,2.85,2.85,1]
["022200000814489","02",95,2013,32.838802020000003,-97.227564959999995,"prestress concrete girder",2.4500000000000002,2.08,1,2.52,2.14,1,2.52,2.14,1,2.4500000000000002,2.08,1,2.52,2.14,1,2.52,2.14,1,2.98,2.5299999999999998,1,3.04,2.58,1,3.04,2.58,1,2.98,2.5299999999999998,1,3.04,2.58,1,3.04,2.58,1,2.68,2.2799999999999998,1,2.73,2.3199999999999998,1,2.73,2.3199999999999998,1,2.68,2.2799999999999998,1,2.73,2.3199999999999998,1,2.73,2.3199999999999998,1]
["022200001416390","02",100,1981,32.737609820000003,-97.320423020000007,"prestress concrete girder",2.0499999999999998,0.86,3,2.15,0.9,3,2.15,0.9,3,2.0499999999999998,0.86,3,2.15,0.9,3,2.15,0.9,3,2.46,1.04,1,2.58,1.0900000000000001,1,2.58,1.0900000000000001,1,2.46,1.04,1,2.58,1.0900000000000001,1,2.58,1.0900000000000001,1,2.2200000000000002,0.94,2,2.3199999999999998,0.98,2,2.3199999999999998,0.98,2,2.2200000000000002,0.94,2,2.3199999999999998,0.98,2,2.3199999999999998,0.98,2]
["022200106801136","02",90,1967,32.7337627,-97.361980259999996,"steel girder",1.43,0.83,3,1.39,0.8,4,1.4,0.81,3,1.36,0.79,4,1.39,0.8,4,1.4,0.81,3,1.64,0.95,2,1.62,0.94,2,1.64,0.95,2,1.61,0.93,2,1.62,0.94,2,1.64,0.95,2,1.47,0.85,3,1.45,0.84,3,1.47,0.85,3,1.45,0.84,3,1.45,0.84,3,1.47,0.85,3]
["022200106801498","02",120,2014,32.73751,-97.353830000000002,"prestress concrete girder",2.33,2.33,1,2.5499999999999998,2.5499999999999998,1,2.66,2.66,1,2.33,2.33,1,2.5499999999999998,2.5499999999999998,1,2.66,2.66,1,2.77,2.77,1,3.01,3.01,1,3.14,3.14,1,2.77,2.77,1,3.01,3.01,1,3.14,3.14,1,2.4900000000000002,2.4900000000000002,1,2.71,2.71,1,2.82,2.82,1,2.4900000000000002,2.4900000000000002,1,2.71,2.71,1,2.82,2.82,1]
["022200226602093","02",70,1992,32.860750510000003,-97.063548909999994,"prestress concrete girder",2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1]
["022490001307067","02",70,1981,33.346094489999999,-97.684063039999998,"prestress concrete girder",2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1]
["032430004309192","03",85,2001,33.935990330000003,-98.518148249999996,"steel girder",1.38,0.9,3,1.35,0.88,3,1.38,0.9,3,1.35,0.88,3,1.35,0.88,3,1.38,0.9,3,1.59,1.04,1,1.59,1.04,1,1.64,1.07,1,1.59,1.04,1,1.59,1.04,1,1.64,1.07,1,1.43,0.94,2,1.42,0.93,2,1.47,0.96,2,1.42,0.93,2,1.42,0.93,2,1.47,0.96,2]
["032430015607049","03",45,1964,34.07818563,-98.557402569999994,"prestress concrete girder",2.2200000000000002,0.78,4,2.2200000000000002,0.78,4,2.2200000000000002,0.78,4,2.23,0.79,4,2.2200000000000002,0.78,4,2.2200000000000002,0.78,4,2.96,1.04,1,2.96,1.04,1,2.96,1.04,1,2.96,1.04,1,2.96,1.04,1,2.96,1.04,1,2.68,0.95,2,2.68,0.95,2,2.68,0.95,2,2.68,0.95,2,2.68,0.95,2,2.68,0.95,2]
["041880009005055","04",75,1969,35.187103430000001,-101.97420357,"prestress concrete girder",2.2599999999999998,0.64,5,2.2599999999999998,0.64,5,2.2599999999999998,0.64,5,2.2599999999999998,0.64,5,2.2599999999999998,0.64,5,2.2599999999999998,0.64,5,2.8,0.79,4,2.8,0.79,4,2.8,0.79,4,2.8,0.79,4,2.8,0.79,4,2.8,0.79,4,2.5099999999999998,0.71,4,2.5099999999999998,0.71,4,2.5099999999999998,0.71,4,2.5099999999999998,0.71,4,2.5099999999999998,0.71,4,2.5099999999999998,0.71,4]
["051520005301074","05",55,1966,33.420253389999999,-101.64287217,"prestress concrete girder",2.19,0.77,4,2.19,0.77,4,2.19,0.77,4,2.19,0.77,4,2.19,0.77,4,2.19,0.77,4,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.59,0.92,2,2.59,0.92,2,2.59,0.92,2,2.59,0.92,2,2.59,0.92,2,2.59,0.92,2]
["052190006703154","05",70,1987,34.519067900000003,-101.79508069000001,"prestress concrete girder",2.23,0.66,5,2.23,0.66,5,2.23,0.66,5,2.23,0.66,5,2.23,0.66,5,2.23,0.66,5,2.79,0.83,3,2.79,0.83,3,2.79,0.83,3,2.79,0.83,3,2.79,0.83,3,2.79,0.83,3,2.5,0.74,4,2.5,0.74,4,2.5,0.74,4,2.5,0.74,4,2.5,0.74,4,2.5,0.74,4]
["061950044105142","06",80,1975,30.993773149999999,-103.6620532,"prestress concrete girder",2.19,0.92,2,2.19,0.92,2,2.19,0.92,2,2.2000000000000002,0.93,2,2.2000000000000002,0.93,2,2.2000000000000002,0.93,2,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1]
["070530014011180","07",80,1976,30.680510309999999,-101.34850794,"prestress concrete girder",2.19,0.92,2,2.19,0.92,2,2.19,0.92,2,2.2000000000000002,0.93,2,2.2000000000000002,0.93,2,2.2000000000000002,0.93,2,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1]
["071340014109136","07",75,1975,30.524036680000002,-99.831074569999998,"prestress concrete girder",2.21,0.93,2,2.21,0.93,2,2.21,0.93,2,2.21,0.93,2,2.21,0.93,2,2.21,0.93,2,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.46,1.04,1,2.46,1.04,1,2.46,1.04,1,2.46,1.04,1,2.46,1.04,1,2.46,1.04,1]
["081050015704052","08",90,1987,32.970139199999998,-99.803058550000003,"prestress concrete girder",2.16,0.8,4,2.17,0.8,4,2.17,0.8,4,2.16,0.8,4,2.17,0.8,4,2.17,0.8,4,2.63,0.98,2,2.63,0.98,2,2.63,0.98,2,2.63,0.98,2,2.63,0.98,2,2.63,0.98,2,2.36,0.88,3,2.36,0.88,3,2.36,0.88,3,2.36,0.88,3,2.36,0.88,3,2.36,0.88,3]
["081680000508054","08",45,1957,32.385740640000002,-100.96109131,"concrete bridge",1.87,0.7,5,2.35,0.87,3,2.42,0.9,3,1.87,0.7,5,2.35,0.87,3,2.42,0.9,3,2.35,0.87,3,2.56,0.95,2,2.56,0.95,2,2.35,0.87,3,2.56,0.95,2,2.56,0.95,2,2.12,0.79,4,2.2999999999999998,0.86,3,2.2999999999999998,0.86,3,2.12,0.79,4,2.2999999999999998,0.86,3,2.2999999999999998,0.86,3]
["081770000603091","08",45,1957,32.488060560000001,-100.33721047,"concrete bridge",1.87,0.79,4,2.35,0.99,2,2.42,1.02,1,1.87,0.79,4,2.35,0.99,2,2.42,1.02,1,2.35,0.99,2,2.56,1.08,1,2.56,1.08,1,2.35,0.99,2,2.56,1.08,1,2.56,1.08,1,2.12,0.89,3,2.2999999999999998,0.97,2,2.2999999999999998,0.97,2,2.12,0.89,3,2.2999999999999998,0.97,2,2.2999999999999998,0.97,2]
["090140001514348","09",145,1976,31.045939999999998,-97.467059999999989,"steel girder",1.66,0.77,4,1.83,0.85,3,1.99,0.92,2,1.56,0.72,4,1.59,0.73,4,1.66,0.77,4,1.98,0.91,2,2.1800000000000002,1.01,1,2.2599999999999998,1.04,1,1.73,0.8,4,1.81,0.83,3,1.95,0.9,3,1.78,0.82,3,1.96,0.91,2,2.0299999999999998,0.94,2,1.55,0.71,4,1.63,0.76,4,1.75,0.81,3]
["091100001424040","09",100,2009,31.999336289999999,-97.097937659999999,"steel girder",2.4300000000000002,2.0699999999999998,1,2.5499999999999998,2.17,1,2.5499999999999998,2.17,1,2.4300000000000002,2.0699999999999998,1,2.5499999999999998,2.17,1,2.5499999999999998,2.17,1,2.91,2.4700000000000002,1,3.05,2.59,1,3.05,2.59,1,2.91,2.4700000000000002,1,3.05,2.59,1,3.05,2.59,1,2.62,2.23,1,2.74,2.33,1,2.74,2.33,1,2.62,2.23,1,2.74,2.33,1,2.74,2.33,1]
["100930049507289","10",130,1997,32.433178179999999,-94.760236550000002,"steel girder",1.7,0.98,2,1.88,1.0900000000000001,1,1.81,1.04,1,1.45,0.84,3,1.54,0.89,3,1.65,0.95,2,2.0499999999999998,1.19,1,2.12,1.22,1,2.02,1.17,1,1.63,0.95,2,1.77,1.02,1,1.9,1.1000000000000001,1,1.84,1.07,1,1.9,1.1000000000000001,1,1.82,1.05,1,1.47,0.85,3,1.59,0.92,2,1.71,0.99,2]
["110030017603033","11",55,2009,31.31209965,-94.721729580000002,"prestress concrete special",2.4,2.4,0,2.4,2.4,0,2.4,2.4,0,2.4,2.4,0,2.4,2.4,0,2.4,2.4,0,3.16,3.16,0,3.16,3.16,0,3.16,3.16,0,3.16,3.16,0,3.16,3.16,0,3.16,3.16,0,2.83,2.83,0,2.83,2.83,0,2.83,2.83,0,2.83,2.83,0,2.83,2.83,0,2.83,2.83,0]
["111870017701127","11",115,2009,30.608291149999999,-94.943117920000006,"prestress concrete girder",2.38,1.79,1,2.56,1.92,1,2.63,1.97,1,2.38,1.79,1,2.56,1.92,1,2.63,1.97,1,2.8,2.1,1,3.05,2.29,1,3.12,2.34,1,2.8,2.1,1,3.05,2.29,1,3.12,2.34,1,2.52,1.89,1,2.75,2.06,1,2.8,2.1,1,2.52,1.89,1,2.75,2.06,1,2.8,2.1,1]
["121020002713088","12",65,1993,29.726049639999999,-95.46825201,"prestress concrete girder",2.25,0.83,3,2.25,0.83,3,2.25,0.83,3,2.25,0.83,3,2.25,0.83,3,2.25,0.83,3,2.86,1.07,1,2.86,1.07,1,2.86,1.07,1,2.86,1.07,1,2.86,1.07,1,2.86,1.07,1,2.56,0.95,2,2.56,0.95,2,2.56,0.95,2,2.56,0.95,2,2.56,0.95,2,2.56,0.95,2]
["121020002713370","12",125,1998,29.65614287,-95.553106150000005,"prestress concrete girder",1.81,0.77,4,2,0.84,3,2.12,0.89,3,1.81,0.77,4,2,0.84,3,2.12,0.89,3,2.16,0.91,2,2.35,0.99,2,2.5,1.05,1,2.16,0.91,2,2.35,0.99,2,2.5,1.05,1,1.95,0.82,3,2.12,0.89,3,2.25,0.94,2,1.95,0.82,3,2.12,0.89,3,2.25,0.94,2]
["121020011006106","12",70,1989,29.88908928,-95.412181219999994,"prestress concrete girder",2.23,0.83,3,2.23,0.83,3,2.23,0.83,3,2.23,0.83,3,2.23,0.83,3,2.23,0.83,3,2.79,1.04,1,2.79,1.04,1,2.79,1.04,1,2.79,1.04,1,2.79,1.04,1,2.79,1.04,1,2.5,0.93,2,2.5,0.93,2,2.5,0.93,2,2.5,0.93,2,2.5,0.93,2,2.5,0.93,2]
["121020017711293","12",275,2003,29.76243689,-95.351252709999997,"Multi Span Long",0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1]
["121020027116235","12",65,1966,29.69183992,-95.325454030000003,"prestress concrete girder",2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3]
["121020050003082","12",55,1980,29.845497550000001,-95.392751009999998,"prestress concrete girder",2.31,0.97,2,2.31,0.97,2,2.31,0.97,2,2.31,0.97,2,2.31,0.97,2,2.31,0.97,2,3.05,1.28,1,3.05,1.28,1,3.05,1.28,1,3.05,1.28,1,3.05,1.28,1,3.05,1.28,1,2.73,1.1499999999999999,1,2.73,1.1499999999999999,1,2.73,1.1499999999999999,1,2.73,1.1499999999999999,1,2.73,1.1499999999999999,1,2.73,1.1499999999999999,1]
["121020050003272","12",55,1985,29.697560549999999,-95.289078970000006,"steel weathered girder",1.32,0.77,4,1.53,0.89,3,1.82,1.05,1,1.32,0.77,4,1.54,0.89,3,1.82,1.05,1,1.72,0.99,2,1.91,1.1000000000000001,1,2.2400000000000002,1.29,1,1.72,0.99,2,1.91,1.1000000000000001,1,2.2400000000000002,1.29,1,1.53,0.89,3,1.72,0.99,2,2.02,1.17,1,1.53,0.89,3,1.72,0.99,2,2.02,1.17,1]
["121020050801188","12",75,1968,29.774222430000002,-95.315588430000005,"prestress concrete girder",2.2599999999999998,0.64,5,2.2599999999999998,0.64,5,2.2599999999999998,0.64,5,2.2599999999999998,0.64,5,2.2599999999999998,0.64,5,2.2599999999999998,0.64,5,2.8,0.79,4,2.8,0.79,4,2.8,0.79,4,2.8,0.79,4,2.8,0.79,4,2.8,0.79,4,2.5099999999999998,0.71,4,2.5099999999999998,0.71,4,2.5099999999999998,0.71,4,2.5099999999999998,0.71,4,2.5099999999999998,0.71,4,2.5099999999999998,0.71,4]
["121700011004124","12",95,1990,30.114014269999998,-95.437678390000002,"prestress concrete girder",2.1,0.88,3,2.16,0.91,2,2.16,0.91,2,2.1,0.88,3,2.16,0.91,2,2.16,0.91,2,2.5499999999999998,1.07,1,2.6,1.1000000000000001,1,2.6,1.1000000000000001,1,2.5499999999999998,1.07,1,2.6,1.1000000000000001,1,2.6,1.1000000000000001,1,2.2999999999999998,0.97,2,2.34,0.99,2,2.34,0.99,2,2.2999999999999998,0.97,2,2.34,0.99,2,2.34,0.99,2]
["130760053507050","13",45,1967,29.69634224,-96.87134897,"concrete bridge",2.4,0.85,3,2.4,0.85,3,2.4,0.85,3,2.41,0.85,3,2.4,0.85,3,2.4,0.85,3,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1]
["130900053505148","13",95,1971,29.664105809999999,-97.363085400000003,"prestress concrete girder",2.33,0.83,3,2.39,0.84,3,2.39,0.84,3,2.33,0.83,3,2.39,0.84,3,2.39,0.84,3,2.83,1,2,2.88,1.01,1,2.88,1.01,1,2.83,1,2,2.88,1.01,1,2.88,1.01,1,2.5499999999999998,0.9,3,2.59,0.92,2,2.59,0.92,2,2.5499999999999998,0.9,3,2.59,0.92,2,2.59,0.92,2]
["132410008907130","13",45,1972,29.316566999999999,-96.124810999999994,"concrete bridge",2.4,0.85,3,2.4,0.85,3,2.4,0.85,3,2.41,0.85,3,2.4,0.85,3,2.4,0.85,3,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1]
["142460001509491","14",130,2006,30.481787199999999,-97.666290950000004,"prestress concrete girder",2.2599999999999998,1.92,1,2.54,2.16,1,2.69,2.29,1,2.2599999999999998,1.92,1,2.54,2.16,1,2.69,2.29,1,2.71,2.2999999999999998,1,2.96,2.52,1,3.19,2.71,1,2.71,2.2999999999999998,1,2.96,2.52,1,3.19,2.71,1,2.44,2.0699999999999998,1,2.66,2.2599999999999998,1,2.87,2.44,1,2.44,2.0699999999999998,1,2.66,2.2599999999999998,1,2.87,2.44,1]
["150150001709127","15",80,2008,29.368214949999999,-98.518375160000005,"steel girder",1.81,1.36,1,1.81,1.36,1,1.87,1.4,1,1.81,1.36,1,1.81,1.36,1,1.87,1.4,1,2.12,1.59,1,2.14,1.61,1,2.25,1.69,1,2.12,1.59,1,2.14,1.61,1,2.25,1.69,1,1.9,1.42,1,1.92,1.44,1,2.02,1.52,1,1.9,1.42,1,1.92,1.44,1,2.02,1.52,1]
["150150002407175","15",95,1997,29.375782969999999,-98.738675119999996,"prestress concrete girder",2.1,0.78,4,2.16,0.8,4,2.16,0.8,4,2.1,0.78,4,2.16,0.8,4,2.16,0.8,4,2.5499999999999998,0.95,2,2.6,0.97,2,2.6,0.97,2,2.5499999999999998,0.95,2,2.6,0.97,2,2.6,0.97,2,2.2999999999999998,0.86,3,2.34,0.87,3,2.34,0.87,3,2.2999999999999998,0.86,3,2.34,0.87,3,2.34,0.87,3]
["150150002502151","15",90,1987,29.396182979999999,-98.502549920000007,"steel girder",1.43,0.94,2,1.39,0.91,2,1.4,0.92,2,1.36,0.89,3,1.39,0.91,2,1.4,0.92,2,1.64,1.07,1,1.62,1.06,1,1.64,1.07,1,1.61,1.05,1,1.62,1.06,1,1.64,1.07,1,1.47,0.96,2,1.45,0.95,2,1.47,0.96,2,1.45,0.95,2,1.45,0.95,2,1.47,0.96,2]
["150150007212044","15",95,1993,29.433149,-98.501414999999994,"steel girder",1.49,0.86,3,1.44,0.83,3,1.43,0.83,3,1.38,0.8,4,1.44,0.83,3,1.43,0.83,3,1.7,0.98,2,1.66,0.96,2,1.66,0.96,2,1.61,0.93,2,1.66,0.96,2,1.66,0.96,2,1.53,0.89,3,1.49,0.86,3,1.49,0.86,3,1.45,0.84,3,1.49,0.86,3,1.49,0.86,3]
["150150007212264","15",95,1994,29.539394189999999,-98.571169749999996,"prestress concrete girder",2.1,0.88,3,2.16,0.91,2,2.16,0.91,2,2.1,0.88,3,2.16,0.91,2,2.16,0.91,2,2.5499999999999998,1.07,1,2.6,1.1000000000000001,1,2.6,1.1000000000000001,1,2.5499999999999998,1.07,1,2.6,1.1000000000000001,1,2.6,1.1000000000000001,1,2.2999999999999998,0.97,2,2.34,0.99,2,2.34,0.99,2,2.2999999999999998,0.97,2,2.34,0.99,2,2.34,0.99,2]
["150150052105053","15",85,1990,29.32704416,-98.619365669999993,"steel girder",1.38,0.8,4,1.35,0.78,4,1.38,0.8,4,1.35,0.78,4,1.35,0.78,4,1.38,0.8,4,1.59,0.92,2,1.59,0.92,2,1.64,0.95,2,1.59,0.92,2,1.59,0.92,2,1.64,0.95,2,1.43,0.83,3,1.42,0.82,3,1.47,0.85,3,1.42,0.82,3,1.42,0.82,3,1.47,0.85,3]
["150460001604239","15",100,2008,29.729360209999999,-98.077943110000007,"prestress concrete girder",2.4300000000000002,2.0699999999999998,1,2.5499999999999998,2.17,1,2.5499999999999998,2.17,1,2.4300000000000002,2.0699999999999998,1,2.5499999999999998,2.17,1,2.5499999999999998,2.17,1,2.91,2.4700000000000002,1,3.05,2.59,1,3.05,2.59,1,2.91,2.4700000000000002,1,3.05,2.59,1,3.05,2.59,1,2.62,2.23,1,2.74,2.33,1,2.74,2.33,1,2.62,2.23,1,2.74,2.33,1,2.74,2.33,1]
["151330014214071","15",50,1967,30.069473339999998,-99.086927299999999,"prestress concrete girder",2.2000000000000002,1.03,1,2.2000000000000002,1.03,1,2.2000000000000002,1.03,1,2.2000000000000002,1.03,1,2.2000000000000002,1.03,1,2.2000000000000002,1.03,1,2.99,1.41,1,2.99,1.41,1,2.99,1.41,1,2.99,1.41,1,2.99,1.41,1,2.99,1.41,1,2.67,1.25,1,2.67,1.25,1,2.67,1.25,1,2.67,1.25,1,2.67,1.25,1,2.67,1.25,1]
["160130010008103","16",120,1973,28.370055669999999,-97.732512270000001,"prestress concrete girder",2.2799999999999998,0.8,4,2.4900000000000002,0.88,3,2.6,0.92,2,2.2799999999999998,0.8,4,2.4900000000000002,0.88,3,2.6,0.92,2,2.71,0.95,2,2.94,1.04,1,3.07,1.08,1,2.71,0.95,2,2.94,1.04,1,3.07,1.08,1,2.44,0.86,3,2.65,0.94,2,2.76,0.98,2,2.44,0.86,3,2.65,0.94,2,2.76,0.98,2]
["161490007402133","16",90,1971,28.161783159999999,-97.859271280000002,"prestress concrete girder",2.35,0.94,2,2.36,0.94,2,2.36,0.94,2,2.35,0.94,2,2.36,0.94,2,2.36,0.94,2,2.85,1.1399999999999999,1,2.85,1.1399999999999999,1,2.85,1.1399999999999999,1,2.85,1.1399999999999999,1,2.85,1.1399999999999999,1,2.85,1.1399999999999999,1,2.56,1.02,1,2.56,1.02,1,2.56,1.02,1,2.56,1.02,1,2.56,1.02,1,2.56,1.02,1]
["161780037310049","16",100,1999,27.81053408,-97.638509060000004,"prestress concrete girder",2.0499999999999998,0.76,4,2.15,0.8,4,2.15,0.8,4,2.0499999999999998,0.76,4,2.15,0.8,4,2.15,0.8,4,2.46,0.92,2,2.58,0.96,2,2.58,0.96,2,2.46,0.92,2,2.58,0.96,2,2.58,0.96,2,2.2200000000000002,0.83,3,2.3199999999999998,0.86,3,2.3199999999999998,0.86,3,2.2200000000000002,0.83,3,2.3199999999999998,0.86,3,2.3199999999999998,0.86,3]
["162050037201020","16",55,1997,27.95679582,-97.576614739999997,"prestress concrete girder",2.31,0.86,3,2.31,0.86,3,2.31,0.86,3,2.31,0.86,3,2.31,0.86,3,2.31,0.86,3,3.05,1.1299999999999999,1,3.05,1.1299999999999999,1,3.05,1.1299999999999999,1,3.05,1.1299999999999999,1,3.05,1.1299999999999999,1,3.05,1.1299999999999999,1,2.73,1.01,1,2.73,1.01,1,2.73,1.01,1,2.73,1.01,1,2.73,1.01,1,2.73,1.01,1]
["180430004706396","18",70,1999,33.121962420000003,-96.666690489999993,"prestress concrete girder",2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1]
["180570000911252","18",60,1963,32.78727404,-96.765737939999994,"prestress concrete girder",2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.84,1,2,2.84,1,2,2.84,1,2,2.84,1,2,2.84,1,2,2.84,1,2,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3]
["180570000911453","18",120,1999,32.832835670000001,-96.612363909999999,"steel girder",1.73,1.1299999999999999,1,1.76,1.1599999999999999,1,1.68,1.1000000000000001,1,1.4,0.92,2,1.53,1,2,1.62,1.06,1,2.08,1.36,1,1.96,1.28,1,1.89,1.24,1,1.59,1.04,1,1.78,1.1599999999999999,1,1.86,1.22,1,1.86,1.22,1,1.76,1.1599999999999999,1,1.7,1.1100000000000001,1,1.43,0.94,2,1.6,1.05,1,1.67,1.1000000000000001,1]
["180570019603100","18",70,1959,32.801812050000002,-96.826976630000004,"prestress concrete girder",2.23,0.63,5,2.23,0.63,5,2.23,0.63,5,2.23,0.63,5,2.23,0.63,5,2.23,0.63,5,2.8,0.79,4,2.8,0.79,4,2.8,0.79,4,2.8,0.79,4,2.8,0.79,4,2.8,0.79,4,2.5099999999999998,0.71,4,2.5099999999999998,0.71,4,2.5099999999999998,0.71,4,2.5099999999999998,0.71,4,2.5099999999999998,0.71,4,2.5099999999999998,0.71,4]
["180570044202085","18",125,2004,32.633184470000003,-96.822976670000003,"prestress concrete girder",1.81,0.77,4,2,0.84,3,2.12,0.89,3,1.81,0.77,4,2,0.84,3,2.12,0.89,3,2.16,0.91,2,2.35,0.99,2,2.5,1.05,1,2.16,0.91,2,2.35,0.99,2,2.5,1.05,1,1.95,0.82,3,2.12,0.89,3,2.25,0.94,2,1.95,0.82,3,2.12,0.89,3,2.25,0.94,2]
["180570106804184","18",70,1994,32.762296829999997,-96.956504510000002,"prestress concrete girder",2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1]
["180570237402135","18",70,1971,32.771185670000001,-96.622907679999997,"prestress concrete girder",2.23,0.79,4,2.23,0.79,4,2.23,0.79,4,2.23,0.79,4,2.23,0.79,4,2.23,0.79,4,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3]
["180570237403323","18",70,1971,32.689146000000001,-96.634247999999999,"prestress concrete girder",2.23,0.79,4,2.23,0.79,4,2.23,0.79,4,2.23,0.79,4,2.23,0.79,4,2.23,0.79,4,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3]
["180570237407401","18",165,1986,32.933986820000001,-97.008261520000005,"prestress concrete girder",2.02,0.85,3,2.2000000000000002,0.93,2,2.38,1,2,1.97,0.83,3,2.1,0.88,3,2.13,0.89,3,2.38,1,2,2.6,1.1000000000000001,1,2.82,1.19,1,2.34,0.99,2,2.37,0.99,2,2.44,1.03,1,2.14,0.9,3,2.34,0.99,2,2.54,1.07,1,2.11,0.88,3,2.14,0.9,3,2.2000000000000002,0.93,2]
["180610019602306","18",85,2006,32.995896000000002,-96.951691999999994,"prestress concrete girder",2.4700000000000002,2.1,1,2.4700000000000002,2.1,1,2.4700000000000002,2.1,1,2.4700000000000002,2.1,1,2.4700000000000002,2.1,1,2.4700000000000002,2.1,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,2.71,2.2999999999999998,1,2.71,2.2999999999999998,1,2.71,2.2999999999999998,1,2.71,2.2999999999999998,1,2.71,2.2999999999999998,1,2.71,2.2999999999999998,1]
["180710009203289","18",80,1995,32.505063700000001,-96.663618229999997,"prestress concrete girder",2.19,0.92,2,2.19,0.92,2,2.19,0.92,2,2.2000000000000002,0.93,2,2.2000000000000002,0.93,2,2.2000000000000002,0.93,2,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1]
["191030049510123","19",65,1965,32.49381382,-94.296727219999994,"steel girder",1.25,0.72,4,1.33,0.77,4,1.51,0.87,3,1.25,0.72,4,1.33,0.77,4,1.51,0.87,3,1.54,0.89,3,1.68,0.97,2,1.93,1.1200000000000001,1,1.54,0.89,3,1.68,0.97,2,1.93,1.1200000000000001,1,1.38,0.8,4,1.51,0.87,3,1.73,1,2,1.38,0.8,4,1.51,0.87,3,1.73,1,2]
["200360050803430","20",80,1991,29.837249450000002,-94.577407679999993,"prestress concrete girder",2.19,0.92,2,2.19,0.92,2,2.19,0.92,2,2.2000000000000002,0.93,2,2.2000000000000002,0.93,2,2.2000000000000002,0.93,2,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1]
["210310003908226","21",50,2007,26.0291277,-97.533356449999999,"prestress concrete girder",2.41,2.0499999999999998,1,2.41,2.0499999999999998,1,2.41,2.0499999999999998,1,2.41,2.0499999999999998,1,2.41,2.0499999999999998,1,2.41,2.0499999999999998,1,3.27,2.78,1,3.27,2.78,1,3.27,2.78,1,3.27,2.78,1,3.27,2.78,1,3.27,2.78,1,2.93,2.4900000000000002,1,2.93,2.4900000000000002,1,2.93,2.4900000000000002,1,2.93,2.4900000000000002,1,2.93,2.4900000000000002,1,2.93,2.4900000000000002,1]
["211090003918412","21",115,2007,26.1516661,-97.931163979999994,"prestress concrete girder",2.38,2.02,1,2.56,2.1800000000000002,1,2.63,2.2400000000000002,1,2.38,2.02,1,2.56,2.1800000000000002,1,2.63,2.2400000000000002,1,2.8,2.38,1,3.05,2.59,1,3.12,2.65,1,2.8,2.38,1,3.05,2.59,1,3.12,2.65,1,2.52,2.14,1,2.75,2.34,1,2.8,2.38,1,2.52,2.14,1,2.75,2.34,1,2.8,2.38,1]
["222330002209079","22",130,2015,29.44194341,-100.918831,"prestress concrete girder",2.2599999999999998,1.92,1,2.54,2.16,1,2.69,2.29,1,2.2599999999999998,1.92,1,2.54,2.16,1,2.69,2.29,1,2.71,2.2999999999999998,1,2.96,2.52,1,3.19,2.71,1,2.71,2.2999999999999998,1,2.96,2.52,1,3.19,2.71,1,2.44,2.0699999999999998,1,2.66,2.2599999999999998,1,2.87,2.44,1,2.44,2.0699999999999998,1,2.66,2.2599999999999998,1,2.87,2.44,1]
["230680000703157","23",75,1972,32.400843209999998,-98.789741230000004,"prestress concrete girder",2.2599999999999998,0.9,3,2.2599999999999998,0.9,3,2.2599999999999998,0.9,3,2.2599999999999998,0.9,3,2.2599999999999998,0.9,3,2.2599999999999998,0.9,3,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.5099999999999998,1,2,2.5099999999999998,1,2,2.5099999999999998,1,2,2.5099999999999998,1,2,2.5099999999999998,1,2,2.5099999999999998,1,2]
["240720212102199","24",80,1969,31.76361854,-106.48885263,"steel girder",1.33,0.61,5,1.33,0.61,5,1.37,0.63,5,1.33,0.61,5,1.33,0.61,5,1.37,0.63,5,1.55,0.71,4,1.57,0.73,4,1.65,0.76,4,1.55,0.71,4,1.57,0.73,4,1.65,0.76,4,1.39,0.64,5,1.41,0.65,5,1.48,0.68,5,1.39,0.64,5,1.41,0.65,5,1.48,0.68,5]
["240720212104294","24",270,2015,31.699777780000002,-106.2821333,"Multi Span Long","Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1]
["010920004702217","01",60,1961,33.635137270000001,-96.616397669999998,"steel girder",1.27,0.74,4,1.41,0.82,3,1.66,0.96,2,1.27,0.74,4,1.41,0.82,3,1.66,0.96,2,1.61,0.93,2,1.81,1.04,1,2.06,1.19,1,1.61,0.93,2,1.81,1.04,1,2.06,1.19,1,1.44,0.83,3,1.62,0.94,2,1.85,1.07,1,1.44,0.83,3,1.62,0.94,2,1.85,1.07,1]
["022200000813110","02",60,1963,32.707971270000002,-97.231423269999993,"steel girder",1.27,0.74,4,1.41,0.82,3,1.66,0.96,2,1.27,0.74,4,1.41,0.82,3,1.66,0.96,2,1.61,0.93,2,1.81,1.04,1,2.06,1.19,1,1.61,0.93,2,1.81,1.04,1,2.06,1.19,1,1.44,0.83,3,1.62,0.94,2,1.85,1.07,1,1.44,0.83,3,1.62,0.94,2,1.85,1.07,1]
["022200000814259","02",95,1977,32.792786659999997,-97.454569100000001,"prestress concrete girder",2.1,0.78,4,2.16,0.8,4,2.16,0.8,4,2.1,0.78,4,2.16,0.8,4,2.16,0.8,4,2.5499999999999998,0.95,2,2.6,0.97,2,2.6,0.97,2,2.5499999999999998,0.95,2,2.6,0.97,2,2.6,0.97,2,2.2999999999999998,0.86,3,2.34,0.87,3,2.34,0.87,3,2.2999999999999998,0.86,3,2.34,0.87,3,2.34,0.87,3]
["022200001416191","02",55,1961,32.766261999999998,-97.317469029999998,"concrete bridge",1.62,0.48,5,1.88,0.56000000000000005,5,2.2400000000000002,0.67,5,1.62,0.48,5,1.89,0.56000000000000005,5,2.2400000000000002,0.67,5,2.11,0.62,5,2.34,0.7,5,2.75,0.82,3,2.11,0.62,5,2.35,0.7,5,2.75,0.82,3,1.88,0.56000000000000005,5,2.11,0.62,5,2.48,0.74,4,1.88,0.56000000000000005,5,2.11,0.62,5,2.48,0.74,4]
["022200001416575","02",120,2016,32.838270000000001,-97.312200000000004,"prestress concrete girder",2.33,2.33,1,2.5499999999999998,2.5499999999999998,1,2.66,2.66,1,2.33,2.33,1,2.5499999999999998,2.5499999999999998,1,2.66,2.66,1,2.77,2.77,1,3.01,3.01,1,3.14,3.14,1,2.77,2.77,1,3.01,3.01,1,3.14,3.14,1,2.4900000000000002,2.4900000000000002,1,2.71,2.71,1,2.82,2.82,1,2.4900000000000002,2.4900000000000002,1,2.71,2.71,1,2.82,2.82,1]
["022200008112210","02",120,2006,32.898646489999997,-97.316635009999999,"prestress concrete girder",2.33,1.75,1,2.5499999999999998,1.91,1,2.66,2,1,2.33,1.75,1,2.5499999999999998,1.91,1,2.66,2,1,2.77,2.08,1,3.01,2.2599999999999998,1,3.14,2.36,1,2.77,2.08,1,3.01,2.2599999999999998,1,3.14,2.36,1,2.4900000000000002,1.87,1,2.71,2.0299999999999998,1,2.82,2.11,1,2.4900000000000002,1.87,1,2.71,2.0299999999999998,1,2.82,2.11,1]
["022200106801455","02",120,2001,32.745027059999998,-97.332216119999998,"prestress concrete girder",1.87,0.79,4,2.04,0.86,3,2.13,0.89,3,1.87,0.79,4,2.04,0.86,3,2.13,0.89,3,2.2200000000000002,0.94,2,2.41,1.01,1,2.5099999999999998,1.05,1,2.2200000000000002,0.94,2,2.41,1.01,1,2.5099999999999998,1.05,1,1.99,0.84,3,2.17,0.91,2,2.2599999999999998,0.95,2,1.99,0.84,3,2.17,0.91,2,2.2599999999999998,0.95,2]
["022200237405235","02",120,1973,32.668050600000001,-97.223334890000004,"prestress concrete girder",2.2799999999999998,0.64,5,2.4900000000000002,0.7,5,2.6,0.73,4,2.2799999999999998,0.64,5,2.4900000000000002,0.7,5,2.6,0.73,4,2.71,0.76,4,2.94,0.83,3,3.07,0.86,3,2.71,0.76,4,2.94,0.83,3,3.07,0.86,3,2.44,0.69,5,2.65,0.75,4,2.76,0.78,4,2.44,0.69,5,2.65,0.75,4,2.76,0.78,4]
["022490001308072","02",105,1995,33.214472309999998,-97.583309589999999,"prestress concrete girder",2.0099999999999998,0.84,3,2.15,0.9,3,2.15,0.9,3,2.0099999999999998,0.84,3,2.15,0.9,3,2.15,0.9,3,2.39,1,2,2.56,1.08,1,2.56,1.08,1,2.39,1,2,2.56,1.08,1,2.56,1.08,1,2.15,0.9,3,2.2999999999999998,0.97,2,2.2999999999999998,0.97,2,2.15,0.9,3,2.2999999999999998,0.97,2,2.2999999999999998,0.97,2]
["032430015607040","03",65,1964,34.10024439,-98.546966859999998,"prestress concrete girder",2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3]
["040330027503089","04",85,1971,35.206946539999997,-101.32842780999999,"prestress concrete girder",2.3199999999999998,0.93,2,2.3199999999999998,0.93,2,2.3199999999999998,0.93,2,2.3199999999999998,0.93,2,2.3199999999999998,0.93,2,2.3199999999999998,0.93,2,2.83,1.1299999999999999,1,2.83,1.1299999999999999,1,2.83,1.1299999999999999,1,2.83,1.1299999999999999,1,2.83,1.1299999999999999,1,2.83,1.1299999999999999,1,2.54,1.01,1,2.54,1.01,1,2.54,1.01,1,2.54,1.01,1,2.54,1.01,1,2.54,1.01,1]
["041910006717140","04",120,1986,34.97968101,-101.8802847,"prestress concrete girder",1.87,0.7,5,2.04,0.76,4,2.13,0.79,4,1.87,0.7,5,2.04,0.76,4,2.13,0.79,4,2.2200000000000002,0.83,3,2.41,0.89,3,2.5099999999999998,0.93,2,2.2200000000000002,0.83,3,2.41,0.89,3,2.5099999999999998,0.93,2,1.99,0.74,4,2.17,0.8,4,2.2599999999999998,0.84,3,1.99,0.74,4,2.17,0.8,4,2.2599999999999998,0.84,3]
["051520006707088","05",110,1978,33.70855443,-101.84001781000001,"prestress concrete girder",2.1,0.78,4,1.98,0.74,4,1.93,0.72,4,1.68,0.62,5,1.84,0.68,5,1.92,0.71,4,2.34,0.87,3,2.2400000000000002,0.83,3,2.1800000000000002,0.81,3,1.95,0.73,4,2.14,0.8,4,2.1800000000000002,0.81,3,2.11,0.78,4,2.0099999999999998,0.74,4,1.96,0.73,4,1.75,0.65,5,1.92,0.71,4,1.96,0.73,4]
["051850016802072","05",60,1993,34.529895779999997,-102.87820562,"prestress concrete girder",2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1]
["061950044109102","06",70,1974,31.04655395,-103.95434944,"prestress concrete girder",2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1]
["072180014104103","07",70,1973,30.578435379999998,-100.64727687,"prestress concrete girder",2.23,0.89,3,2.23,0.89,3,2.23,0.89,3,2.23,0.89,3,2.23,0.89,3,2.23,0.89,3,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.5099999999999998,1,2,2.5099999999999998,1,2,2.5099999999999998,1,2,2.5099999999999998,1,2,2.5099999999999998,1,2,2.5099999999999998,1,2]
["080300000702108","08",45,1966,32.371634989999997,-99.195697620000004,"concrete bridge",1.87,0.7,5,2.35,0.87,3,2.42,0.9,3,1.87,0.7,5,2.35,0.87,3,2.42,0.9,3,2.35,0.87,3,2.56,0.95,2,2.56,0.95,2,2.35,0.87,3,2.56,0.95,2,2.56,0.95,2,2.12,0.79,4,2.2999999999999998,0.86,3,2.2999999999999998,0.86,3,2.12,0.79,4,2.2999999999999998,0.86,3,2.2999999999999998,0.86,3]
["082210000605324","08",80,2008,32.48134864,-99.773854999999998,"prestress concrete girder",2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1]
["090140018501044","09",125,2010,31.013866999999998,-97.305267000000001,"prestress concrete girder",2.29,1.95,1,2.54,2.16,1,2.69,2.29,1,2.2999999999999998,1.95,1,2.54,2.16,1,2.69,2.29,1,2.74,2.33,1,2.98,2.5299999999999998,1,3.17,2.69,1,2.74,2.33,1,2.98,2.5299999999999998,1,3.17,2.69,1,2.4700000000000002,2.1,1,2.68,2.2799999999999998,1,2.85,2.42,1,2.4700000000000002,2.1,1,2.68,2.2799999999999998,1,2.85,2.42,1]
["091610001501470","09",65,2003,31.639557839999998,-97.096432239999999,"prestress concrete special",2.25,0.94,0,2.25,0.94,0,2.25,0.94,0,2.25,0.94,0,2.25,0.94,0,2.25,0.94,0,2.86,1.21,0,2.86,1.21,0,2.86,1.21,0,2.86,1.21,0,2.86,1.21,0,2.86,1.21,0,2.56,1.08,0,2.56,1.08,0,2.56,1.08,0,2.56,1.08,0,2.56,1.08,0,2.56,1.08,0]
["091610025809077","09",60,1969,31.547049080000001,-97.070055069999995,"concrete bridge",1.55,0.46,5,1.73,0.52,5,2.04,0.61,5,1.55,0.46,5,1.73,0.52,5,2.04,0.61,5,1.98,0.59,5,2.2200000000000002,0.66,5,2.5299999999999998,0.75,4,1.98,0.59,5,2.2200000000000002,0.66,5,2.5299999999999998,0.75,4,1.77,0.53,5,1.99,0.59,5,2.27,0.67,5,1.77,0.53,5,1.99,0.59,5,2.27,0.67,5]
["111870017605091","11",70,1989,30.924062930000002,-94.825588780000004,"prestress concrete girder",2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1]
["120800027105293","12",45,1989,29.77739506,-95.826979969999996,"concrete bridge",2.42,0.9,3,2.42,0.9,3,2.42,0.9,3,2.4300000000000002,0.9,3,2.42,0.9,3,2.42,0.9,3,3.23,1.2,1,3.23,1.2,1,3.23,1.2,1,3.23,1.2,1,3.23,1.2,1,3.23,1.2,1,2.92,1.0900000000000001,1,2.92,1.0900000000000001,1,2.92,1.0900000000000001,1,2.92,1.0900000000000001,1,2.92,1.0900000000000001,1,2.92,1.0900000000000001,1]
["121020002713241","12",115,1992,29.716822090000001,-95.499307939999994,"prestress concrete girder",1.93,0.72,4,2.08,0.77,4,2.13,0.79,4,1.93,0.72,4,2.08,0.77,4,2.13,0.79,4,2.27,0.84,3,2.4700000000000002,0.92,2,2.5299999999999998,0.94,2,2.27,0.84,3,2.4700000000000002,0.92,2,2.5299999999999998,0.94,2,2.04,0.76,4,2.23,0.83,3,2.27,0.84,3,2.04,0.76,4,2.23,0.83,3,2.27,0.84,3]
["121020005009482","12",120,2016,29.867717630000001,-95.542232510000005,"prestress concrete girder",2.33,2.33,1,2.5499999999999998,2.5499999999999998,1,2.66,2.66,1,2.33,2.33,1,2.5499999999999998,2.5499999999999998,1,2.66,2.66,1,2.77,2.77,1,3.01,3.01,1,3.14,3.14,1,2.77,2.77,1,3.01,3.01,1,3.14,3.14,1,2.4900000000000002,2.4900000000000002,1,2.71,2.71,1,2.82,2.82,1,2.4900000000000002,2.4900000000000002,1,2.71,2.71,1,2.82,2.82,1]
["121020027106688","12",120,2014,29.787485999999998,-95.777476399999998,"prestress concrete special",2.33,1.98,0,2.5499999999999998,2.17,0,2.66,2.2599999999999998,0,2.33,1.98,0,2.5499999999999998,2.17,0,2.66,2.2599999999999998,0,2.77,2.35,0,3.01,2.56,0,3.14,2.67,0,2.77,2.35,0,3.01,2.56,0,3.14,2.67,0,2.4900000000000002,2.12,0,2.71,2.2999999999999998,0,2.82,2.4,0,2.4900000000000002,2.12,0,2.71,2.2999999999999998,0,2.82,2.4,0]
["121020027107604","12",60,2005,29.785195999999999,-95.609788999999992,"prestress concrete girder",2.4,2.04,1,2.4,2.04,1,2.4,2.04,1,2.4,2.04,1,2.4,2.04,1,2.4,2.04,1,3.1,2.64,1,3.1,2.64,1,3.1,2.64,1,3.1,2.64,1,3.1,2.64,1,3.1,2.64,1,2.77,2.35,1,2.77,2.35,1,2.77,2.35,1,2.77,2.35,1,2.77,2.35,1,2.77,2.35,1]
["121020027114651","12",50,2010,29.80423377,-95.284854089999996,"prestress concrete girder",2.41,2.0499999999999998,1,2.41,2.0499999999999998,1,2.41,2.0499999999999998,1,2.41,2.0499999999999998,1,2.41,2.0499999999999998,1,2.41,2.0499999999999998,1,3.27,2.78,1,3.27,2.78,1,3.27,2.78,1,3.27,2.78,1,3.27,2.78,1,3.27,2.78,1,2.93,2.4900000000000002,1,2.93,2.4900000000000002,1,2.93,2.4900000000000002,1,2.93,2.4900000000000002,1,2.93,2.4900000000000002,1,2.93,2.4900000000000002,1]
["121020027115706","12",120,1973,29.727505999999998,-95.266865999999993,"prestress concrete girder",2.2799999999999998,0.8,4,2.4900000000000002,0.88,3,2.6,0.92,2,2.2799999999999998,0.8,4,2.4900000000000002,0.88,3,2.6,0.92,2,2.71,0.95,2,2.94,1.04,1,3.07,1.08,1,2.71,0.95,2,2.94,1.04,1,3.07,1.08,1,2.44,0.86,3,2.65,0.94,2,2.76,0.98,2,2.44,0.86,3,2.65,0.94,2,2.76,0.98,2]
["121020050003215","12",65,1962,29.76193907,-95.371749109999996,"steel girder",1.25,0.72,4,1.33,0.77,4,1.51,0.87,3,1.25,0.72,4,1.33,0.77,4,1.51,0.87,3,1.54,0.89,3,1.68,0.97,2,1.93,1.1200000000000001,1,1.54,0.89,3,1.68,0.97,2,1.93,1.1200000000000001,1,1.38,0.8,4,1.51,0.87,3,1.73,1,2,1.38,0.8,4,1.51,0.87,3,1.73,1,2]
["121020050003297","12",110,1992,29.675625050000001,-95.267892380000006,"prestress concrete girder",1.97,0.74,4,2.12,0.79,4,2.14,0.8,4,1.97,0.74,4,2.12,0.79,4,2.14,0.8,4,2.3199999999999998,0.86,3,2.54,0.95,2,2.54,0.95,2,2.3199999999999998,0.86,3,2.54,0.95,2,2.54,0.95,2,2.09,0.77,4,2.2799999999999998,0.85,3,2.2799999999999998,0.85,3,2.09,0.77,4,2.2799999999999998,0.85,3,2.2799999999999998,0.85,3]
["121020050801249","12",80,1990,29.777920170000002,-95.283976510000002,"concrete bridge",1.63,0.49,5,1.63,0.49,5,1.68,0.5,5,1.63,0.49,5,1.63,0.49,5,1.68,0.5,5,1.91,0.56999999999999995,5,1.93,0.57999999999999996,5,2.0299999999999998,0.6,5,1.91,0.56999999999999995,5,1.93,0.57999999999999996,5,2.0299999999999998,0.6,5,1.71,0.51,5,1.73,0.52,5,1.82,0.54,5,1.71,0.51,5,1.73,0.52,5,1.82,0.54,5]
["121700011004135","12",90,1991,30.207143179999999,-95.456317080000005,"prestress concrete girder",2.16,0.8,4,2.17,0.8,4,2.17,0.8,4,2.16,0.8,4,2.17,0.8,4,2.17,0.8,4,2.63,0.98,2,2.63,0.98,2,2.63,0.98,2,2.63,0.98,2,2.63,0.98,2,2.63,0.98,2,2.36,0.88,3,2.36,0.88,3,2.36,0.88,3,2.36,0.88,3,2.36,0.88,3,2.36,0.88,3]
["130900053505158","13",75,1972,29.682866839999999,-97.268354509999995,"prestress concrete girder",2.2599999999999998,0.9,3,2.2599999999999998,0.9,3,2.2599999999999998,0.9,3,2.2599999999999998,0.9,3,2.2599999999999998,0.9,3,2.2599999999999998,0.9,3,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.5099999999999998,1,2,2.5099999999999998,1,2,2.5099999999999998,1,2,2.5099999999999998,1,2,2.5099999999999998,1,2,2.5099999999999998,1,2]
["130900053505161","13",85,1972,29.688805729999999,-97.253199210000005,"prestress concrete girder",2.3199999999999998,0.82,3,2.3199999999999998,0.82,3,2.3199999999999998,0.82,3,2.3199999999999998,0.82,3,2.3199999999999998,0.82,3,2.3199999999999998,0.82,3,2.83,1,2,2.83,1,2,2.83,1,2,2.83,1,2,2.83,1,2,2.83,1,2,2.54,0.89,3,2.54,0.89,3,2.54,0.89,3,2.54,0.89,3,2.54,0.89,3,2.54,0.89,3]
["141060001603132","14",70,1993,29.869318790000001,-97.939022890000004,"prestress concrete girder",2.23,0.83,3,2.23,0.83,3,2.23,0.83,3,2.23,0.83,3,2.23,0.83,3,2.23,0.83,3,2.79,1.04,1,2.79,1.04,1,2.79,1.04,1,2.79,1.04,1,2.79,1.04,1,2.79,1.04,1,2.5,0.93,2,2.5,0.93,2,2.5,0.93,2,2.5,0.93,2,2.5,0.93,2,2.5,0.93,2]
["142270001513385","14",120,1980,30.322037699999999,-97.706849879999993,"prestress concrete girder",1.87,0.79,4,2.04,0.86,3,2.13,0.89,3,1.87,0.79,4,2.04,0.86,3,2.13,0.89,3,2.2200000000000002,0.94,2,2.41,1.01,1,2.5099999999999998,1.05,1,2.2200000000000002,0.94,2,2.41,1.01,1,2.5099999999999998,1.05,1,1.99,0.84,3,2.17,0.91,2,2.2599999999999998,0.95,2,1.99,0.84,3,2.17,0.91,2,2.2599999999999998,0.95,2]
["142460001509684","14",130,2017,30.53566,-97.692267000000001,"concrete bridge",2.2599999999999998,2.2599999999999998,1,2.54,2.54,1,2.69,2.69,1,2.2599999999999998,2.2599999999999998,1,2.54,2.54,1,2.69,2.69,1,2.71,2.71,1,2.96,2.96,1,3.19,3.19,1,2.71,2.71,1,2.96,2.96,1,3.19,3.19,1,2.44,2.44,1,2.66,2.66,1,2.87,2.87,1,2.44,2.44,1,2.66,2.66,1,2.87,2.87,1]
["150150001607169","15",75,1986,29.56688956,-98.334340389999994,"prestress concrete girder",2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2]
["150150001710295","15",130,1972,29.436844870000002,-98.476952679999997,"steel girder",1.7,0.98,2,1.88,1.0900000000000001,1,1.81,1.04,1,1.45,0.84,3,1.54,0.89,3,1.65,0.95,2,2.0499999999999998,1.19,1,2.12,1.22,1,2.02,1.17,1,1.63,0.95,2,1.77,1.02,1,1.9,1.1000000000000001,1,1.84,1.07,1,1.9,1.1000000000000001,1,1.82,1.05,1,1.47,0.85,3,1.59,0.92,2,1.71,0.99,2]
["150150002502179","15",90,1968,29.408840770000001,-98.436817399999995,"steel girder",1.43,0.83,3,1.39,0.8,4,1.4,0.81,3,1.36,0.79,4,1.39,0.8,4,1.4,0.81,3,1.64,0.95,2,1.62,0.94,2,1.64,0.95,2,1.61,0.93,2,1.62,0.94,2,1.64,0.95,2,1.47,0.85,3,1.45,0.84,3,1.47,0.85,3,1.45,0.84,3,1.45,0.84,3,1.47,0.85,3]
["150150007308049","15",120,1969,29.37540688,-98.459525749999997,"steel girder",1.73,1,2,1.76,1.02,1,1.68,0.97,2,1.4,0.81,3,1.53,0.89,3,1.62,0.94,2,2.08,1.2,1,1.96,1.1299999999999999,1,1.89,1.1000000000000001,1,1.59,0.92,2,1.78,1.03,1,1.86,1.07,1,1.86,1.07,1,1.76,1.02,1,1.7,0.98,2,1.43,0.83,3,1.6,0.92,2,1.67,0.97,2]
["150150007308070","15",75,1969,29.330692920000001,-98.41278337,"steel girder",1.29,0.74,4,1.31,0.76,4,1.38,0.8,4,1.29,0.74,4,1.31,0.76,4,1.38,0.8,4,1.53,0.89,3,1.58,0.92,2,1.7,0.98,2,1.53,0.89,3,1.58,0.92,2,1.7,0.98,2,1.37,0.79,4,1.41,0.82,3,1.52,0.88,3,1.37,0.79,4,1.41,0.82,3,1.52,0.88,3]
["150150052105137","15",80,1987,29.320015649999998,-98.516741809999999,"steel girder",1.33,0.77,4,1.33,0.77,4,1.37,0.79,4,1.33,0.77,4,1.33,0.77,4,1.37,0.79,4,1.55,0.89,3,1.57,0.91,2,1.65,0.95,2,1.55,0.89,3,1.57,0.91,2,1.65,0.95,2,1.39,0.8,4,1.41,0.82,3,1.48,0.86,3,1.39,0.8,4,1.41,0.82,3,1.48,0.86,3]
["150950053501064","15",60,1967,29.59917111,-97.939477980000007,"prestress concrete girder",2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.84,1,2,2.84,1,2,2.84,1,2,2.84,1,2,2.84,1,2,2.84,1,2,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3]
["151630002405042","15",75,1994,29.349027299999999,-99.117450030000001,"prestress concrete girder",2.21,0.93,2,2.21,0.93,2,2.21,0.93,2,2.21,0.93,2,2.21,0.93,2,2.21,0.93,2,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.46,1.04,1,2.46,1.04,1,2.46,1.04,1,2.46,1.04,1,2.46,1.04,1,2.46,1.04,1]
["161490007402134","16",90,1971,28.161837160000001,-97.859177270000004,"prestress concrete girder",2.35,0.94,2,2.36,0.94,2,2.36,0.94,2,2.35,0.94,2,2.36,0.94,2,2.36,0.94,2,2.85,1.1399999999999999,1,2.85,1.1399999999999999,1,2.85,1.1399999999999999,1,2.85,1.1399999999999999,1,2.85,1.1399999999999999,1,2.85,1.1399999999999999,1,2.56,1.02,1,2.56,1.02,1,2.56,1.02,1,2.56,1.02,1,2.56,1.02,1,2.56,1.02,1]
["161960037102075","16",105,1986,28.52445367,-97.043666400000006,"prestress concrete girder",2.0099999999999998,0.59,5,2.15,0.64,5,2.15,0.64,5,2.0099999999999998,0.59,5,2.15,0.64,5,2.15,0.64,5,2.39,0.71,4,2.56,0.76,4,2.56,0.76,4,2.39,0.71,4,2.56,0.76,4,2.56,0.76,4,2.15,0.64,5,2.2999999999999998,0.68,5,2.2999999999999998,0.68,5,2.15,0.64,5,2.2999999999999998,0.68,5,2.2999999999999998,0.68,5]
["171540067505082","17",105,1964,31.01406639,-95.922774660000002,"steel girder",1.63,0.95,2,1.55,0.89,3,1.52,0.88,3,1.37,0.79,4,1.49,0.86,3,1.52,0.88,3,1.83,1.06,1,1.76,1.02,1,1.73,1,2,1.6,0.92,2,1.73,1,2,1.73,1,2,1.65,0.95,2,1.58,0.92,2,1.56,0.9,3,1.44,0.83,3,1.56,0.9,3,1.56,0.9,3]
["180570000911486","18",125,2016,32.76859898,-96.803672910000003,"prestress concrete girder",2.29,1.95,1,2.54,2.16,1,2.69,2.29,1,2.2999999999999998,1.95,1,2.54,2.16,1,2.69,2.29,1,2.74,2.33,1,2.98,2.5299999999999998,1,3.17,2.69,1,2.74,2.33,1,2.98,2.5299999999999998,1,3.17,2.69,1,2.4700000000000002,2.1,1,2.68,2.2799999999999998,1,2.85,2.42,1,2.4700000000000002,2.1,1,2.68,2.2799999999999998,1,2.85,2.42,1]
["180570004707389","18",90,1999,32.815704760000003,-96.789164720000002,"prestress concrete girder",2.16,0.91,2,2.17,0.91,2,2.17,0.91,2,2.16,0.91,2,2.17,0.91,2,2.17,0.91,2,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2]
["180570019603161","18",55,1963,32.887840060000002,-96.897856099999998,"prestress concrete girder",2.19,0.88,3,2.19,0.88,3,2.19,0.88,3,2.19,0.88,3,2.19,0.88,3,2.19,0.88,3,2.89,1.1599999999999999,1,2.89,1.1599999999999999,1,2.89,1.1599999999999999,1,2.89,1.1599999999999999,1,2.89,1.1599999999999999,1,2.89,1.1599999999999999,1,2.59,1.04,1,2.59,1.04,1,2.59,1.04,1,2.59,1.04,1,2.59,1.04,1,2.59,1.04,1]
["180570044202348","18",120,2008,32.575038489999997,-96.822582949999997,"prestress concrete girder",2.33,1.98,1,2.5499999999999998,2.17,1,2.66,2.2599999999999998,1,2.33,1.98,1,2.5499999999999998,2.17,1,2.66,2.2599999999999998,1,2.77,2.35,1,3.01,2.56,1,3.14,2.67,1,2.77,2.35,1,3.01,2.56,1,3.14,2.67,1,2.4900000000000002,2.12,1,2.71,2.2999999999999998,1,2.82,2.4,1,2.4900000000000002,2.12,1,2.71,2.2999999999999998,1,2.82,2.4,1]
["180570237401535","18",125,2014,32.911710999999997,-96.881160999999992,"prestress concrete girder",2.29,1.95,1,2.54,2.16,1,2.69,2.29,1,2.2999999999999998,1.95,1,2.54,2.16,1,2.69,2.29,1,2.74,2.33,1,2.98,2.5299999999999998,1,3.17,2.69,1,2.74,2.33,1,2.98,2.5299999999999998,1,3.17,2.69,1,2.4700000000000002,2.1,1,2.68,2.2799999999999998,1,2.85,2.42,1,2.4700000000000002,2.1,1,2.68,2.2799999999999998,1,2.85,2.42,1]
["180570237402328","18",100,1971,32.79272623,-96.624666739999995,"steel girder",1.56,1.02,1,1.49,0.98,2,1.47,0.96,2,1.38,0.9,3,1.47,0.96,2,1.47,0.96,2,1.76,1.1599999999999999,1,1.7,1.1100000000000001,1,1.69,1.1100000000000001,1,1.63,1.07,1,1.7,1.1100000000000001,1,1.69,1.1100000000000001,1,1.58,1.04,1,1.53,1,2,1.52,0.99,2,1.46,0.95,2,1.53,1,2,1.52,0.99,2]
["180570237407347","18",55,1992,32.941372000000001,-97.014452999999989,"prestress concrete girder",1.62,0.68,5,1.88,0.79,4,2.2400000000000002,0.94,2,1.62,0.68,5,1.89,0.8,4,2.2400000000000002,0.94,2,2.11,0.88,3,2.34,0.99,2,2.75,1.1599999999999999,1,2.11,0.88,3,2.35,0.99,2,2.75,1.1599999999999999,1,1.88,0.79,4,2.11,0.88,3,2.48,1.05,1,1.88,0.79,4,2.11,0.88,3,2.48,1.05,1]
["180610008113100","18",45,1969,33.165504050000003,-97.185140250000003,"concrete bridge",2.4,0.85,3,2.4,0.85,3,2.4,0.85,3,2.41,0.85,3,2.4,0.85,3,2.4,0.85,3,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1]
["181300049501159","18",90,1964,32.712527209999998,-96.300689840000004,"steel girder",1.43,0.83,3,1.39,0.8,4,1.4,0.81,3,1.36,0.79,4,1.39,0.8,4,1.4,0.81,3,1.64,0.95,2,1.62,0.94,2,1.64,0.95,2,1.61,0.93,2,1.62,0.94,2,1.64,0.95,2,1.47,0.85,3,1.45,0.84,3,1.47,0.85,3,1.45,0.84,3,1.45,0.84,3,1.47,0.85,3]
["181300049501204","18",75,1965,32.6639354,-96.126882030000004,"steel girder",1.29,0.74,4,1.31,0.76,4,1.38,0.8,4,1.29,0.74,4,1.31,0.76,4,1.38,0.8,4,1.53,0.89,3,1.58,0.92,2,1.7,0.98,2,1.53,0.89,3,1.58,0.92,2,1.7,0.98,2,1.37,0.79,4,1.41,0.82,3,1.52,0.88,3,1.37,0.79,4,1.41,0.82,3,1.52,0.88,3]
["192250061003057","19",50,1965,33.169663849999999,-95.000037239999997,"prestress concrete girder",2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.99,1.2,1,2.99,1.2,1,2.99,1.2,1,2.99,1.2,1,2.99,1.2,1,2.99,1.2,1,2.67,1.06,1,2.67,1.06,1,2.67,1.06,1,2.67,1.06,1,2.67,1.06,1,2.67,1.06,1]
["201460033805212","20",80,2007,30.336543370000001,-95.103057410000005,"prestress concrete girder",2.4500000000000002,1.84,1,2.4500000000000002,1.84,1,2.4500000000000002,1.84,1,2.4500000000000002,1.84,1,2.4500000000000002,1.84,1,2.4500000000000002,1.84,1,3.01,2.2599999999999998,1,3.01,2.2599999999999998,1,3.01,2.2599999999999998,1,3.01,2.2599999999999998,1,3.01,2.2599999999999998,1,3.01,2.2599999999999998,1,2.7,2.0299999999999998,1,2.7,2.0299999999999998,1,2.7,2.0299999999999998,1,2.7,2.0299999999999998,1,2.7,2.0299999999999998,1,2.7,2.0299999999999998,1]
["210310003908239","21",95,2004,25.990468490000001,-97.520783999999992,"prestress concrete girder",2.1,0.88,3,2.16,0.91,2,2.16,0.91,2,2.1,0.88,3,2.16,0.91,2,2.16,0.91,2,2.5499999999999998,1.07,1,2.6,1.1000000000000001,1,2.6,1.1000000000000001,1,2.5499999999999998,1.07,1,2.6,1.1000000000000001,1,2.6,1.1000000000000001,1,2.2999999999999998,0.97,2,2.34,0.99,2,2.34,0.99,2,2.2999999999999998,0.97,2,2.34,0.99,2,2.34,0.99,2]
["211090003918282","21",110,2002,26.19273755,-98.134212700000006,"prestress concrete girder",1.97,0.83,3,2.12,0.89,3,2.14,0.9,3,1.97,0.83,3,2.12,0.89,3,2.14,0.9,3,2.3199999999999998,0.98,2,2.54,1.07,1,2.54,1.07,1,2.3199999999999998,0.98,2,2.54,1.07,1,2.54,1.07,1,2.09,0.88,3,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.09,0.88,3,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2]
["221590030002010","22",45,1953,28.630941199999999,-100.1185222,"concrete bridge",2.4,0.85,3,2.4,0.85,3,2.4,0.85,3,2.41,0.85,3,2.4,0.85,3,2.4,0.85,3,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1]
["240720016701041","24",160,1972,31.770333999999998,-106.44769700000001,"steel girder",1.65,0.95,2,1.79,1.04,1,1.95,1.1299999999999999,1,1.62,0.94,2,1.67,0.97,2,1.71,0.99,2,1.94,1.1200000000000001,1,2.13,1.23,1,2.31,1.34,1,1.86,1.07,1,1.9,1.1000000000000001,1,1.97,1.1399999999999999,1,1.75,1.01,1,1.91,1.1000000000000001,1,2.08,1.2,1,1.68,0.97,2,1.71,0.99,2,1.77,1.02,1]
["240720212104131","24",65,1960,31.519306999999998,-106.131298,"prestress concrete girder",2.21,0.62,5,2.21,0.62,5,2.21,0.62,5,2.21,0.62,5,2.21,0.62,5,2.21,0.62,5,2.81,0.79,4,2.81,0.79,4,2.81,0.79,4,2.81,0.79,4,2.81,0.79,4,2.81,0.79,4,2.52,0.71,4,2.52,0.71,4,2.52,0.71,4,2.52,0.71,4,2.52,0.71,4,2.52,0.71,4]
["240720212104297","24",275,2012,31.70661389,-106.2907611,"Multi Span Long","Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1]
["011170000913464","01",80,2010,33.119150269999999,-96.096550969999996,"prestress concrete girder",2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1]
["021840B00422001","02",120,1993,32.768693999999996,-97.673990500000002,"prestress concrete girder",1.87,0.79,4,2.04,0.86,3,2.13,0.89,3,1.87,0.79,4,2.04,0.86,3,2.13,0.89,3,2.2200000000000002,0.94,2,2.41,1.01,1,2.5099999999999998,1.05,1,2.2200000000000002,0.94,2,2.41,1.01,1,2.5099999999999998,1.05,1,1.99,0.84,3,2.17,0.91,2,2.2599999999999998,0.95,2,1.99,0.84,3,2.17,0.91,2,2.2599999999999998,0.95,2]
["022200000813441","02",125,2002,32.831396999999996,-97.208669,"prestress concrete girder",1.81,0.77,4,2,0.84,3,2.12,0.89,3,1.81,0.77,4,2,0.84,3,2.12,0.89,3,2.16,0.91,2,2.35,0.99,2,2.5,1.05,1,2.16,0.91,2,2.35,0.99,2,2.5,1.05,1,1.95,0.82,3,2.12,0.89,3,2.25,0.94,2,1.95,0.82,3,2.12,0.89,3,2.25,0.94,2]
["022200000816307","02",90,1982,32.686114860000004,-97.464046269999997,"prestress concrete girder",2.16,0.91,2,2.17,0.91,2,2.17,0.91,2,2.16,0.91,2,2.17,0.91,2,2.17,0.91,2,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2]
["022200001416458","02",95,2001,32.862245379999997,-97.314391259999994,"prestress concrete girder",2.1,0.88,3,2.16,0.91,2,2.16,0.91,2,2.1,0.88,3,2.16,0.91,2,2.16,0.91,2,2.5499999999999998,1.07,1,2.6,1.1000000000000001,1,2.6,1.1000000000000001,1,2.5499999999999998,1.07,1,2.6,1.1000000000000001,1,2.6,1.1000000000000001,1,2.2999999999999998,0.97,2,2.34,0.99,2,2.34,0.99,2,2.2999999999999998,0.97,2,2.34,0.99,2,2.34,0.99,2]
["022200001416586","02",140,2016,32.756050000000002,-97.319269999999989,"prestress concrete girder",2.2000000000000002,2.2000000000000002,1,2.46,2.46,1,2.68,2.68,1,2.19,2.19,1,2.46,2.46,1,2.68,2.68,1,2.61,2.61,1,2.92,2.92,1,3.13,3.13,1,2.61,2.61,1,2.92,2.92,1,3.13,3.13,1,2.34,2.34,1,2.62,2.62,1,2.81,2.81,1,2.34,2.34,1,2.62,2.62,1,2.81,2.81,1]
["022200106801327","02",125,2003,32.746658359999998,-97.335923070000007,"prestress concrete girder",1.81,0.77,4,2,0.84,3,2.12,0.89,3,1.81,0.77,4,2,0.84,3,2.12,0.89,3,2.16,0.91,2,2.35,0.99,2,2.5,1.05,1,2.16,0.91,2,2.35,0.99,2,2.5,1.05,1,1.95,0.82,3,2.12,0.89,3,2.25,0.94,2,1.95,0.82,3,2.12,0.89,3,2.25,0.94,2]
["022200106801456","02",130,1999,32.744346929999999,-97.329976130000006,"prestress concrete girder",1.76,0.74,4,1.97,0.83,3,2.1,0.88,3,1.76,0.74,4,1.97,0.83,3,2.1,0.88,3,2.11,0.88,3,2.2999999999999998,0.97,2,2.48,1.05,1,2.11,0.88,3,2.2999999999999998,0.97,2,2.48,1.05,1,1.9,0.8,4,2.0699999999999998,0.87,3,2.23,0.94,2,1.9,0.8,4,2.0699999999999998,0.87,3,2.23,0.94,2]
["022490001307087","02",95,1986,33.239662369999998,-97.600573560000001,"prestress concrete girder",2.1,0.88,3,2.16,0.91,2,2.16,0.91,2,2.1,0.88,3,2.16,0.91,2,2.16,0.91,2,2.5499999999999998,1.07,1,2.6,1.1000000000000001,1,2.6,1.1000000000000001,1,2.5499999999999998,1.07,1,2.6,1.1000000000000001,1,2.6,1.1000000000000001,1,2.2999999999999998,0.97,2,2.34,0.99,2,2.34,0.99,2,2.2999999999999998,0.97,2,2.34,0.99,2,2.34,0.99,2]
["032430004308139","03",85,1970,33.96690925,-98.725534679999996,"prestress concrete girder",2.3199999999999998,0.82,3,2.3199999999999998,0.82,3,2.3199999999999998,0.82,3,2.3199999999999998,0.82,3,2.3199999999999998,0.82,3,2.3199999999999998,0.82,3,2.83,1,2,2.83,1,2,2.83,1,2,2.83,1,2,2.83,1,2,2.83,1,2,2.54,0.89,3,2.54,0.89,3,2.54,0.89,3,2.54,0.89,3,2.54,0.89,3,2.54,0.89,3]
["032440004306072","03",55,1959,34.131565999999999,-99.136998999999989,"steel girder",1.32,0.77,4,1.53,0.89,3,1.82,1.05,1,1.32,0.77,4,1.54,0.89,3,1.82,1.05,1,1.72,0.99,2,1.91,1.1000000000000001,1,2.2400000000000002,1.29,1,1.72,0.99,2,1.91,1.1000000000000001,1,2.2400000000000002,1.29,1,1.53,0.89,3,1.72,0.99,2,2.02,1.17,1,1.53,0.89,3,1.72,0.99,2,2.02,1.17,1]
["040910027511143","04",95,1982,35.213625280000002,-100.72339327,"prestress concrete girder",2.1,0.78,4,2.16,0.8,4,2.16,0.8,4,2.1,0.78,4,2.16,0.8,4,2.16,0.8,4,2.5499999999999998,0.95,2,2.6,0.97,2,2.6,0.97,2,2.5499999999999998,0.95,2,2.6,0.97,2,2.6,0.97,2,2.2999999999999998,0.86,3,2.34,0.87,3,2.34,0.87,3,2.2999999999999998,0.86,3,2.34,0.87,3,2.34,0.87,3]
["041880027501157","04",190,2002,35.192402360000003,-101.8328142,"Multi Span Long",0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1]
["050960006706100","05",100,1982,34.047668639999998,-101.85333004,"prestress concrete girder",1.91,0.71,4,1.83,0.68,5,1.8,0.67,5,1.69,0.63,5,1.8,0.67,5,1.8,0.67,5,2.16,0.8,4,2.09,0.77,4,2.08,0.77,4,2,0.74,4,2.08,0.77,4,2.08,0.77,4,1.94,0.72,4,1.88,0.7,5,1.87,0.7,5,1.8,0.67,5,1.87,0.7,5,1.87,0.7,5]
["061860014002149","06",110,1975,30.879459780000001,-102.46080876000001,"prestress concrete girder",1.97,0.59,5,2.12,0.63,5,2.14,0.64,5,1.97,0.59,5,2.12,0.63,5,2.14,0.64,5,2.3199999999999998,0.69,5,2.54,0.76,4,2.54,0.76,4,2.3199999999999998,0.69,5,2.54,0.76,4,2.54,0.76,4,2.09,0.62,5,2.2799999999999998,0.68,5,2.2799999999999998,0.68,5,2.09,0.62,5,2.2799999999999998,0.68,5,2.2799999999999998,0.68,5]
["061860014005213","06",110,1978,30.8079131,-101.98974676,"prestress concrete girder",1.97,0.59,5,2.12,0.63,5,2.14,0.64,5,1.97,0.59,5,2.12,0.63,5,2.14,0.64,5,2.3199999999999998,0.69,5,2.54,0.76,4,2.54,0.76,4,2.3199999999999998,0.69,5,2.54,0.76,4,2.54,0.76,4,2.09,0.62,5,2.2799999999999998,0.68,5,2.2799999999999998,0.68,5,2.09,0.62,5,2.2799999999999998,0.68,5,2.2799999999999998,0.68,5]
["071340014108151","07",70,1978,30.46975977,-100.11362231,"prestress concrete girder",2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1]
["072260015802065","07",85,2000,31.476554610000001,-100.39835874000001,"prestress concrete girder",2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.39,1,2,2.39,1,2,2.39,1,2,2.39,1,2,2.39,1,2,2.39,1,2]
["080300000701086","08",45,1965,32.391604950000001,-99.345029940000003,"concrete bridge",1.87,0.7,5,2.35,0.87,3,2.42,0.9,3,1.87,0.7,5,2.35,0.87,3,2.42,0.9,3,2.35,0.87,3,2.56,0.95,2,2.56,0.95,2,2.35,0.87,3,2.56,0.95,2,2.56,0.95,2,2.12,0.79,4,2.2999999999999998,0.86,3,2.2999999999999998,0.86,3,2.12,0.79,4,2.2999999999999998,0.86,3,2.2999999999999998,0.86,3]
["081680000601156","08",45,1958,32.409591679999998,-100.69472163,"concrete bridge",1.87,0.79,4,2.35,0.99,2,2.42,1.02,1,1.87,0.79,4,2.35,0.99,2,2.42,1.02,1,2.35,0.99,2,2.56,1.08,1,2.56,1.08,1,2.35,0.99,2,2.56,1.08,1,2.56,1.08,1,2.12,0.89,3,2.2999999999999998,0.97,2,2.2999999999999998,0.97,2,2.12,0.89,3,2.2999999999999998,0.97,2,2.2999999999999998,0.97,2]
["082210003306074","08",75,1964,32.44387777,-99.786744490000004,"steel girder",1.29,0.59,5,1.31,0.61,5,1.38,0.64,5,1.29,0.59,5,1.31,0.61,5,1.38,0.64,5,1.53,0.71,4,1.58,0.73,4,1.7,0.79,4,1.53,0.71,4,1.58,0.73,4,1.7,0.79,4,1.37,0.63,5,1.41,0.65,5,1.52,0.7,5,1.37,0.63,5,1.41,0.65,5,1.52,0.7,5]
["090140001514373","09",100,1977,31.080319999999997,-97.412210000000002,"prestress concrete special",1.91,0.81,0,1.83,0.77,0,1.8,0.76,0,1.69,0.71,0,1.8,0.76,0,1.8,0.76,0,2.16,0.91,0,2.09,0.88,0,2.08,0.88,0,2,0.84,0,2.08,0.88,0,2.08,0.88,0,1.94,0.82,0,1.88,0.79,0,1.87,0.79,0,1.8,0.76,0,1.87,0.79,0,1.87,0.79,0]
["091610001501261","09",80,1991,31.535167340000001,-97.129962559999996,"concrete bridge",1.63,0.49,5,1.63,0.49,5,1.68,0.5,5,1.63,0.49,5,1.63,0.49,5,1.68,0.5,5,1.91,0.56999999999999995,5,1.93,0.57999999999999996,5,2.0299999999999998,0.6,5,1.91,0.56999999999999995,5,1.93,0.57999999999999996,5,2.0299999999999998,0.6,5,1.71,0.51,5,1.73,0.52,5,1.82,0.54,5,1.71,0.51,5,1.73,0.52,5,1.82,0.54,5]
["091610001501636","09",250,2014,31.558244420000001,-97.119094649999994,"Multi Span Long","Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1]
["102340049503076","10",85,1962,32.559363869999999,-95.807835229999995,"steel girder",1.38,0.8,4,1.35,0.78,4,1.38,0.8,4,1.35,0.78,4,1.35,0.78,4,1.38,0.8,4,1.59,0.92,2,1.59,0.92,2,1.64,0.95,2,1.59,0.92,2,1.59,0.92,2,1.64,0.95,2,1.43,0.83,3,1.42,0.82,3,1.47,0.85,3,1.42,0.82,3,1.42,0.82,3,1.47,0.85,3]
["111870017605103","11",85,1980,30.711903209999999,-94.95300245,"prestress concrete girder",2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.39,1,2,2.39,1,2,2.39,1,2,2.39,1,2,2.39,1,2,2.39,1,2]
["121020002713208","12",165,2003,29.721875900000001,-95.493310739999998,"steel weathered girder",1.64,0.95,2,1.79,1.04,1,1.94,1.1200000000000001,1,1.61,0.93,2,1.71,0.99,2,1.73,1,2,1.94,1.1200000000000001,1,2.12,1.22,1,2.2999999999999998,1.33,1,1.91,1.1000000000000001,1,1.93,1.1200000000000001,1,1.99,1.1499999999999999,1,1.74,1.01,1,1.9,1.1000000000000001,1,2.0699999999999998,1.19,1,1.72,0.99,2,1.74,1.01,1,1.79,1.04,1]
["121020005009486","12",190,2016,29.851118999999997,-95.509193999999994,"steel girder",2.1,2.1,1,2.27,2.27,1,2.4500000000000002,2.4500000000000002,1,1.85,1.85,1,2.13,2.13,1,2.44,2.44,1,2.4300000000000002,2.4300000000000002,1,2.63,2.63,1,2.85,2.85,1,2.25,2.25,1,2.5499999999999998,2.5499999999999998,1,2.85,2.85,1,2.19,2.19,1,2.36,2.36,1,2.56,2.56,1,2.02,2.02,1,2.2999999999999998,2.2999999999999998,1,2.56,2.56,1]
["121020017711170","12",125,1995,29.848733169999999,-95.333381299999999,"prestress concrete special",1.81,0.68,0,2,0.74,0,2.12,0.79,0,1.81,0.68,0,2,0.74,0,2.12,0.79,0,2.16,0.8,0,2.35,0.87,0,2.5,0.93,0,2.16,0.8,0,2.35,0.87,0,2.5,0.93,0,1.95,0.73,0,2.12,0.79,0,2.25,0.83,0,1.95,0.73,0,2.12,0.79,0,2.25,0.83,0]
["121020027107578","12",250,2005,29.77972222,-95.450833329999995,"Multi Span Long","Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1]
["121020027115352","12",85,1974,29.709030120000001,-95.268582370000004,"prestress concrete girder",2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.66,0.99,2,2.66,0.99,2,2.66,0.99,2,2.66,0.99,2,2.66,0.99,2,2.66,0.99,2,2.39,0.89,3,2.39,0.89,3,2.39,0.89,3,2.39,0.89,3,2.39,0.89,3,2.39,0.89,3]
["121020027117571","12",120,2014,29.784544,-95.452345260000001,"prestress concrete special",2.33,1.98,0,2.5499999999999998,2.17,0,2.66,2.2599999999999998,0,2.33,1.98,0,2.5499999999999998,2.17,0,2.66,2.2599999999999998,0,2.77,2.35,0,3.01,2.56,0,3.14,2.67,0,2.77,2.35,0,3.01,2.56,0,3.14,2.67,0,2.4900000000000002,2.12,0,2.71,2.2999999999999998,0,2.82,2.4,0,2.4900000000000002,2.12,0,2.71,2.2999999999999998,0,2.82,2.4,0]
["121020050801209","12",120,1954,29.770156,-95.350416999999993,"steel girder",2.23,0.98,2,2.44,1.08,1,2.54,1.1200000000000001,1,2.23,0.98,2,2.44,1.08,1,2.54,1.1200000000000001,1,2.65,1.17,1,2.88,1.27,1,3,1.32,1,2.65,1.17,1,2.88,1.27,1,3,1.32,1,2.38,1.05,1,2.59,1.1399999999999999,1,2.7,1.19,1,2.38,1.05,1,2.59,1.1399999999999999,1,2.7,1.19,1]
["122370005004153","12",235,1994,30.115995999999999,-96.076207999999994,"Multi Span Long",0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1]
["130080027103225","13",70,1966,29.765098890000001,-96.150570810000005,"prestress concrete girder",2.23,0.79,4,2.23,0.79,4,2.23,0.79,4,2.23,0.79,4,2.23,0.79,4,2.23,0.79,4,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3]
["130760053507048","13",45,1967,29.696299239999998,-96.874274049999997,"concrete bridge",2.4,0.85,3,2.4,0.85,3,2.4,0.85,3,2.41,0.85,3,2.4,0.85,3,2.4,0.85,3,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1]
["140280053503126","14",70,1969,29.650821260000001,-97.60231564,"prestress concrete girder",2.23,0.79,4,2.23,0.79,4,2.23,0.79,4,2.23,0.79,4,2.23,0.79,4,2.23,0.79,4,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3]
["142270001513358","14",115,2001,30.286566959999998,-97.724821829999996,"prestress concrete girder",1.93,0.82,3,2.08,0.88,3,2.13,0.89,3,1.93,0.82,3,2.08,0.88,3,2.13,0.89,3,2.27,0.95,2,2.4700000000000002,1.04,1,2.5299999999999998,1.06,1,2.27,0.95,2,2.4700000000000002,1.04,1,2.5299999999999998,1.06,1,2.04,0.86,3,2.23,0.94,2,2.27,0.95,2,2.04,0.86,3,2.23,0.94,2,2.27,0.95,2]
["142460001508486","14",220,2006,30.688475350000001,-97.657619100000005,"Multi Span Long","Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1]
["150150001607172","15",90,1986,29.563441659999999,-98.338332489999999,"prestress concrete girder",2.16,0.91,2,2.17,0.91,2,2.17,0.91,2,2.16,0.91,2,2.17,0.91,2,2.17,0.91,2,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2]
["150150001710390","15",100,2016,29.520616,-98.394437999999994,"prestress concrete girder",2.4300000000000002,2.4300000000000002,1,2.5499999999999998,2.5499999999999998,1,2.5499999999999998,2.5499999999999998,1,2.4300000000000002,2.4300000000000002,1,2.5499999999999998,2.5499999999999998,1,2.5499999999999998,2.5499999999999998,1,2.91,2.91,1,3.05,3.05,1,3.05,3.05,1,2.91,2.91,1,3.05,3.05,1,3.05,3.05,1,2.62,2.62,1,2.74,2.74,1,2.74,2.74,1,2.62,2.62,1,2.74,2.74,1,2.74,2.74,1]
["150150007208156","15",65,1995,29.590205099999999,-98.598265510000004,"prestress concrete girder",2.25,0.83,3,2.25,0.83,3,2.25,0.83,3,2.25,0.83,3,2.25,0.83,3,2.25,0.83,3,2.86,1.07,1,2.86,1.07,1,2.86,1.07,1,2.86,1.07,1,2.86,1.07,1,2.86,1.07,1,2.56,0.95,2,2.56,0.95,2,2.56,0.95,2,2.56,0.95,2,2.56,0.95,2,2.56,0.95,2]
["150150007212300","15",120,2008,29.474780719999998,-98.518131370000006,"prestress concrete girder",2.33,1.98,1,2.5499999999999998,2.17,1,2.66,2.2599999999999998,1,2.33,1.98,1,2.5499999999999998,2.17,1,2.66,2.2599999999999998,1,2.77,2.35,1,3.01,2.56,1,3.14,2.67,1,2.77,2.35,1,3.01,2.56,1,3.14,2.67,1,2.4900000000000002,2.12,1,2.71,2.2999999999999998,1,2.82,2.4,1,2.4900000000000002,2.12,1,2.71,2.2999999999999998,1,2.82,2.4,1]
["150150052104239","15",80,1964,29.520169889999998,-98.396726299999997,"steel girder",1.33,0.77,4,1.33,0.77,4,1.37,0.79,4,1.33,0.77,4,1.33,0.77,4,1.37,0.79,4,1.55,0.89,3,1.57,0.91,2,1.65,0.95,2,1.55,0.89,3,1.57,0.91,2,1.65,0.95,2,1.39,0.8,4,1.41,0.82,3,1.48,0.86,3,1.39,0.8,4,1.41,0.82,3,1.48,0.86,3]
["150150052105049","15",60,1997,29.361034999999998,-98.633043999999998,"steel girder",1.27,0.74,4,1.41,0.82,3,1.66,0.96,2,1.27,0.74,4,1.41,0.82,3,1.66,0.96,2,1.61,0.93,2,1.81,1.04,1,2.06,1.19,1,1.61,0.93,2,1.81,1.04,1,2.06,1.19,1,1.44,0.83,3,1.62,0.94,2,1.85,1.07,1,1.44,0.83,3,1.62,0.94,2,1.85,1.07,1]
["150460001605137","15",65,2006,29.625444900000002,-98.239961999999991,"prestress concrete girder",2.4,2.04,1,2.4,2.04,1,2.4,2.04,1,2.4,2.04,1,2.4,2.04,1,2.4,2.04,1,3.05,2.59,1,3.05,2.59,1,3.05,2.59,1,3.05,2.59,1,3.05,2.59,1,3.05,2.59,1,2.74,2.33,1,2.74,2.33,1,2.74,2.33,1,2.74,2.33,1,2.74,2.33,1,2.74,2.33,1]
["151330014212143","15",45,1974,30.186631819999999,-99.316526820000007,"prestress concrete girder",2.42,0.9,3,2.42,0.9,3,2.42,0.9,3,2.4300000000000002,0.9,3,2.42,0.9,3,2.42,0.9,3,3.23,1.2,1,3.23,1.2,1,3.23,1.2,1,3.23,1.2,1,3.23,1.2,1,3.23,1.2,1,2.92,1.0900000000000001,1,2.92,1.0900000000000001,1,2.92,1.0900000000000001,1,2.92,1.0900000000000001,1,2.92,1.0900000000000001,1,2.92,1.0900000000000001,1]
["160130010101057","16",45,1976,28.276714729999998,-97.692315559999997,"prestress concrete girder",2.42,0.72,4,2.42,0.72,4,2.42,0.72,4,2.4300000000000002,0.72,4,2.42,0.72,4,2.42,0.72,4,3.23,0.96,2,3.23,0.96,2,3.23,0.96,2,3.23,0.96,2,3.23,0.96,2,3.23,0.96,2,2.92,0.87,3,2.92,0.87,3,2.92,0.87,3,2.92,0.87,3,2.92,0.87,3,2.92,0.87,3]
["172390018605054","17",60,1995,30.294074479999999,-96.499871830000004,"prestress concrete girder",2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1]
["180570000911407","18",85,1994,32.780878479999998,-96.77084705,"prestress concrete girder",2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.39,1,2,2.39,1,2,2.39,1,2,2.39,1,2,2.39,1,2,2.39,1,2]
["180570004707364","18",115,1998,32.862603069999999,-96.769850660000003,"prestress concrete girder",2.16,0.91,2,2.06,0.87,3,1.99,0.84,3,1.7,0.71,4,1.86,0.78,4,1.96,0.82,3,2.44,1.03,1,2.3199999999999998,0.98,2,2.25,0.94,2,1.94,0.82,3,2.16,0.91,2,2.2400000000000002,0.94,2,2.19,0.92,2,2.08,0.88,3,2.02,0.85,3,1.75,0.74,4,1.94,0.82,3,2.0099999999999998,0.84,3]
["180570009214229","18",75,1974,32.683922809999999,-96.746237559999997,"prestress concrete girder",2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2]
["180570019603071","18",70,2014,32.938812980000002,-96.902790859999996,"steel girder",1.71,1.45,1,1.77,1.5,1,1.94,1.65,1,1.71,1.45,1,1.78,1.51,1,1.94,1.65,1,2.06,1.75,1,2.1800000000000002,1.85,1,2.4300000000000002,2.0699999999999998,1,2.06,1.75,1,2.1800000000000002,1.85,1,2.4300000000000002,2.0699999999999998,1,1.85,1.57,1,1.96,1.67,1,2.1800000000000002,1.85,1,1.85,1.57,1,1.96,1.67,1,2.1800000000000002,1.85,1]
["180570106804321","18",105,2006,32.767637110000003,-96.835193649999994,"prestress concrete girder",2.41,2.0499999999999998,1,2.57,2.1800000000000002,1,2.57,2.1800000000000002,1,2.41,2.0499999999999998,1,2.57,2.1800000000000002,1,2.57,2.1800000000000002,1,2.87,2.44,1,3.07,2.61,1,3.07,2.61,1,2.87,2.44,1,3.07,2.61,1,3.07,2.61,1,2.58,2.19,1,2.76,2.35,1,2.76,2.35,1,2.58,2.19,1,2.76,2.35,1,2.76,2.35,1]
["180570237401534","18",120,2014,32.924483330000001,-96.841394399999999,"prestress concrete girder",2.33,2.33,1,2.5499999999999998,2.5499999999999998,1,2.66,2.66,1,2.33,2.33,1,2.5499999999999998,2.5499999999999998,1,2.66,2.66,1,2.77,2.77,1,3.01,3.01,1,3.14,3.14,1,2.77,2.77,1,3.01,3.01,1,3.14,3.14,1,2.4900000000000002,2.4900000000000002,1,2.71,2.71,1,2.82,2.82,1,2.4900000000000002,2.4900000000000002,1,2.71,2.71,1,2.82,2.82,1]
["180570237402091","18",100,1969,32.72463922,-96.615318590000001,"steel girder",1.56,0.9,3,1.49,0.86,3,1.47,0.85,3,1.38,0.8,4,1.47,0.85,3,1.47,0.85,3,1.76,1.02,1,1.7,0.98,2,1.69,0.98,2,1.63,0.95,2,1.7,0.98,2,1.69,0.98,2,1.58,0.92,2,1.53,0.89,3,1.52,0.88,3,1.46,0.84,3,1.53,0.89,3,1.52,0.88,3]
["180570237403318","18",175,1971,32.68806343,-96.634471860000005,"steel girder",1.65,0.95,2,1.78,1.03,1,1.92,1.1100000000000001,1,1.57,0.91,2,1.77,1.02,1,1.79,1.04,1,1.93,1.1200000000000001,1,2.1,1.22,1,2.27,1.31,1,1.9,1.1000000000000001,1,2.0099999999999998,1.1599999999999999,1,2.04,1.18,1,1.73,1,2,1.88,1.0900000000000001,1,2.04,1.18,1,1.71,0.99,2,1.81,1.04,1,1.83,1.06,1]
["180610019502065","18",65,1958,33.298853860000001,-97.177798170000003,"steel girder",1.25,0.72,4,1.33,0.77,4,1.51,0.87,3,1.25,0.72,4,1.33,0.77,4,1.51,0.87,3,1.54,0.89,3,1.68,0.97,2,1.93,1.1200000000000001,1,1.54,0.89,3,1.68,0.97,2,1.93,1.1200000000000001,1,1.38,0.8,4,1.51,0.87,3,1.73,1,2,1.38,0.8,4,1.51,0.87,3,1.73,1,2]
["180710004808172","18",125,2007,32.173063460000002,-96.911247279999998,"prestress concrete girder",2.29,1.95,1,2.54,2.16,1,2.69,2.29,1,2.2999999999999998,1.95,1,2.54,2.16,1,2.69,2.29,1,2.74,2.33,1,2.98,2.5299999999999998,1,3.17,2.69,1,2.74,2.33,1,2.98,2.5299999999999998,1,3.17,2.69,1,2.4700000000000002,2.1,1,2.68,2.2799999999999998,1,2.85,2.42,1,2.4700000000000002,2.1,1,2.68,2.2799999999999998,1,2.85,2.42,1]
["181750009206382","18",70,2005,32.182119,-96.472189,"prestress concrete girder",2.42,2.06,1,2.42,2.06,1,2.42,2.06,1,2.42,2.06,1,2.42,2.06,1,2.42,2.06,1,3.03,2.58,1,3.03,2.58,1,3.03,2.58,1,3.03,2.58,1,3.03,2.58,1,3.03,2.58,1,2.71,2.2999999999999998,1,2.71,2.2999999999999998,1,2.71,2.2999999999999998,1,2.71,2.2999999999999998,1,2.71,2.2999999999999998,1,2.71,2.2999999999999998,1]
["190190061007204","19",115,2010,33.470118130000003,-94.043016429999994,"prestress concrete girder",2.38,2.02,1,2.56,2.1800000000000002,1,2.63,2.2400000000000002,1,2.38,2.02,1,2.56,2.1800000000000002,1,2.63,2.2400000000000002,1,2.8,2.38,1,3.05,2.59,1,3.12,2.65,1,2.8,2.38,1,3.05,2.59,1,3.12,2.65,1,2.52,2.14,1,2.75,2.34,1,2.8,2.38,1,2.52,2.14,1,2.75,2.34,1,2.8,2.38,1]
["191030049508266","19",70,1966,32.460023159999999,-94.667557389999999,"prestress concrete girder",2.23,0.89,3,2.23,0.89,3,2.23,0.89,3,2.23,0.89,3,2.23,0.89,3,2.23,0.89,3,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.5099999999999998,1,2,2.5099999999999998,1,2,2.5099999999999998,1,2,2.5099999999999998,1,2,2.5099999999999998,1,2,2.5099999999999998,1,2]
["201810002811270","20",90,2008,30.135845969999998,-94.002336220000004,"prestress concrete girder",2.4900000000000002,2.12,1,2.5,2.13,1,2.5,2.13,1,2.4900000000000002,2.12,1,2.5,2.13,1,2.5,2.13,1,3.02,2.57,1,3.02,2.57,1,3.02,2.57,1,3.02,2.57,1,3.02,2.57,1,3.02,2.57,1,2.72,2.31,1,2.72,2.31,1,2.72,2.31,1,2.72,2.31,1,2.72,2.31,1,2.72,2.31,1]
["210310003908232","21",65,2007,26.06729219,-97.570065720000002,"prestress concrete girder",2.4,2.04,1,2.4,2.04,1,2.4,2.04,1,2.4,2.04,1,2.4,2.04,1,2.4,2.04,1,3.05,2.59,1,3.05,2.59,1,3.05,2.59,1,3.05,2.59,1,3.05,2.59,1,3.05,2.59,1,2.74,2.33,1,2.74,2.33,1,2.74,2.33,1,2.74,2.33,1,2.74,2.33,1,2.74,2.33,1]
["211090003918346","21",115,2005,26.17306524,-97.990588200000005,"prestress concrete girder",2.38,2.02,1,2.56,2.1800000000000002,1,2.63,2.2400000000000002,1,2.38,2.02,1,2.56,2.1800000000000002,1,2.63,2.2400000000000002,1,2.8,2.38,1,3.05,2.59,1,3.12,2.65,1,2.8,2.38,1,3.05,2.59,1,3.12,2.65,1,2.52,2.14,1,2.75,2.34,1,2.8,2.38,1,2.52,2.14,1,2.75,2.34,1,2.8,2.38,1]
["240550000211273","24",80,2010,31.037083590000002,-104.87707731,"prestress concrete girder",2.4500000000000002,1.84,1,2.4500000000000002,1.84,1,2.4500000000000002,1.84,1,2.4500000000000002,1.84,1,2.4500000000000002,1.84,1,2.4500000000000002,1.84,1,3.01,2.2599999999999998,1,3.01,2.2599999999999998,1,3.01,2.2599999999999998,1,3.01,2.2599999999999998,1,3.01,2.2599999999999998,1,3.01,2.2599999999999998,1,2.7,2.0299999999999998,1,2.7,2.0299999999999998,1,2.7,2.0299999999999998,1,2.7,2.0299999999999998,1,2.7,2.0299999999999998,1,2.7,2.0299999999999998,1]
["240720212102174","24",80,1963,31.777165999999998,-106.432793,"steel girder",1.33,0.87,3,1.33,0.87,3,1.37,0.89,3,1.33,0.87,3,1.33,0.87,3,1.37,0.89,3,1.55,1.01,1,1.57,1.03,1,1.65,1.08,1,1.55,1.01,1,1.57,1.03,1,1.65,1.08,1,1.39,0.91,2,1.41,0.93,2,1.48,0.97,2,1.39,0.91,2,1.41,0.93,2,1.48,0.97,2]
["010920004701354","01",90,1991,33.809258450000002,-96.534839849999997,"prestress concrete girder",2.16,0.8,4,2.17,0.8,4,2.17,0.8,4,2.16,0.8,4,2.17,0.8,4,2.17,0.8,4,2.63,0.98,2,2.63,0.98,2,2.63,0.98,2,2.63,0.98,2,2.63,0.98,2,2.63,0.98,2,2.36,0.88,3,2.36,0.88,3,2.36,0.88,3,2.36,0.88,3,2.36,0.88,3,2.36,0.88,3]
["011130061001022","01",65,1963,33.162037400000003,-95.405220909999997,"prestress concrete girder",2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3]
["021820031403125","02",80,1970,32.514980000000001,-98.367719999999991,"prestress concrete girder",2.29,0.81,3,2.29,0.81,3,2.29,0.81,3,2.29,0.81,3,2.29,0.81,3,2.29,0.81,3,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3]
["022200000812333","02",100,1986,32.664635330000003,-97.331862200000003,"prestress concrete girder",2.0499999999999998,0.76,4,2.15,0.8,4,2.15,0.8,4,2.0499999999999998,0.76,4,2.15,0.8,4,2.15,0.8,4,2.46,0.92,2,2.58,0.96,2,2.58,0.96,2,2.46,0.92,2,2.58,0.96,2,2.58,0.96,2,2.2200000000000002,0.83,3,2.3199999999999998,0.86,3,2.3199999999999998,0.86,3,2.2200000000000002,0.83,3,2.3199999999999998,0.86,3,2.3199999999999998,0.86,3]
["022200000813443","02",95,2003,32.778168999999998,-97.212949999999992,"prestress concrete girder",2.1,0.88,3,2.16,0.91,2,2.16,0.91,2,2.1,0.88,3,2.16,0.91,2,2.16,0.91,2,2.5499999999999998,1.07,1,2.6,1.1000000000000001,1,2.6,1.1000000000000001,1,2.5499999999999998,1.07,1,2.6,1.1000000000000001,1,2.6,1.1000000000000001,1,2.2999999999999998,0.97,2,2.34,0.99,2,2.34,0.99,2,2.2999999999999998,0.97,2,2.34,0.99,2,2.34,0.99,2]
["022200000814515","02",125,2014,32.827618000000001,-97.205309,"prestress concrete girder",2.29,1.95,1,2.54,2.16,1,2.69,2.29,1,2.2999999999999998,1.95,1,2.54,2.16,1,2.69,2.29,1,2.74,2.33,1,2.98,2.5299999999999998,1,3.17,2.69,1,2.74,2.33,1,2.98,2.5299999999999998,1,3.17,2.69,1,2.4700000000000002,2.1,1,2.68,2.2799999999999998,1,2.85,2.42,1,2.4700000000000002,2.1,1,2.68,2.2799999999999998,1,2.85,2.42,1]
["022200008112083","02",65,1967,32.933465750000003,-97.315384710000004,"prestress concrete girder",2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3]
["022200106801127","02",50,1998,32.738201889999999,-97.466941419999998,"prestress concrete girder",2.36,0.88,3,2.36,0.88,3,2.36,0.88,3,2.36,0.88,3,2.36,0.88,3,2.36,0.88,3,3.2,1.19,1,3.2,1.19,1,3.2,1.19,1,3.2,1.19,1,3.2,1.19,1,3.2,1.19,1,2.86,1.07,1,2.86,1.07,1,2.86,1.07,1,2.86,1.07,1,2.86,1.07,1,2.86,1.07,1]
["022200106802330","02",125,1983,32.759084020000003,-97.217755929999996,"prestress concrete girder",1.81,0.68,5,2,0.74,4,2.12,0.79,4,1.81,0.68,5,2,0.74,4,2.12,0.79,4,2.16,0.8,4,2.35,0.87,3,2.5,0.93,2,2.16,0.8,4,2.35,0.87,3,2.5,0.93,2,1.95,0.73,4,2.12,0.79,4,2.25,0.83,3,1.95,0.73,4,2.12,0.79,4,2.25,0.83,3]
["022490001306327","02",70,2010,33.387446730000001,-97.720502089999997,"prestress concrete girder",2.42,2.06,1,2.42,2.06,1,2.42,2.06,1,2.42,2.06,1,2.42,2.06,1,2.42,2.06,1,3.03,2.58,1,3.03,2.58,1,3.03,2.58,1,3.03,2.58,1,3.03,2.58,1,3.03,2.58,1,2.71,2.2999999999999998,1,2.71,2.2999999999999998,1,2.71,2.2999999999999998,1,2.71,2.2999999999999998,1,2.71,2.2999999999999998,1,2.71,2.2999999999999998,1]
["031690022403051","03",125,1977,33.553566439999997,-97.863642870000007,"prestress concrete girder",1.81,0.68,5,2,0.74,4,2.12,0.79,4,1.81,0.68,5,2,0.74,4,2.12,0.79,4,2.16,0.8,4,2.35,0.87,3,2.5,0.93,2,2.16,0.8,4,2.35,0.87,3,2.5,0.93,2,1.95,0.73,4,2.12,0.79,4,2.25,0.83,3,1.95,0.73,4,2.12,0.79,4,2.25,0.83,3]
["032430015604097","03",90,1990,33.892108829999998,-98.506987069999994,"prestress concrete girder",2.16,0.91,2,2.17,0.91,2,2.17,0.91,2,2.16,0.91,2,2.17,0.91,2,2.17,0.91,2,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2]
["040330027502053","04",60,1966,35.221018000000001,-101.507079,"concrete bridge",1.55,0.57999999999999996,5,1.73,0.65,5,2.04,0.76,4,1.55,0.57999999999999996,5,1.73,0.65,5,2.04,0.76,4,1.98,0.74,4,2.2200000000000002,0.83,3,2.5299999999999998,0.94,2,1.98,0.74,4,2.2200000000000002,0.83,3,2.5299999999999998,0.94,2,1.77,0.66,5,1.99,0.74,4,2.27,0.84,3,1.77,0.66,5,1.99,0.74,4,2.27,0.84,3]
["041880027501043","04",65,1987,35.192446910000001,-101.77877384999999,"steel girder",1.25,0.72,4,1.33,0.77,4,1.51,0.87,3,1.25,0.72,4,1.33,0.77,4,1.51,0.87,3,1.54,0.89,3,1.68,0.97,2,1.93,1.1200000000000001,1,1.54,0.89,3,1.68,0.97,2,1.93,1.1200000000000001,1,1.38,0.8,4,1.51,0.87,3,1.73,1,2,1.38,0.8,4,1.51,0.87,3,1.73,1,2]
["051520006707079","05",105,1978,33.657690170000002,-101.83650264000001,"prestress concrete girder",2.0099999999999998,0.74,4,1.9,0.71,4,1.86,0.69,5,1.68,0.62,5,1.83,0.68,5,1.86,0.69,5,2.25,0.83,3,2.16,0.8,4,2.13,0.79,4,1.97,0.74,4,2.12,0.79,4,2.13,0.79,4,2.02,0.75,4,1.94,0.72,4,1.91,0.71,4,1.77,0.66,5,1.91,0.71,4,1.91,0.71,4]
["061860014003160","06",65,1975,30.89511731,-102.36906635,"prestress concrete girder",2.25,0.94,2,2.25,0.94,2,2.25,0.94,2,2.25,0.94,2,2.25,0.94,2,2.25,0.94,2,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.56,1.08,1,2.56,1.08,1,2.56,1.08,1,2.56,1.08,1,2.56,1.08,1,2.56,1.08,1]
["061950044109069","06",110,1971,31.049192659999999,-103.97327602,"prestress concrete girder",2.31,0.93,2,2.5,0.99,2,2.5099999999999998,1,2,2.3199999999999998,0.93,2,2.5,0.99,2,2.5099999999999998,1,2,2.73,1.0900000000000001,1,2.99,1.2,1,2.99,1.2,1,2.73,1.0900000000000001,1,2.99,1.2,1,2.99,1.2,1,2.46,0.99,2,2.69,1.07,1,2.69,1.07,1,2.46,0.99,2,2.69,1.07,1,2.69,1.07,1]
["070880006902144","07",100,2003,32.016801559999998,-101.30215483000001,"prestress concrete girder",2.0499999999999998,0.86,3,2.15,0.9,3,2.15,0.9,3,2.0499999999999998,0.86,3,2.15,0.9,3,2.15,0.9,3,2.46,1.04,1,2.58,1.0900000000000001,1,2.58,1.0900000000000001,1,2.46,1.04,1,2.58,1.0900000000000001,1,2.58,1.0900000000000001,1,2.2200000000000002,0.94,2,2.3199999999999998,0.98,2,2.3199999999999998,0.98,2,2.2200000000000002,0.94,2,2.3199999999999998,0.98,2,2.3199999999999998,0.98,2]
["080300000607276","08",70,1964,32.432211959999997,-99.605059990000001,"concrete bridge",1.54,0.56999999999999995,5,1.6,0.59,5,1.75,0.65,5,1.54,0.56999999999999995,5,1.61,0.6,5,1.75,0.65,5,1.87,0.7,5,1.97,0.74,4,2.2000000000000002,0.82,3,1.87,0.7,5,1.97,0.74,4,2.2000000000000002,0.82,3,1.67,0.62,5,1.77,0.66,5,1.97,0.74,4,1.67,0.62,5,1.77,0.66,5,1.97,0.74,4]
["081150000506081","08",50,1959,32.2642983,-101.43235756,"prestress concrete girder",2.2000000000000002,0.62,5,2.2000000000000002,0.62,5,2.2000000000000002,0.62,5,2.2000000000000002,0.62,5,2.2000000000000002,0.62,5,2.2000000000000002,0.62,5,2.99,0.85,3,2.99,0.85,3,2.99,0.85,3,2.99,0.85,3,2.99,0.85,3,2.99,0.85,3,2.67,0.75,4,2.67,0.75,4,2.67,0.75,4,2.67,0.75,4,2.67,0.75,4,2.67,0.75,4]
["081680000601158","08",65,1958,32.406633839999998,-100.68546547,"prestress concrete girder",2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3]
["082210003306313","08",85,1982,32.452623639999999,-99.786113009999994,"steel girder",1.38,0.8,4,1.35,0.78,4,1.38,0.8,4,1.35,0.78,4,1.35,0.78,4,1.38,0.8,4,1.59,0.92,2,1.59,0.92,2,1.64,0.95,2,1.59,0.92,2,1.59,0.92,2,1.64,0.95,2,1.43,0.83,3,1.42,0.82,3,1.47,0.85,3,1.42,0.82,3,1.42,0.82,3,1.47,0.85,3]
["091100004809497","09",120,2006,32.056124179999998,-97.093048780000004,"prestress concrete special",2.33,1.98,0,2.5499999999999998,2.17,0,2.66,2.2599999999999998,0,2.33,1.98,0,2.5499999999999998,2.17,0,2.66,2.2599999999999998,0,2.77,2.35,0,3.01,2.56,0,3.14,2.67,0,2.77,2.35,0,3.01,2.56,0,3.14,2.67,0,2.4900000000000002,2.12,0,2.71,2.2999999999999998,0,2.82,2.4,0,2.4900000000000002,2.12,0,2.71,2.2999999999999998,0,2.82,2.4,0]
["091610025809095","09",100,2007,31.50852343,-97.103870580000006,"prestress concrete girder",2.4300000000000002,2.0699999999999998,1,2.5499999999999998,2.17,1,2.5499999999999998,2.17,1,2.4300000000000002,2.0699999999999998,1,2.5499999999999998,2.17,1,2.5499999999999998,2.17,1,2.91,2.4700000000000002,1,3.05,2.59,1,3.05,2.59,1,2.91,2.4700000000000002,1,3.05,2.59,1,3.05,2.59,1,2.62,2.23,1,2.74,2.33,1,2.74,2.33,1,2.62,2.23,1,2.74,2.33,1,2.74,2.33,1]
["102340049502306","10",70,1963,32.632533780000003,-96.02189808,"steel girder",1.26,0.57999999999999996,5,1.31,0.61,5,1.43,0.66,5,1.26,0.57999999999999996,5,1.31,0.61,5,1.43,0.66,5,1.52,0.7,5,1.61,0.74,4,1.79,0.83,3,1.52,0.7,5,1.61,0.74,4,1.79,0.83,3,1.36,0.63,5,1.44,0.67,5,1.61,0.74,4,1.36,0.63,5,1.44,0.67,5,1.61,0.74,4]
["120800002712289","12",130,2000,29.638737079999999,-95.581443719999996,"prestress concrete girder",1.76,0.74,4,1.97,0.83,3,2.1,0.88,3,1.76,0.74,4,1.97,0.83,3,2.1,0.88,3,2.11,0.88,3,2.2999999999999998,0.97,2,2.48,1.05,1,2.11,0.88,3,2.2999999999999998,0.97,2,2.48,1.05,1,1.9,0.8,4,2.0699999999999998,0.87,3,2.23,0.94,2,1.9,0.8,4,2.0699999999999998,0.87,3,2.23,0.94,2]
["121020002713237","12",115,1992,29.700455730000002,-95.517797540000004,"prestress concrete girder",1.93,0.72,4,2.08,0.77,4,2.13,0.79,4,1.93,0.72,4,2.08,0.77,4,2.13,0.79,4,2.27,0.84,3,2.4700000000000002,0.92,2,2.5299999999999998,0.94,2,2.27,0.84,3,2.4700000000000002,0.92,2,2.5299999999999998,0.94,2,2.04,0.76,4,2.23,0.83,3,2.27,0.84,3,2.04,0.76,4,2.23,0.83,3,2.27,0.84,3]
["121020005009089","12",75,1988,29.859566709999999,-95.524357670000001,"prestress concrete girder",2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2]
["121020017707210","12",125,1997,29.981966750000002,-95.277078619999997,"prestress concrete special",1.81,0.77,0,2,0.84,0,2.12,0.89,0,1.81,0.77,0,2,0.84,0,2.12,0.89,0,2.16,0.91,0,2.35,0.99,0,2.5,1.05,0,2.16,0.91,0,2.35,0.99,0,2.5,1.05,0,1.95,0.82,0,2.12,0.89,0,2.25,0.94,0,1.95,0.82,0,2.12,0.89,0,2.25,0.94,0]
["121020027106686","12",125,2013,29.782124999999997,-95.777147220000003,"prestress concrete special",2.29,1.95,0,2.54,2.16,0,2.69,2.29,0,2.2999999999999998,1.95,0,2.54,2.16,0,2.69,2.29,0,2.74,2.33,0,2.98,2.5299999999999998,0,3.17,2.69,0,2.74,2.33,0,2.98,2.5299999999999998,0,3.17,2.69,0,2.4700000000000002,2.1,0,2.68,2.2799999999999998,0,2.85,2.42,0,2.4700000000000002,2.1,0,2.68,2.2799999999999998,0,2.85,2.42,0]
["121020027115354","12",150,1974,29.70997109,-95.267176329999998,"steel girder",1.65,0.95,2,1.81,1.04,1,1.97,1.1399999999999999,1,1.6,0.92,2,1.61,0.93,2,1.67,0.97,2,1.97,1.1399999999999999,1,2.16,1.24,1,2.34,1.35,1,1.77,1.02,1,1.83,1.06,1,1.95,1.1299999999999999,1,1.77,1.02,1,1.94,1.1200000000000001,1,2.1,1.22,1,1.59,0.92,2,1.65,0.95,2,1.75,1.01,1]
["121020027117561","12",245,2006,29.782677899999999,-95.451767329999996,"Multi Span Long","Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1,"Inf",1,1]
["121020050003281","12",145,1988,29.74219261,-95.357659830000003,"steel weathered girder",1.66,1.0900000000000001,1,1.83,1.2,1,1.99,1.3,1,1.56,1.02,1,1.59,1.04,1,1.66,1.0900000000000001,1,1.98,1.29,1,2.1800000000000002,1.43,1,2.2599999999999998,1.48,1,1.73,1.1299999999999999,1,1.81,1.18,1,1.95,1.28,1,1.78,1.1599999999999999,1,1.96,1.28,1,2.0299999999999998,1.33,1,1.55,1.01,1,1.63,1.07,1,1.75,1.1499999999999999,1]
["121020050801150","12",50,1985,29.773059119999999,-95.232993149999999,"prestress concrete girder",2.36,0.88,3,2.36,0.88,3,2.36,0.88,3,2.36,0.88,3,2.36,0.88,3,2.36,0.88,3,3.2,1.19,1,3.2,1.19,1,3.2,1.19,1,3.2,1.19,1,3.2,1.19,1,3.2,1.19,1,2.86,1.07,1,2.86,1.07,1,2.86,1.07,1,2.86,1.07,1,2.86,1.07,1,2.86,1.07,1]
["121020050801455","12",50,1990,29.776989149999999,-95.272037190000006,"concrete bridge",1.75,0.65,5,2.04,0.76,4,2.37,0.88,3,1.75,0.65,5,2.04,0.76,4,2.37,0.88,3,2.2200000000000002,0.83,3,2.5299999999999998,0.94,2,2.77,1.03,1,2.2200000000000002,0.83,3,2.5299999999999998,0.94,2,2.77,1.03,1,1.99,0.74,4,2.2799999999999998,0.85,3,2.5,0.93,2,1.99,0.74,4,2.2799999999999998,0.85,3,2.5,0.93,2]
["121700067508237","12",120,2012,30.455764420000001,-95.495502830000007,"prestress concrete girder",2.33,1.98,1,2.5499999999999998,2.17,1,2.66,2.2599999999999998,1,2.33,1.98,1,2.5499999999999998,2.17,1,2.66,2.2599999999999998,1,2.77,2.35,1,3.01,2.56,1,3.14,2.67,1,2.77,2.35,1,3.01,2.56,1,3.14,2.67,1,2.4900000000000002,2.12,1,2.71,2.2999999999999998,1,2.82,2.4,1,2.4900000000000002,2.12,1,2.71,2.2999999999999998,1,2.82,2.4,1]
["122370027104253","12",50,1967,29.778850250000001,-95.951347819999995,"prestress concrete girder",2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.99,1.06,1,2.99,1.06,1,2.99,1.06,1,2.99,1.06,1,2.99,1.06,1,2.99,1.06,1,2.67,0.94,2,2.67,0.94,2,2.67,0.94,2,2.67,0.94,2,2.67,0.94,2,2.67,0.94,2]
["132410008906086","13",80,1970,29.174302440000002,-96.302737250000007,"prestress concrete girder",2.29,0.81,3,2.29,0.81,3,2.29,0.81,3,2.29,0.81,3,2.29,0.81,3,2.29,0.81,3,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3]
["142460044001240","14",100,2014,30.844166999999999,-97.786389,"prestress concrete girder",2.4300000000000002,2.0699999999999998,1,2.5499999999999998,2.17,1,2.5499999999999998,2.17,1,2.4300000000000002,2.0699999999999998,1,2.5499999999999998,2.17,1,2.5499999999999998,2.17,1,2.91,2.4700000000000002,1,3.05,2.59,1,3.05,2.59,1,2.91,2.4700000000000002,1,3.05,2.59,1,3.05,2.59,1,2.62,2.23,1,2.74,2.33,1,2.74,2.33,1,2.62,2.23,1,2.74,2.33,1,2.74,2.33,1]
["150150001709139","15",80,1989,29.336975949999999,-98.566830280000005,"steel girder",1.33,0.77,4,1.33,0.77,4,1.37,0.79,4,1.33,0.77,4,1.33,0.77,4,1.37,0.79,4,1.55,0.89,3,1.57,0.91,2,1.65,0.95,2,1.55,0.89,3,1.57,0.91,2,1.65,0.95,2,1.39,0.8,4,1.41,0.82,3,1.48,0.86,3,1.39,0.8,4,1.41,0.82,3,1.48,0.86,3]
["150150001710355","15",110,1988,29.40483867,-98.510345180000002,"prestress concrete girder",1.97,0.74,4,2.12,0.79,4,2.14,0.8,4,1.97,0.74,4,2.12,0.79,4,2.14,0.8,4,2.3199999999999998,0.86,3,2.54,0.95,2,2.54,0.95,2,2.3199999999999998,0.86,3,2.54,0.95,2,2.54,0.95,2,2.09,0.77,4,2.2799999999999998,0.85,3,2.2799999999999998,0.85,3,2.09,0.77,4,2.2799999999999998,0.85,3,2.2799999999999998,0.85,3]
["150150002502110","15",45,1962,29.472255919999998,-98.269910609999997,"concrete bridge",2.4,0.85,3,2.4,0.85,3,2.4,0.85,3,2.41,0.85,3,2.4,0.85,3,2.4,0.85,3,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1]
["150150007208254","15",120,1992,29.604429,-98.601732999999996,"prestress concrete girder",1.87,0.79,4,2.04,0.86,3,2.13,0.89,3,1.87,0.79,4,2.04,0.86,3,2.13,0.89,3,2.2200000000000002,0.94,2,2.41,1.01,1,2.5099999999999998,1.05,1,2.2200000000000002,0.94,2,2.41,1.01,1,2.5099999999999998,1.05,1,1.99,0.84,3,2.17,0.91,2,2.2599999999999998,0.95,2,1.99,0.84,3,2.17,0.91,2,2.2599999999999998,0.95,2]
["150150007308038","15",85,1967,29.395589080000001,-98.478660340000005,"steel girder",1.38,0.8,4,1.35,0.78,4,1.38,0.8,4,1.35,0.78,4,1.35,0.78,4,1.38,0.8,4,1.59,0.92,2,1.59,0.92,2,1.64,0.95,2,1.59,0.92,2,1.59,0.92,2,1.64,0.95,2,1.43,0.83,3,1.42,0.82,3,1.47,0.85,3,1.42,0.82,3,1.42,0.82,3,1.47,0.85,3]
["150150052104262","15",60,1988,29.435717,-98.644261,"prestress concrete girder",2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1]
["150150052104374","15",105,2008,29.518440999999999,-98.468367000000001,"prestress concrete girder",2.41,2.0499999999999998,1,2.57,2.1800000000000002,1,2.57,2.1800000000000002,1,2.41,2.0499999999999998,1,2.57,2.1800000000000002,1,2.57,2.1800000000000002,1,2.87,2.44,1,3.07,2.61,1,3.07,2.61,1,2.87,2.44,1,3.07,2.61,1,3.07,2.61,1,2.58,2.19,1,2.76,2.35,1,2.76,2.35,1,2.58,2.19,1,2.76,2.35,1,2.76,2.35,1]
["150950053501028","15",95,1966,29.571368570000001,-98.014484539999998,"steel girder",1.49,0.69,5,1.44,0.67,5,1.43,0.66,5,1.38,0.64,5,1.44,0.67,5,1.43,0.66,5,1.7,0.79,4,1.66,0.77,4,1.66,0.77,4,1.61,0.74,4,1.66,0.77,4,1.66,0.77,4,1.53,0.71,4,1.49,0.69,5,1.49,0.69,5,1.45,0.67,5,1.49,0.69,5,1.49,0.69,5]
["151330014214120","15",65,1972,30.11716285,-99.201961330000003,"prestress concrete girder",2.21,0.88,3,2.21,0.88,3,2.21,0.88,3,2.21,0.88,3,2.21,0.88,3,2.21,0.88,3,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.52,1,2,2.52,1,2,2.52,1,2,2.52,1,2,2.52,1,2,2.52,1,2]
["161490007402144","16",95,1971,28.24566338,-97.917663709999999,"prestress concrete girder",2.33,0.94,2,2.39,0.95,2,2.39,0.95,2,2.33,0.94,2,2.39,0.95,2,2.39,0.95,2,2.83,1.1299999999999999,1,2.88,1.1499999999999999,1,2.88,1.1499999999999999,1,2.83,1.1299999999999999,1,2.88,1.1499999999999999,1,2.88,1.1499999999999999,1,2.5499999999999998,1.02,1,2.59,1.04,1,2.59,1.04,1,2.5499999999999998,1.02,1,2.59,1.04,1,2.59,1.04,1]
["161490007402160","16",45,1972,28.26161068,-97.930270999999991,"concrete bridge",2.4,0.85,3,2.4,0.85,3,2.4,0.85,3,2.41,0.85,3,2.4,0.85,3,2.4,0.85,3,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1]
["171450067503151","17",60,1987,31.4110838,-96.042195550000002,"prestress concrete girder",2.2799999999999998,0.85,3,2.2799999999999998,0.85,3,2.2799999999999998,0.85,3,2.2799999999999998,0.85,3,2.2799999999999998,0.85,3,2.2799999999999998,0.85,3,2.94,1.1000000000000001,1,2.94,1.1000000000000001,1,2.94,1.1000000000000001,1,2.94,1.1000000000000001,1,2.94,1.1000000000000001,1,2.94,1.1000000000000001,1,2.64,0.98,2,2.64,0.98,2,2.64,0.98,2,2.64,0.98,2,2.64,0.98,2,2.64,0.98,2]
["180570000911253","18",60,1963,32.788581100000002,-96.764149689999996,"prestress concrete girder",2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.84,1,2,2.84,1,2,2.84,1,2,2.84,1,2,2.84,1,2,2.84,1,2,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3]
["180570004707243","18",175,1983,32.791719999999998,-96.792783,"steel girder",1.65,1.08,1,1.78,1.1599999999999999,1,1.92,1.26,1,1.57,1.03,1,1.77,1.1599999999999999,1,1.79,1.17,1,1.93,1.27,1,2.1,1.38,1,2.27,1.49,1,1.9,1.24,1,2.0099999999999998,1.32,1,2.04,1.33,1,1.73,1.1299999999999999,1,1.88,1.23,1,2.04,1.33,1,1.71,1.1200000000000001,1,1.81,1.18,1,1.83,1.2,1]
["180570009214210","18",85,1973,32.787165770000001,-96.792146310000007,"steel girder",1.38,0.9,3,1.35,0.88,3,1.38,0.9,3,1.35,0.88,3,1.35,0.88,3,1.38,0.9,3,1.59,1.04,1,1.59,1.04,1,1.64,1.07,1,1.59,1.04,1,1.59,1.04,1,1.64,1.07,1,1.43,0.94,2,1.42,0.93,2,1.47,0.96,2,1.42,0.93,2,1.42,0.93,2,1.47,0.96,2]
["180570044202027","18",80,1999,32.734473979999997,-96.823814049999996,"steel girder",1.33,0.77,4,1.33,0.77,4,1.37,0.79,4,1.33,0.77,4,1.33,0.77,4,1.37,0.79,4,1.55,0.89,3,1.57,0.91,2,1.65,0.95,2,1.55,0.89,3,1.57,0.91,2,1.65,0.95,2,1.39,0.8,4,1.41,0.82,3,1.48,0.86,3,1.39,0.8,4,1.41,0.82,3,1.48,0.86,3]
["180570237401469","18",115,2003,32.920551840000002,-96.748177519999999,"prestress concrete special",1.93,0.82,0,2.08,0.88,0,2.13,0.89,0,1.93,0.82,0,2.08,0.88,0,2.13,0.89,0,2.27,0.95,0,2.4700000000000002,1.04,0,2.5299999999999998,1.06,0,2.27,0.95,0,2.4700000000000002,1.04,0,2.5299999999999998,1.06,0,2.04,0.86,0,2.23,0.94,0,2.27,0.95,0,2.04,0.86,0,2.23,0.94,0,2.27,0.95,0]
["180570237402076","18",100,1967,32.855946109999998,-96.648285990000005,"steel girder",1.56,0.9,3,1.49,0.86,3,1.47,0.85,3,1.38,0.8,4,1.47,0.85,3,1.47,0.85,3,1.76,1.02,1,1.7,0.98,2,1.69,0.98,2,1.63,0.95,2,1.7,0.98,2,1.69,0.98,2,1.58,0.92,2,1.53,0.89,3,1.52,0.88,3,1.46,0.84,3,1.53,0.89,3,1.52,0.88,3]
["180570237402420","18",80,1987,32.704209999999996,-96.622807359999996,"concrete bridge",1.63,0.69,5,1.63,0.69,5,1.68,0.71,4,1.63,0.69,5,1.63,0.69,5,1.68,0.71,4,1.91,0.81,3,1.93,0.82,3,2.0299999999999998,0.85,3,1.91,0.81,3,1.93,0.82,3,2.0299999999999998,0.85,3,1.71,0.72,4,1.73,0.73,4,1.82,0.77,4,1.71,0.72,4,1.73,0.73,4,1.82,0.77,4]
["180570237403166","18",65,1970,32.680217669999998,-96.670747379999995,"prestress concrete girder",2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3]
["180570237403167","18",65,1970,32.679355139999998,-96.672352540000006,"prestress concrete girder",2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3]
["180570237403186","18",155,1974,32.642690760000001,-96.819657950000007,"steel girder",1.65,0.95,2,1.8,1.04,1,1.96,1.1299999999999999,1,1.63,0.95,2,1.64,0.95,2,1.69,0.98,2,1.96,1.1299999999999999,1,2.15,1.24,1,2.33,1.34,1,1.81,1.04,1,1.86,1.07,1,1.96,1.1299999999999999,1,1.76,1.02,1,1.93,1.1200000000000001,1,2.1,1.22,1,1.63,0.95,2,1.68,0.97,2,1.76,1.02,1]
["180570237403192","18",310,1971,32.67825157,-96.68547658,"Multi Span Long",0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1]
["180570237403193","18",310,1971,32.676769280000002,-96.693061900000004,"Multi Span Long",0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1]
["180570237403215","18",70,1973,32.663696229999999,-96.721253399999995,"prestress concrete girder",2.23,0.79,4,2.23,0.79,4,2.23,0.79,4,2.23,0.79,4,2.23,0.79,4,2.23,0.79,4,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.8,0.99,2,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3,2.5099999999999998,0.89,3]
["180570237403303","18",105,1973,32.663681670000003,-96.722262999999998,"steel girder",1.63,0.95,2,1.55,0.89,3,1.52,0.88,3,1.37,0.79,4,1.49,0.86,3,1.52,0.88,3,1.83,1.06,1,1.76,1.02,1,1.73,1,2,1.6,0.92,2,1.73,1,2,1.73,1,2,1.65,0.95,2,1.58,0.92,2,1.56,0.9,3,1.44,0.83,3,1.56,0.9,3,1.56,0.9,3]
["180570237404219","18",105,1974,32.653746159999997,-96.877945229999995,"steel girder",1.63,0.95,2,1.55,0.89,3,1.52,0.88,3,1.37,0.79,4,1.49,0.86,3,1.52,0.88,3,1.83,1.06,1,1.76,1.02,1,1.73,1,2,1.6,0.92,2,1.73,1,2,1.73,1,2,1.65,0.95,2,1.58,0.92,2,1.56,0.9,3,1.44,0.83,3,1.56,0.9,3,1.56,0.9,3]
["180570237404229","18",100,1974,32.645575870000002,-96.857202060000006,"prestress concrete girder",2.0499999999999998,0.76,4,2.15,0.8,4,2.15,0.8,4,2.0499999999999998,0.76,4,2.15,0.8,4,2.15,0.8,4,2.46,0.92,2,2.58,0.96,2,2.58,0.96,2,2.46,0.92,2,2.58,0.96,2,2.58,0.96,2,2.2200000000000002,0.83,3,2.3199999999999998,0.86,3,2.3199999999999998,0.86,3,2.2200000000000002,0.83,3,2.3199999999999998,0.86,3,2.3199999999999998,0.86,3]
["180570237404249","18",100,1974,32.672546160000003,-96.985005830000006,"prestress concrete girder",2.0499999999999998,0.76,4,2.15,0.8,4,2.15,0.8,4,2.0499999999999998,0.76,4,2.15,0.8,4,2.15,0.8,4,2.46,0.92,2,2.58,0.96,2,2.58,0.96,2,2.46,0.92,2,2.58,0.96,2,2.58,0.96,2,2.2200000000000002,0.83,3,2.3199999999999998,0.86,3,2.3199999999999998,0.86,3,2.2200000000000002,0.83,3,2.3199999999999998,0.86,3,2.3199999999999998,0.86,3]
["180570237407344","18",85,1992,32.947283999999996,-97.026749999999993,"prestress concrete girder",2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.66,0.99,2,2.66,0.99,2,2.66,0.99,2,2.66,0.99,2,2.66,0.99,2,2.66,0.99,2,2.39,0.89,3,2.39,0.89,3,2.39,0.89,3,2.39,0.89,3,2.39,0.89,3,2.39,0.89,3]
["180570237407386","18",105,2014,32.907319389999998,-96.910741569999999,"prestress concrete girder",2.41,1.81,1,2.57,1.93,1,2.57,1.93,1,2.41,1.81,1,2.57,1.93,1,2.57,1.93,1,2.87,2.15,1,3.07,2.2999999999999998,1,3.07,2.2999999999999998,1,2.87,2.15,1,3.07,2.2999999999999998,1,3.07,2.2999999999999998,1,2.58,1.94,1,2.76,2.0699999999999998,1,2.76,2.0699999999999998,1,2.58,1.94,1,2.76,2.0699999999999998,1,2.76,2.0699999999999998,1]
["180570237407448","18",120,2001,32.918546110000001,-96.975276699999995,"prestress concrete girder",1.87,0.79,4,2.04,0.86,3,2.13,0.89,3,1.87,0.79,4,2.04,0.86,3,2.13,0.89,3,2.2200000000000002,0.94,2,2.41,1.01,1,2.5099999999999998,1.05,1,2.2200000000000002,0.94,2,2.41,1.01,1,2.5099999999999998,1.05,1,1.99,0.84,3,2.17,0.91,2,2.2599999999999998,0.95,2,1.99,0.84,3,2.17,0.91,2,2.2599999999999998,0.95,2]
["180610008113099","18",80,1969,33.171743910000004,-97.181263139999999,"prestress concrete girder",2.29,0.65,5,2.29,0.65,5,2.29,0.65,5,2.29,0.65,5,2.29,0.65,5,2.29,0.65,5,2.81,0.79,4,2.81,0.79,4,2.81,0.79,4,2.81,0.79,4,2.81,0.79,4,2.81,0.79,4,2.52,0.71,4,2.52,0.71,4,2.52,0.71,4,2.52,0.71,4,2.52,0.71,4,2.52,0.71,4]
["180610019503090","18",85,2016,33.191507999999999,-97.114564000000001,"steel girder",1.86,1.86,1,1.83,1.83,1,1.86,1.86,1,1.82,1.82,1,1.83,1.83,1,1.86,1.86,1,2.15,2.15,1,2.14,2.14,1,2.21,2.21,1,2.14,2.14,1,2.14,2.14,1,2.21,2.21,1,1.93,1.93,1,1.93,1.93,1,1.99,1.99,1,1.92,1.92,1,1.93,1.93,1,1.99,1.99,1]
["180610019503144","18",85,2001,33.195859069999997,-97.13602247,"prestress concrete girder",2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.39,1,2,2.39,1,2,2.39,1,2,2.39,1,2,2.39,1,2,2.39,1,2]
["180610019602304","18",65,1995,32.990460999999996,-96.94338599999999,"prestress concrete girder",2.25,0.94,2,2.25,0.94,2,2.25,0.94,2,2.25,0.94,2,2.25,0.94,2,2.25,0.94,2,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.56,1.08,1,2.56,1.08,1,2.56,1.08,1,2.56,1.08,1,2.56,1.08,1,2.56,1.08,1]
["180610019602308","18",80,2006,32.997552999999996,-96.954584999999994,"prestress concrete girder",2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1]
["180610019602373","18",135,2006,32.995151,-96.96479699999999,"prestress concrete girder",2.23,1.9,1,2.4900000000000002,2.12,1,2.68,2.2799999999999998,1,2.23,1.9,1,2.4900000000000002,2.12,1,2.68,2.2799999999999998,1,2.65,2.25,1,2.94,2.5,1,3.15,2.68,1,2.65,2.25,1,2.94,2.5,1,3.15,2.68,1,2.39,2.0299999999999998,1,2.65,2.25,1,2.84,2.41,1,2.39,2.0299999999999998,1,2.65,2.25,1,2.84,2.41,1]
["180610036403106","18",130,2009,33.059676750000001,-96.901671109999995,"prestress concrete girder",2.2599999999999998,1.92,1,2.54,2.16,1,2.69,2.29,1,2.2599999999999998,1.92,1,2.54,2.16,1,2.69,2.29,1,2.71,2.2999999999999998,1,2.96,2.52,1,3.19,2.71,1,2.71,2.2999999999999998,1,2.96,2.52,1,3.19,2.71,1,2.44,2.0699999999999998,1,2.66,2.2599999999999998,1,2.87,2.44,1,2.44,2.0699999999999998,1,2.66,2.2599999999999998,1,2.87,2.44,1]
["180610354701014","18",115,1999,33.012253029999997,-96.943055900000004,"prestress concrete girder",1.93,0.82,3,2.08,0.88,3,2.13,0.89,3,1.93,0.82,3,2.08,0.88,3,2.13,0.89,3,2.27,0.95,2,2.4700000000000002,1.04,1,2.5299999999999998,1.06,1,2.27,0.95,2,2.4700000000000002,1.04,1,2.5299999999999998,1.06,1,2.04,0.86,3,2.23,0.94,2,2.27,0.95,2,2.04,0.86,3,2.23,0.94,2,2.27,0.95,2]
["180710004808170","18",80,2006,32.137406999999996,-96.950015999999991,"prestress concrete girder",2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1]
["180710004808174","18",90,2007,32.177126620000003,-96.909293430000005,"prestress concrete girder",2.4900000000000002,2.12,1,2.5,2.13,1,2.5,2.13,1,2.4900000000000002,2.12,1,2.5,2.13,1,2.5,2.13,1,3.02,2.57,1,3.02,2.57,1,3.02,2.57,1,3.02,2.57,1,3.02,2.57,1,3.02,2.57,1,2.72,2.31,1,2.72,2.31,1,2.72,2.31,1,2.72,2.31,1,2.72,2.31,1,2.72,2.31,1]
["180710009203285","18",90,1993,32.467932580000003,-96.661506180000003,"prestress concrete girder",2.16,0.91,2,2.17,0.91,2,2.17,0.91,2,2.16,0.91,2,2.17,0.91,2,2.17,0.91,2,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2]
["180710009203286","18",85,1995,32.46828421,-96.661502749999997,"prestress concrete girder",2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.1800000000000002,0.92,2,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.66,1.1200000000000001,1,2.39,1,2,2.39,1,2,2.39,1,2,2.39,1,2,2.39,1,2,2.39,1,2]
["180710009204333","18",95,1996,32.359375649999997,-96.631876410000004,"prestress concrete girder",2.1,0.88,3,2.16,0.91,2,2.16,0.91,2,2.1,0.88,3,2.16,0.91,2,2.16,0.91,2,2.5499999999999998,1.07,1,2.6,1.1000000000000001,1,2.6,1.1000000000000001,1,2.5499999999999998,1.07,1,2.6,1.1000000000000001,1,2.6,1.1000000000000001,1,2.2999999999999998,0.97,2,2.34,0.99,2,2.34,0.99,2,2.2999999999999998,0.97,2,2.34,0.99,2,2.34,0.99,2]
["180710009205335","18",80,1998,32.310514959999999,-96.596867770000003,"prestress concrete girder",2.19,0.81,3,2.19,0.81,3,2.19,0.81,3,2.2000000000000002,0.82,3,2.2000000000000002,0.82,3,2.2000000000000002,0.82,3,2.7,1.01,1,2.7,1.01,1,2.7,1.01,1,2.7,1.01,1,2.7,1.01,1,2.7,1.01,1,2.42,0.9,3,2.42,0.9,3,2.42,0.9,3,2.42,0.9,3,2.42,0.9,3,2.42,0.9,3]
["180710009205336","18",80,1996,32.324684660000003,-96.608845349999996,"prestress concrete girder",2.19,0.92,2,2.19,0.92,2,2.19,0.92,2,2.2000000000000002,0.93,2,2.2000000000000002,0.93,2,2.2000000000000002,0.93,2,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1]
["180710044203413","18",75,1999,32.531828359999999,-96.822098460000007,"prestress concrete girder",2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2]
["181300009514352","18",95,1987,32.69930179,-96.452526759999998,"prestress concrete girder",2.1,0.78,4,2.16,0.8,4,2.16,0.8,4,2.1,0.78,4,2.16,0.8,4,2.16,0.8,4,2.5499999999999998,0.95,2,2.6,0.97,2,2.6,0.97,2,2.5499999999999998,0.95,2,2.6,0.97,2,2.6,0.97,2,2.2999999999999998,0.86,3,2.34,0.87,3,2.34,0.87,3,2.2999999999999998,0.86,3,2.34,0.87,3,2.34,0.87,3]
["181300009514353","18",140,1987,32.697604849999998,-96.436258129999999,"prestress concrete girder",1.67,0.71,4,1.86,0.78,4,2.0299999999999998,0.85,3,1.66,0.7,5,1.86,0.78,4,2.0299999999999998,0.85,3,1.98,0.83,3,2.21,0.93,2,2.37,0.99,2,1.98,0.83,3,2.21,0.93,2,2.37,0.99,2,1.78,0.75,4,1.99,0.84,3,2.13,0.89,3,1.78,0.75,4,1.99,0.84,3,2.13,0.89,3]
["181300009514360","18",75,1987,32.698360780000002,-96.373068660000001,"prestress concrete girder",2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2]
["181300049501203","18",95,1965,32.668799300000003,-96.146130779999993,"steel girder",1.49,0.86,3,1.44,0.83,3,1.43,0.83,3,1.38,0.8,4,1.44,0.83,3,1.43,0.83,3,1.7,0.98,2,1.66,0.96,2,1.66,0.96,2,1.61,0.93,2,1.66,0.96,2,1.66,0.96,2,1.53,0.89,3,1.49,0.86,3,1.49,0.86,3,1.45,0.84,3,1.49,0.86,3,1.49,0.86,3]
["181300049501308","18",120,1983,32.701360620000003,-96.275186849999997,"prestress concrete girder",1.87,0.7,5,2.04,0.76,4,2.13,0.79,4,1.87,0.7,5,2.04,0.76,4,2.13,0.79,4,2.2200000000000002,0.83,3,2.41,0.89,3,2.5099999999999998,0.93,2,2.2200000000000002,0.83,3,2.41,0.89,3,2.5099999999999998,0.93,2,1.99,0.74,4,2.17,0.8,4,2.2599999999999998,0.84,3,1.99,0.74,4,2.17,0.8,4,2.2599999999999998,0.84,3]
["181750009301072","18",45,1964,32.085519130000002,-96.438858400000001,"prestress concrete girder",2.2200000000000002,0.88,3,2.2200000000000002,0.88,3,2.2200000000000002,0.88,3,2.23,0.89,3,2.2200000000000002,0.88,3,2.2200000000000002,0.88,3,2.96,1.18,1,2.96,1.18,1,2.96,1.18,1,2.96,1.18,1,2.96,1.18,1,2.96,1.18,1,2.68,1.07,1,2.68,1.07,1,2.68,1.07,1,2.68,1.07,1,2.68,1.07,1,2.68,1.07,1]
["181750009301075","18",90,1997,32.077274410000001,-96.442806500000003,"prestress concrete girder",2.16,0.91,2,2.17,0.91,2,2.17,0.91,2,2.16,0.91,2,2.17,0.91,2,2.17,0.91,2,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2]
["181750009301089","18",65,2005,31.963367999999999,-96.420839999999998,"prestress concrete girder",2.4,2.04,1,2.4,2.04,1,2.4,2.04,1,2.4,2.04,1,2.4,2.04,1,2.4,2.04,1,3.05,2.59,1,3.05,2.59,1,3.05,2.59,1,3.05,2.59,1,3.05,2.59,1,3.05,2.59,1,2.74,2.33,1,2.74,2.33,1,2.74,2.33,1,2.74,2.33,1,2.74,2.33,1,2.74,2.33,1]
["181750016203096","18",80,1996,31.940779079999999,-96.680335970000002,"prestress concrete girder",2.19,0.81,3,2.19,0.81,3,2.19,0.81,3,2.2000000000000002,0.82,3,2.2000000000000002,0.82,3,2.2000000000000002,0.82,3,2.7,1.01,1,2.7,1.01,1,2.7,1.01,1,2.7,1.01,1,2.7,1.01,1,2.7,1.01,1,2.42,0.9,3,2.42,0.9,3,2.42,0.9,3,2.42,0.9,3,2.42,0.9,3,2.42,0.9,3]
["181750016601072","18",80,1968,31.904564229999998,-96.383101080000003,"prestress concrete girder",2.29,0.81,3,2.29,0.81,3,2.29,0.81,3,2.29,0.81,3,2.29,0.81,3,2.29,0.81,3,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3]
["181990000912125","18",80,1987,32.969145619999999,-96.33205452,"steel girder",1.33,0.77,4,1.33,0.77,4,1.37,0.79,4,1.33,0.77,4,1.33,0.77,4,1.37,0.79,4,1.55,0.89,3,1.57,0.91,2,1.65,0.95,2,1.55,0.89,3,1.57,0.91,2,1.65,0.95,2,1.39,0.8,4,1.41,0.82,3,1.48,0.86,3,1.39,0.8,4,1.41,0.82,3,1.48,0.86,3]
["190190061005146","19",90,1971,33.415358830000002,-94.558215599999997,"prestress concrete girder",2.35,0.94,2,2.36,0.94,2,2.36,0.94,2,2.35,0.94,2,2.36,0.94,2,2.36,0.94,2,2.85,1.1399999999999999,1,2.85,1.1399999999999999,1,2.85,1.1399999999999999,1,2.85,1.1399999999999999,1,2.85,1.1399999999999999,1,2.85,1.1399999999999999,1,2.56,1.02,1,2.56,1.02,1,2.56,1.02,1,2.56,1.02,1,2.56,1.02,1,2.56,1.02,1]
["190190061006100","19",45,1965,33.474643520000001,-94.289369500000006,"concrete bridge",1.87,0.79,4,2.35,0.99,2,2.42,1.02,1,1.87,0.79,4,2.35,0.99,2,2.42,1.02,1,2.35,0.99,2,2.56,1.08,1,2.56,1.08,1,2.35,0.99,2,2.56,1.08,1,2.56,1.08,1,2.12,0.89,3,2.2999999999999998,0.97,2,2.2999999999999998,0.97,2,2.12,0.89,3,2.2999999999999998,0.97,2,2.2999999999999998,0.97,2]
["190190061006101","19",45,1965,33.474511530000001,-94.289052490000003,"concrete bridge",1.87,0.79,4,2.35,0.99,2,2.42,1.02,1,1.87,0.79,4,2.35,0.99,2,2.42,1.02,1,2.35,0.99,2,2.56,1.08,1,2.56,1.08,1,2.35,0.99,2,2.56,1.08,1,2.56,1.08,1,2.12,0.89,3,2.2999999999999998,0.97,2,2.2999999999999998,0.97,2,2.12,0.89,3,2.2999999999999998,0.97,2,2.2999999999999998,0.97,2]
["190190061006110","19",80,1985,33.470906200000002,-94.45647735,"prestress concrete girder",2.19,0.81,3,2.19,0.81,3,2.19,0.81,3,2.2000000000000002,0.82,3,2.2000000000000002,0.82,3,2.2000000000000002,0.82,3,2.7,1.01,1,2.7,1.01,1,2.7,1.01,1,2.7,1.01,1,2.7,1.01,1,2.7,1.01,1,2.42,0.9,3,2.42,0.9,3,2.42,0.9,3,2.42,0.9,3,2.42,0.9,3,2.42,0.9,3]
["190190061007039","19",60,1963,33.470209140000001,-94.050321089999997,"prestress concrete girder",2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.84,1,2,2.84,1,2,2.84,1,2,2.84,1,2,2.84,1,2,2.84,1,2,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3]
["190190061007082","19",65,1965,33.466626759999997,-94.218454039999997,"prestress concrete girder",2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.21,0.78,4,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3]
["190190061007207","19",80,2009,33.451868210000001,-94.108563140000001,"prestress concrete girder",2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1]
["190190061007210","19",105,2011,33.45091,-94.099739999999997,"prestress concrete girder",2.41,2.0499999999999998,1,2.57,2.1800000000000002,1,2.57,2.1800000000000002,1,2.41,2.0499999999999998,1,2.57,2.1800000000000002,1,2.57,2.1800000000000002,1,2.87,2.44,1,3.07,2.61,1,3.07,2.61,1,2.87,2.44,1,3.07,2.61,1,3.07,2.61,1,2.58,2.19,1,2.76,2.35,1,2.76,2.35,1,2.58,2.19,1,2.76,2.35,1,2.76,2.35,1]
["191030020705021","19",80,1996,32.372422229999998,-94.456442300000006,"prestress concrete girder",2.19,0.92,2,2.19,0.92,2,2.19,0.92,2,2.2000000000000002,0.93,2,2.2000000000000002,0.93,2,2.2000000000000002,0.93,2,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1]
["191030049508271","19",70,1966,32.466695319999999,-94.621464489999994,"prestress concrete girder",2.23,0.63,5,2.23,0.63,5,2.23,0.63,5,2.23,0.63,5,2.23,0.63,5,2.23,0.63,5,2.8,0.79,4,2.8,0.79,4,2.8,0.79,4,2.8,0.79,4,2.8,0.79,4,2.8,0.79,4,2.5099999999999998,0.71,4,2.5099999999999998,0.71,4,2.5099999999999998,0.71,4,2.5099999999999998,0.71,4,2.5099999999999998,0.71,4,2.5099999999999998,0.71,4]
["191030049510119","19",65,2009,32.467774730000002,-94.056265030000006,"prestress concrete girder",2.4,2.04,1,2.4,2.04,1,2.4,2.04,1,2.4,2.04,1,2.4,2.04,1,2.4,2.04,1,3.05,2.59,1,3.05,2.59,1,3.05,2.59,1,3.05,2.59,1,3.05,2.59,1,3.05,2.59,1,2.74,2.33,1,2.74,2.33,1,2.74,2.33,1,2.74,2.33,1,2.74,2.33,1,2.74,2.33,1]
["192250061003118","19",60,1965,33.174648900000001,-94.983452810000003,"prestress concrete girder",2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.84,1.1299999999999999,1,2.84,1.1299999999999999,1,2.84,1.1299999999999999,1,2.84,1.1299999999999999,1,2.84,1.1299999999999999,1,2.84,1.1299999999999999,1,2.5499999999999998,1.02,1,2.5499999999999998,1.02,1,2.5499999999999998,1.02,1,2.5499999999999998,1.02,1,2.5499999999999998,1.02,1,2.5499999999999998,1.02,1]
["192250061003123","19",70,1967,33.188513,-94.944445000000002,"prestress concrete girder",2.23,0.89,3,2.23,0.89,3,2.23,0.89,3,2.23,0.89,3,2.23,0.89,3,2.23,0.89,3,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.8,1.1200000000000001,1,2.5099999999999998,1,2,2.5099999999999998,1,2,2.5099999999999998,1,2,2.5099999999999998,1,2,2.5099999999999998,1,2,2.5099999999999998,1,2]
["192250061003139","19",110,1969,33.263339600000002,-94.826750790000006,"steel girder",1.71,0.79,4,1.62,0.75,4,1.57,0.73,4,1.37,0.63,5,1.5,0.7,5,1.56,0.72,4,1.91,0.88,3,1.82,0.84,3,1.78,0.82,3,1.59,0.73,4,1.74,0.8,4,1.78,0.82,3,1.72,0.79,4,1.64,0.76,4,1.6,0.74,4,1.43,0.66,5,1.57,0.73,4,1.6,0.74,4]
["200360050802243","20",80,1977,29.825874249999998,-94.846621060000004,"prestress concrete girder",2.19,0.92,2,2.19,0.92,2,2.19,0.92,2,2.2000000000000002,0.93,2,2.2000000000000002,0.93,2,2.2000000000000002,0.93,2,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1]
["201240002813091","20",80,1989,30.09624457,-94.129987569999997,"steel girder",1.33,0.77,4,1.33,0.77,4,1.37,0.79,4,1.33,0.77,4,1.33,0.77,4,1.37,0.79,4,1.55,0.89,3,1.57,0.91,2,1.65,0.95,2,1.55,0.89,3,1.57,0.91,2,1.65,0.95,2,1.39,0.8,4,1.41,0.82,3,1.48,0.86,3,1.39,0.8,4,1.41,0.82,3,1.48,0.86,3]
["201240002813162","20",60,1989,30.094655999999997,-94.100032999999996,"prestress concrete girder",2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1]
["201240002813222","20",90,1993,30.089787999999999,-94.136242999999993,"prestress concrete girder",2.16,0.91,2,2.17,0.91,2,2.17,0.91,2,2.16,0.91,2,2.17,0.91,2,2.17,0.91,2,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2]
["201240002813224","20",90,1993,30.08563681,-94.135980750000002,"prestress concrete girder",2.16,0.91,2,2.17,0.91,2,2.17,0.91,2,2.16,0.91,2,2.17,0.91,2,2.17,0.91,2,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.63,1.1100000000000001,1,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2]
["201460017703154","20",95,1987,30.344370860000001,-95.095845019999999,"prestress concrete girder",2.1,0.78,4,2.16,0.8,4,2.16,0.8,4,2.1,0.78,4,2.16,0.8,4,2.16,0.8,4,2.5499999999999998,0.95,2,2.6,0.97,2,2.6,0.97,2,2.5499999999999998,0.95,2,2.6,0.97,2,2.6,0.97,2,2.2999999999999998,0.86,3,2.34,0.87,3,2.34,0.87,3,2.2999999999999998,0.86,3,2.34,0.87,3,2.34,0.87,3]
["201460017703156","20",80,1987,30.352631509999998,-95.090053049999995,"prestress concrete girder",2.19,0.92,2,2.19,0.92,2,2.19,0.92,2,2.2000000000000002,0.93,2,2.2000000000000002,0.93,2,2.2000000000000002,0.93,2,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1]
["201810002809242","20",80,2006,30.095161600000001,-94.076451419999998,"prestress concrete girder",2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,2.4500000000000002,2.08,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,3.01,2.56,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1,2.7,2.2999999999999998,1]
["201810002811248","20",90,2008,30.135457290000002,-94.002962719999999,"prestress concrete girder",2.4900000000000002,2.12,1,2.5,2.13,1,2.5,2.13,1,2.4900000000000002,2.12,1,2.5,2.13,1,2.5,2.13,1,3.02,2.57,1,3.02,2.57,1,3.02,2.57,1,3.02,2.57,1,3.02,2.57,1,3.02,2.57,1,2.72,2.31,1,2.72,2.31,1,2.72,2.31,1,2.72,2.31,1,2.72,2.31,1,2.72,2.31,1]
["201810002814243","20",290,2002,30.124353859999999,-93.708273910000003,"Multi Span Long",0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1,0,1,1]
["201810002814513","20",120,2012,30.113860590000002,-93.80391419,"prestress concrete girder",2.33,1.98,1,2.5499999999999998,2.17,1,2.66,2.2599999999999998,1,2.33,1.98,1,2.5499999999999998,2.17,1,2.66,2.2599999999999998,1,2.77,2.35,1,3.01,2.56,1,3.14,2.67,1,2.77,2.35,1,3.01,2.56,1,3.14,2.67,1,2.4900000000000002,2.12,1,2.71,2.2999999999999998,1,2.82,2.4,1,2.4900000000000002,2.12,1,2.71,2.2999999999999998,1,2.82,2.4,1]
["210310003907301","21",120,2004,26.18219946,-97.714817980000007,"prestress concrete girder",1.87,0.7,5,2.04,0.76,4,2.13,0.79,4,1.87,0.7,5,2.04,0.76,4,2.13,0.79,4,2.2200000000000002,0.83,3,2.41,0.89,3,2.5099999999999998,0.93,2,2.2200000000000002,0.83,3,2.41,0.89,3,2.5099999999999998,0.93,2,1.99,0.74,4,2.17,0.8,4,2.2599999999999998,0.84,3,1.99,0.74,4,2.17,0.8,4,2.2599999999999998,0.84,3]
["210310003907302","21",120,2005,26.181982779999998,-97.714135540000001,"prestress concrete girder",2.33,1.75,1,2.5499999999999998,1.91,1,2.66,2,1,2.33,1.75,1,2.5499999999999998,1.91,1,2.66,2,1,2.77,2.08,1,3.01,2.2599999999999998,1,3.14,2.36,1,2.77,2.08,1,3.01,2.2599999999999998,1,3.14,2.36,1,2.4900000000000002,1.87,1,2.71,2.0299999999999998,1,2.82,2.11,1,2.4900000000000002,1.87,1,2.71,2.0299999999999998,1,2.82,2.11,1]
["210310003907303","21",105,2004,26.179287479999999,-97.710650819999998,"steel girder",1.95,1.46,1,1.97,1.48,1,1.92,1.44,1,1.74,1.31,1,1.89,1.42,1,1.92,1.44,1,2.33,1.75,1,2.23,1.67,1,2.2000000000000002,1.65,1,2.0299999999999998,1.52,1,2.19,1.64,1,2.2000000000000002,1.65,1,2.09,1.57,1,2.0099999999999998,1.51,1,1.97,1.48,1,1.83,1.37,1,1.97,1.48,1,1.97,1.48,1]
["210310003907361","21",95,2007,26.191883489999999,-97.718733850000007,"prestress concrete girder",2.4500000000000002,2.08,1,2.52,2.14,1,2.52,2.14,1,2.4500000000000002,2.08,1,2.52,2.14,1,2.52,2.14,1,2.98,2.5299999999999998,1,3.04,2.58,1,3.04,2.58,1,2.98,2.5299999999999998,1,3.04,2.58,1,3.04,2.58,1,2.68,2.2799999999999998,1,2.73,2.3199999999999998,1,2.73,2.3199999999999998,1,2.68,2.2799999999999998,1,2.73,2.3199999999999998,1,2.73,2.3199999999999998,1]
["210310003907362","21",115,2005,26.14038201,-97.655024119999993,"prestress concrete girder",2.38,1.79,1,2.56,1.92,1,2.63,1.97,1,2.38,1.79,1,2.56,1.92,1,2.63,1.97,1,2.8,2.1,1,3.05,2.29,1,3.12,2.34,1,2.8,2.1,1,3.05,2.29,1,3.12,2.34,1,2.52,1.89,1,2.75,2.06,1,2.8,2.1,1,2.52,1.89,1,2.75,2.06,1,2.8,2.1,1]
["210310003908241","21",65,2004,26.00442121,-97.529844460000007,"prestress concrete girder",2.25,0.94,2,2.25,0.94,2,2.25,0.94,2,2.25,0.94,2,2.25,0.94,2,2.25,0.94,2,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.56,1.08,1,2.56,1.08,1,2.56,1.08,1,2.56,1.08,1,2.56,1.08,1,2.56,1.08,1]
["210310003909236","21",95,2004,25.978702729999998,-97.518091699999999,"prestress concrete girder",2.1,0.88,3,2.16,0.91,2,2.16,0.91,2,2.1,0.88,3,2.16,0.91,2,2.16,0.91,2,2.5499999999999998,1.07,1,2.6,1.1000000000000001,1,2.6,1.1000000000000001,1,2.5499999999999998,1.07,1,2.6,1.1000000000000001,1,2.6,1.1000000000000001,1,2.2999999999999998,0.97,2,2.34,0.99,2,2.34,0.99,2,2.2999999999999998,0.97,2,2.34,0.99,2,2.34,0.99,2]
["210310003916170","21",175,2000,25.908940220000002,-97.488202310000005,"steel girder",1.35,0.78,4,1.46,0.84,3,1.59,0.92,2,1.23,0.71,4,1.43,0.83,3,1.59,0.92,2,1.56,0.9,3,1.71,0.99,2,1.87,1.08,1,1.49,0.86,3,1.71,0.99,2,1.87,1.08,1,1.41,0.82,3,1.53,0.89,3,1.68,0.97,2,1.34,0.77,4,1.53,0.89,3,1.68,0.97,2]
["210310003916171","21",175,2000,25.908865219999999,-97.488318320000005,"steel girder",1.35,0.78,4,1.46,0.84,3,1.59,0.92,2,1.23,0.71,4,1.43,0.83,3,1.59,0.92,2,1.56,0.9,3,1.71,0.99,2,1.87,1.08,1,1.49,0.86,3,1.71,0.99,2,1.87,1.08,1,1.41,0.82,3,1.53,0.89,3,1.68,0.97,2,1.34,0.77,4,1.53,0.89,3,1.68,0.97,2]
["210310003916385","21",120,2005,25.935998390000002,-97.498120540000002,"prestress concrete girder",2.33,1.98,1,2.5499999999999998,2.17,1,2.66,2.2599999999999998,1,2.33,1.98,1,2.5499999999999998,2.17,1,2.66,2.2599999999999998,1,2.77,2.35,1,3.01,2.56,1,3.14,2.67,1,2.77,2.35,1,3.01,2.56,1,3.14,2.67,1,2.4900000000000002,2.12,1,2.71,2.2999999999999998,1,2.82,2.4,1,2.4900000000000002,2.12,1,2.71,2.2999999999999998,1,2.82,2.4,1]
["210310362201261","21",110,2016,26.022817199999999,-97.512774899999997,"prestress concrete girder",2.4,2.04,1,2.58,2.19,1,2.6,2.21,1,2.4,2.04,1,2.58,2.19,1,2.6,2.21,1,2.83,2.41,1,3.09,2.63,1,3.09,2.63,1,2.83,2.41,1,3.09,2.63,1,3.09,2.63,1,2.54,2.16,1,2.78,2.36,1,2.78,2.36,1,2.54,2.16,1,2.78,2.36,1,2.78,2.36,1]
["211090003902189","21",45,1969,26.268233819999999,-98.545132409999994,"concrete bridge",2.4,0.96,2,2.4,0.96,2,2.4,0.96,2,2.41,0.96,2,2.4,0.96,2,2.4,0.96,2,3.2,1.28,1,3.2,1.28,1,3.2,1.28,1,3.2,1.28,1,3.2,1.28,1,3.2,1.28,1,2.89,1.1599999999999999,1,2.89,1.1599999999999999,1,2.89,1.1599999999999999,1,2.89,1.1599999999999999,1,2.89,1.1599999999999999,1,2.89,1.1599999999999999,1]
["211090003917106","21",65,1993,26.20616746,-98.194321810000005,"prestress concrete girder",2.25,0.94,2,2.25,0.94,2,2.25,0.94,2,2.25,0.94,2,2.25,0.94,2,2.25,0.94,2,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.56,1.08,1,2.56,1.08,1,2.56,1.08,1,2.56,1.08,1,2.56,1.08,1,2.56,1.08,1]
["211090003917275","21",130,1998,26.187818570000001,-98.215478899999994,"prestress concrete girder",1.76,0.74,4,1.97,0.83,3,2.1,0.88,3,1.76,0.74,4,1.97,0.83,3,2.1,0.88,3,2.11,0.88,3,2.2999999999999998,0.97,2,2.48,1.05,1,2.11,0.88,3,2.2999999999999998,0.97,2,2.48,1.05,1,1.9,0.8,4,2.0699999999999998,0.87,3,2.23,0.94,2,1.9,0.8,4,2.0699999999999998,0.87,3,2.23,0.94,2]
["211090003917321","21",115,2004,26.201145749999998,-98.328727119999996,"prestress concrete girder",1.93,0.82,3,2.08,0.88,3,2.13,0.89,3,1.93,0.82,3,2.08,0.88,3,2.13,0.89,3,2.27,0.95,2,2.4700000000000002,1.04,1,2.5299999999999998,1.06,1,2.27,0.95,2,2.4700000000000002,1.04,1,2.5299999999999998,1.06,1,2.04,0.86,3,2.23,0.94,2,2.27,0.95,2,2.04,0.86,3,2.23,0.94,2,2.27,0.95,2]
["211090003918281","21",110,2002,26.19299998,-98.133488700000001,"prestress concrete girder",1.97,0.83,3,2.12,0.89,3,2.14,0.9,3,1.97,0.83,3,2.12,0.89,3,2.14,0.9,3,2.3199999999999998,0.98,2,2.54,1.07,1,2.54,1.07,1,2.3199999999999998,0.98,2,2.54,1.07,1,2.54,1.07,1,2.09,0.88,3,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.09,0.88,3,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2]
["211090003918287","21",110,2002,26.186390620000001,-98.085573179999997,"prestress concrete girder",1.97,0.83,3,2.12,0.89,3,2.14,0.9,3,1.97,0.83,3,2.12,0.89,3,2.14,0.9,3,2.3199999999999998,0.98,2,2.54,1.07,1,2.54,1.07,1,2.3199999999999998,0.98,2,2.54,1.07,1,2.54,1.07,1,2.09,0.88,3,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.09,0.88,3,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2]
["211090003918339","21",95,2006,26.183369890000002,-98.066207019999993,"prestress concrete girder",2.4500000000000002,2.08,1,2.52,2.14,1,2.52,2.14,1,2.4500000000000002,2.08,1,2.52,2.14,1,2.52,2.14,1,2.98,2.5299999999999998,1,3.04,2.58,1,3.04,2.58,1,2.98,2.5299999999999998,1,3.04,2.58,1,3.04,2.58,1,2.68,2.2799999999999998,1,2.73,2.3199999999999998,1,2.73,2.3199999999999998,1,2.68,2.2799999999999998,1,2.73,2.3199999999999998,1,2.73,2.3199999999999998,1]
["211090003918340","21",95,2005,26.181758420000001,-98.052087610000001,"prestress concrete girder",2.4500000000000002,2.08,1,2.52,2.14,1,2.52,2.14,1,2.4500000000000002,2.08,1,2.52,2.14,1,2.52,2.14,1,2.98,2.5299999999999998,1,3.04,2.58,1,3.04,2.58,1,2.98,2.5299999999999998,1,3.04,2.58,1,3.04,2.58,1,2.68,2.2799999999999998,1,2.73,2.3199999999999998,1,2.73,2.3199999999999998,1,2.68,2.2799999999999998,1,2.73,2.3199999999999998,1,2.73,2.3199999999999998,1]
["211090003918344","21",115,2006,26.17286876,-98.006701759999999,"prestress concrete girder",2.38,2.02,1,2.56,2.1800000000000002,1,2.63,2.2400000000000002,1,2.38,2.02,1,2.56,2.1800000000000002,1,2.63,2.2400000000000002,1,2.8,2.38,1,3.05,2.59,1,3.12,2.65,1,2.8,2.38,1,3.05,2.59,1,3.12,2.65,1,2.52,2.14,1,2.75,2.34,1,2.8,2.38,1,2.52,2.14,1,2.75,2.34,1,2.8,2.38,1]
["211090003918409","21",130,2008,26.153335989999999,-97.941794869999995,"prestress concrete girder",2.2599999999999998,1.92,1,2.54,2.16,1,2.69,2.29,1,2.2599999999999998,1.92,1,2.54,2.16,1,2.69,2.29,1,2.71,2.2999999999999998,1,2.96,2.52,1,3.19,2.71,1,2.71,2.2999999999999998,1,2.96,2.52,1,3.19,2.71,1,2.44,2.0699999999999998,1,2.66,2.2599999999999998,1,2.87,2.44,1,2.44,2.0699999999999998,1,2.66,2.2599999999999998,1,2.87,2.44,1]
["211090003918424","21",115,2008,26.15887734,-97.894404980000004,"prestress concrete girder",2.38,2.02,1,2.56,2.1800000000000002,1,2.63,2.2400000000000002,1,2.38,2.02,1,2.56,2.1800000000000002,1,2.63,2.2400000000000002,1,2.8,2.38,1,3.05,2.59,1,3.12,2.65,1,2.8,2.38,1,3.05,2.59,1,3.12,2.65,1,2.52,2.14,1,2.75,2.34,1,2.8,2.38,1,2.52,2.14,1,2.75,2.34,1,2.8,2.38,1]
["212450032710067","21",95,2007,26.5041118,-97.771580029999996,"prestress concrete girder",2.4500000000000002,2.08,1,2.52,2.14,1,2.52,2.14,1,2.4500000000000002,2.08,1,2.52,2.14,1,2.52,2.14,1,2.98,2.5299999999999998,1,3.04,2.58,1,3.04,2.58,1,2.98,2.5299999999999998,1,3.04,2.58,1,3.04,2.58,1,2.68,2.2799999999999998,1,2.73,2.3199999999999998,1,2.73,2.3199999999999998,1,2.68,2.2799999999999998,1,2.73,2.3199999999999998,1,2.73,2.3199999999999998,1]
["212530003802037","21",55,1967,27.219112200000001,-99.417899809999994,"steel girder",2.0699999999999998,1.37,1,2.0699999999999998,1.37,1,2.0699999999999998,1.37,1,2.0699999999999998,1.37,1,2.0699999999999998,1.37,1,2.0699999999999998,1.37,1,2.73,1.81,1,2.73,1.81,1,2.73,1.81,1,2.73,1.81,1,2.73,1.81,1,2.73,1.81,1,2.44,1.61,1,2.44,1.61,1,2.44,1.61,1,2.44,1.61,1,2.44,1.61,1,2.44,1.61,1]
["221420001801100","22",60,1971,28.417697100000002,-99.251442220000001,"prestress concrete girder",2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.2000000000000002,0.88,3,2.84,1.1299999999999999,1,2.84,1.1299999999999999,1,2.84,1.1299999999999999,1,2.84,1.1299999999999999,1,2.84,1.1299999999999999,1,2.84,1.1299999999999999,1,2.5499999999999998,1.02,1,2.5499999999999998,1.02,1,2.5499999999999998,1.02,1,2.5499999999999998,1.02,1,2.5499999999999998,1.02,1,2.5499999999999998,1.02,1]
["221420001801107","22",75,1975,28.317570029999999,-99.273290459999998,"prestress concrete girder",2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.21,0.82,3,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.74,1.02,1,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2,2.46,0.92,2]
["221590029903018","22",50,1972,29.064353999999998,-100.63887,"steel girder",2.06,1.36,1,2.06,1.36,1,2.06,1.36,1,2.06,1.36,1,2.06,1.36,1,2.06,1.36,1,2.79,1.85,1,2.79,1.85,1,2.79,1.85,1,2.79,1.85,1,2.79,1.85,1,2.79,1.85,1,2.5,1.65,1,2.5,1.65,1,2.5,1.65,1,2.5,1.65,1,2.5,1.65,1,2.5,1.65,1]
["222400001803142","22",60,1978,28.030008160000001,-99.357701579999997,"prestress concrete girder",2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.2799999999999998,0.96,2,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.94,1.24,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1,2.64,1.1100000000000001,1]
["222400001803160","22",50,1983,27.952299740000001,-99.381622919999998,"prestress concrete girder",2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,3.2,1.34,1,3.2,1.34,1,3.2,1.34,1,3.2,1.34,1,3.2,1.34,1,3.2,1.34,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1]
["222400001806176","22",160,2008,27.62592364,-99.489548940000006,"prestress concrete girder",2.13,1.81,1,2.34,1.99,1,2.58,2.19,1,2.02,1.72,1,2.34,1.99,1,2.58,2.19,1,2.4900000000000002,2.12,1,2.76,2.35,1,3.06,2.6,1,2.4500000000000002,2.08,1,2.76,2.35,1,3.06,2.6,1,2.2400000000000002,1.9,1,2.48,2.11,1,2.75,2.34,1,2.2000000000000002,1.87,1,2.48,2.11,1,2.75,2.34,1]
["222400003801079","22",50,1999,27.396750709999999,-99.477676869999996,"prestress concrete girder",2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,3.2,1.34,1,3.2,1.34,1,3.2,1.34,1,3.2,1.34,1,3.2,1.34,1,3.2,1.34,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1]
["222400003801082","22",80,2003,27.363519709999998,-99.460371379999998,"prestress concrete girder",2.19,0.92,2,2.19,0.92,2,2.19,0.92,2,2.2000000000000002,0.93,2,2.2000000000000002,0.93,2,2.2000000000000002,0.93,2,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.7,1.1399999999999999,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1,2.42,1.02,1]
["222400008601061","22",50,1992,27.505942019999999,-99.496395160000006,"prestress concrete girder",2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,2.36,0.99,2,3.2,1.34,1,3.2,1.34,1,3.2,1.34,1,3.2,1.34,1,3.2,1.34,1,3.2,1.34,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1]
["230680000703154","23",80,1972,32.381168619999997,-98.815922729999997,"prestress concrete girder",2.29,0.81,3,2.29,0.81,3,2.29,0.81,3,2.29,0.81,3,2.29,0.81,3,2.29,0.81,3,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.81,0.99,2,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3,2.52,0.89,3]
["230680000706148","23",60,2014,32.460021500000003,-98.641445270000006,"prestress concrete girder",2.4,2.04,1,2.4,2.04,1,2.4,2.04,1,2.4,2.04,1,2.4,2.04,1,2.4,2.04,1,3.1,2.64,1,3.1,2.64,1,3.1,2.64,1,3.1,2.64,1,3.1,2.64,1,3.1,2.64,1,2.77,2.35,1,2.77,2.35,1,2.77,2.35,1,2.77,2.35,1,2.77,2.35,1,2.77,2.35,1]
["231410027301012","23",90,1991,31.057593099999998,-98.179500619999999,"steel girder",1.43,0.83,3,1.39,0.8,4,1.4,0.81,3,1.36,0.79,4,1.39,0.8,4,1.4,0.81,3,1.64,0.95,2,1.62,0.94,2,1.64,0.95,2,1.61,0.93,2,1.62,0.94,2,1.64,0.95,2,1.47,0.85,3,1.45,0.84,3,1.47,0.85,3,1.45,0.84,3,1.45,0.84,3,1.47,0.85,3]
["240550000301178","24",70,1975,31.039651209999999,-104.81738999,"prestress concrete girder",2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1]
["240550000301180","24",70,1975,31.040039999999998,-104.817268,"prestress concrete girder",2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.23,0.94,2,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.79,1.17,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1,2.5,1.05,1]
["240550000302138","24",120,1971,31.062094999999999,-104.501346,"prestress concrete girder",2.2799999999999998,0.8,4,2.4900000000000002,0.88,3,2.6,0.92,2,2.2799999999999998,0.8,4,2.4900000000000002,0.88,3,2.6,0.92,2,2.71,0.95,2,2.94,1.04,1,3.07,1.08,1,2.71,0.95,2,2.94,1.04,1,3.07,1.08,1,2.44,0.86,3,2.65,0.94,2,2.76,0.98,2,2.44,0.86,3,2.65,0.94,2,2.76,0.98,2]
["240550000302142","24",50,1971,31.07331357,-104.42134462999999,"prestress concrete special",2.2000000000000002,0.88,0,2.2000000000000002,0.88,0,2.2000000000000002,0.88,0,2.2000000000000002,0.88,0,2.2000000000000002,0.88,0,2.2000000000000002,0.88,0,2.99,1.2,0,2.99,1.2,0,2.99,1.2,0,2.99,1.2,0,2.99,1.2,0,2.99,1.2,0,2.67,1.06,0,2.67,1.06,0,2.67,1.06,0,2.67,1.06,0,2.67,1.06,0,2.67,1.06,0]
["240550000303090","24",60,1969,31.066561910000001,-104.21712966,"prestress concrete girder",2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.84,1,2,2.84,1,2,2.84,1,2,2.84,1,2,2.84,1,2,2.84,1,2,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3]
["240720212102161","24",65,1990,31.777518520000001,-106.42209115,"prestress concrete girder",2.25,0.94,2,2.25,0.94,2,2.25,0.94,2,2.25,0.94,2,2.25,0.94,2,2.25,0.94,2,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.86,1.21,1,2.56,1.08,1,2.56,1.08,1,2.56,1.08,1,2.56,1.08,1,2.56,1.08,1,2.56,1.08,1]
["240720212102184","24",95,2002,31.771948380000001,-106.47304232,"steel girder",1.71,0.99,2,1.76,1.02,1,1.76,1.02,1,1.71,0.99,2,1.76,1.02,1,1.76,1.02,1,2.08,1.2,1,2.12,1.22,1,2.12,1.22,1,2.08,1.2,1,2.12,1.22,1,2.12,1.22,1,1.87,1.08,1,1.9,1.1000000000000001,1,1.9,1.1000000000000001,1,1.87,1.08,1,1.9,1.1000000000000001,1,1.9,1.1000000000000001,1]
["240720212102280","24",65,1968,31.759361999999999,-106.49659199999999,"prestress concrete girder",2.21,0.88,3,2.21,0.88,3,2.21,0.88,3,2.21,0.88,3,2.21,0.88,3,2.21,0.88,3,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.81,1.1200000000000001,1,2.52,1,2,2.52,1,2,2.52,1,2,2.52,1,2,2.52,1,2,2.52,1,2]
["240720212103235","24",85,1989,31.778532179999999,-106.39298895,"prestress concrete girder",2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.66,0.99,2,2.66,0.99,2,2.66,0.99,2,2.66,0.99,2,2.66,0.99,2,2.66,0.99,2,2.39,0.89,3,2.39,0.89,3,2.39,0.89,3,2.39,0.89,3,2.39,0.89,3,2.39,0.89,3]
["240720212103236","24",85,1989,31.771519999999999,-106.376876,"prestress concrete girder",2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.1800000000000002,0.81,3,2.66,0.99,2,2.66,0.99,2,2.66,0.99,2,2.66,0.99,2,2.66,0.99,2,2.66,0.99,2,2.39,0.89,3,2.39,0.89,3,2.39,0.89,3,2.39,0.89,3,2.39,0.89,3,2.39,0.89,3]
["240720212103274","24",95,2002,31.739799869999999,-106.32459636999999,"prestress concrete girder",2.1,0.88,3,2.16,0.91,2,2.16,0.91,2,2.1,0.88,3,2.16,0.91,2,2.16,0.91,2,2.5499999999999998,1.07,1,2.6,1.1000000000000001,1,2.6,1.1000000000000001,1,2.5499999999999998,1.07,1,2.6,1.1000000000000001,1,2.6,1.1000000000000001,1,2.2999999999999998,0.97,2,2.34,0.99,2,2.34,0.99,2,2.2999999999999998,0.97,2,2.34,0.99,2,2.34,0.99,2]
["240720212104293","24",150,2015,31.695505560000001,-106.2772806,"prestress concrete girder",2.16,1.84,1,2.39,2.0299999999999998,1,2.65,2.25,1,2.11,1.79,1,2.39,2.0299999999999998,1,2.65,2.25,1,2.54,2.16,1,2.84,2.41,1,3.09,2.63,1,2.54,2.16,1,2.84,2.41,1,3.09,2.63,1,2.2799999999999998,1.94,1,2.5499999999999998,2.17,1,2.78,2.36,1,2.2799999999999998,1.94,1,2.5499999999999998,2.17,1,2.78,2.36,1]
["240720212104296","24",125,2012,31.706009999999999,-106.28059399999999,"prestress concrete girder",2.29,2.29,1,2.54,2.54,1,2.69,2.69,1,2.2999999999999998,2.2999999999999998,1,2.54,2.54,1,2.69,2.69,1,2.74,2.74,1,2.98,2.98,1,3.17,3.17,1,2.74,2.74,1,2.98,2.98,1,3.17,3.17,1,2.4700000000000002,2.4700000000000002,1,2.68,2.68,1,2.85,2.85,1,2.4700000000000002,2.4700000000000002,1,2.68,2.68,1,2.85,2.85,1]
["240720212104302","24",65,2016,31.600377779999999,-106.1940389,"prestress concrete girder",2.4,2.04,1,2.4,2.04,1,2.4,2.04,1,2.4,2.04,1,2.4,2.04,1,2.4,2.04,1,3.05,2.59,1,3.05,2.59,1,3.05,2.59,1,3.05,2.59,1,3.05,2.59,1,3.05,2.59,1,2.74,2.33,1,2.74,2.33,1,2.74,2.33,1,2.74,2.33,1,2.74,2.33,1,2.74,2.33,1]
["240720212105158","24",65,1962,31.464959740000001,-106.05265848000001,"prestress concrete girder",2.21,0.62,5,2.21,0.62,5,2.21,0.62,5,2.21,0.62,5,2.21,0.62,5,2.21,0.62,5,2.81,0.79,4,2.81,0.79,4,2.81,0.79,4,2.81,0.79,4,2.81,0.79,4,2.81,0.79,4,2.52,0.71,4,2.52,0.71,4,2.52,0.71,4,2.52,0.71,4,2.52,0.71,4,2.52,0.71,4]
["241160000207135","24",50,1965,31.173478999999997,-105.357829,"prestress concrete girder",2.2000000000000002,0.52,5,2.2000000000000002,0.52,5,2.2000000000000002,0.52,5,2.2000000000000002,0.52,5,2.2000000000000002,0.52,5,2.2000000000000002,0.52,5,2.99,0.71,4,2.99,0.71,4,2.99,0.71,4,2.99,0.71,4,2.99,0.71,4,2.99,0.71,4,2.67,0.63,5,2.67,0.63,5,2.67,0.63,5,2.67,0.63,5,2.67,0.63,5,2.67,0.63,5]
["241160000208138","24",75,1986,31.171087999999997,-105.346081,"steel girder",1.29,0.74,4,1.31,0.76,4,1.38,0.8,4,1.29,0.74,4,1.31,0.76,4,1.38,0.8,4,1.53,0.89,3,1.58,0.92,2,1.7,0.98,2,1.53,0.89,3,1.58,0.92,2,1.7,0.98,2,1.37,0.79,4,1.41,0.82,3,1.52,0.88,3,1.37,0.79,4,1.41,0.82,3,1.52,0.88,3]
["241230000304098","24",45,1969,31.065283999999998,-104.144977,"concrete bridge",2.4,0.85,3,2.4,0.85,3,2.4,0.85,3,2.41,0.85,3,2.4,0.85,3,2.4,0.85,3,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,3.2,1.1299999999999999,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1,2.89,1.02,1]
["250380004212065","25",60,1968,34.481839190000002,-100.33471252,"prestress concrete girder",2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.2000000000000002,0.77,4,2.84,1,2,2.84,1,2,2.84,1,2,2.84,1,2,2.84,1,2,2.84,1,2,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3,2.5499999999999998,0.9,3]
["251000004304201","25",75,2003,34.256055070000002,-99.527250980000005,"prestress concrete girder",2.21,0.93,2,2.21,0.93,2,2.21,0.93,2,2.21,0.93,2,2.21,0.93,2,2.21,0.93,2,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.74,1.1599999999999999,1,2.46,1.04,1,2.46,1.04,1,2.46,1.04,1,2.46,1.04,1,2.46,1.04,1,2.46,1.04,1]
["251380015702059","25",125,2006,33.441791180000003,-99.622539520000004,"prestress concrete girder",2.29,1.95,1,2.54,2.16,1,2.69,2.29,1,2.2999999999999998,1.95,1,2.54,2.16,1,2.69,2.29,1,2.74,2.33,1,2.98,2.5299999999999998,1,3.17,2.69,1,2.74,2.33,1,2.98,2.5299999999999998,1,3.17,2.69,1,2.4700000000000002,2.1,1,2.68,2.2799999999999998,1,2.85,2.42,1,2.4700000000000002,2.1,1,2.68,2.2799999999999998,1,2.85,2.42,1]
["252420027512110","25",125,1973,35.228504549999997,-100.26951433000001,"prestress concrete girder",2.25,0.64,5,2.4900000000000002,0.7,5,2.64,0.74,4,2.25,0.64,5,2.4900000000000002,0.7,5,2.64,0.74,4,2.69,0.76,4,2.93,0.83,3,3.11,0.88,3,2.69,0.76,4,2.93,0.83,3,3.11,0.88,3,2.42,0.68,5,2.63,0.74,4,2.8,0.79,4,2.42,0.68,5,2.63,0.74,4,2.8,0.79,4]
[null,null,0,null,null,null,null,0,0,null,0,0,null,0,0,null,0,0,null,0,0,null,0,0,null,0,0,null,0,0,null,0,0,null,0,0,null,0,0,null,0,0,null,0,0,null,0,0,null,0,0,null,0,0,null,0,0,null,0,0]